--- a/ath/if_ath.c
+++ b/ath/if_ath.c
@@ -606,6 +606,14 @@ ath_attach(u_int16_t devid, struct net_d
 	}
 	sc->sc_ah = ah;
 
+	/* WAR for AR7100 PCI bug */
+#ifdef CONFIG_ATHEROS_AR71XX
+	if ((ar_device(sc->devid) >= 5210) && (ar_device(sc->devid) < 5416)) {
+		ath_hal_setcapability(ah, HAL_CAP_DMABURST_RX, 0, HAL_DMABURST_4B, NULL);
+		ath_hal_setcapability(ah, HAL_CAP_DMABURST_TX, 0, HAL_DMABURST_4B, NULL);
+	}
+#endif
+
 	/*
 	 * Check if the MAC has multi-rate retry support.
 	 * We do this by trying to setup a fake extended
@@ -7553,7 +7561,7 @@ ath_txq_setup(struct ath_softc *sc, int 
 	if (qtype == HAL_TX_QUEUE_UAPSD)
 		qi.tqi_qflags = HAL_TXQ_TXDESCINT_ENABLE;
 	else
-		qi.tqi_qflags = HAL_TXQ_TXEOLINT_ENABLE | 
+		qi.tqi_qflags = HAL_TXQ_TXEOLINT_ENABLE | HAL_TXQ_TXOKINT_ENABLE |
 			HAL_TXQ_TXDESCINT_ENABLE;
 	qnum = ath_hal_setuptxqueue(ah, qtype, &qi);
 	if (qnum == -1) {
--- a/ath_hal/ah_os.c
+++ b/ath_hal/ah_os.c
@@ -126,6 +126,13 @@ ath_hal_printf(struct ath_hal *ah, const
 }
 EXPORT_SYMBOL(ath_hal_printf);
 
+void __ahdecl
+ath_hal_printstr(struct ath_hal *ah, const char *str)
+{
+	printk("%s", str);
+}
+EXPORT_SYMBOL(ath_hal_printstr);
+
 /*
  * Format an Ethernet MAC for printing.
  */
--- a/ath_hal/ah_os.h
+++ b/ath_hal/ah_os.h
@@ -156,69 +156,23 @@ extern u_int32_t __ahdecl ath_hal_getupt
 #endif
 #endif				/* AH_BYTE_ORDER */
 
-/*
- * Some big-endian architectures don't set CONFIG_GENERIC_IOMAP, but fail to
- * implement iowrite32be and ioread32be.  Provide compatibility macros when
- * it's needed.
- *
- * As of Linux 2.6.24, only MIPS, PARISC and PowerPC implement iowrite32be and
- * ioread32be as functions.
- *
- * The downside or the replacement macros it that we may be byte-swapping data
- * for the second time, so the native implementations should be preferred.
- */
-#if (LINUX_VERSION_CODE >= KERNEL_VERSION(2,6,12)) && \
-	!defined(CONFIG_GENERIC_IOMAP) && (AH_BYTE_ORDER == AH_BIG_ENDIAN) && \
-	!defined(__mips__) && !defined(__hppa__) && !defined(__powerpc__)
-# ifndef iowrite32be
-#  define iowrite32be(_val, _addr) iowrite32(swab32((_val)), (_addr))
-# endif
-# ifndef ioread32be
-#  define ioread32be(_addr) swab32(ioread32((_addr)))
-# endif
-#endif
+#define IS_SWAPPED(_ah, _reg) \
+	((_ah)->ah_swapped && \
+		(((0x4000 <= (_reg)) && ((_reg) < 0x5000)) || \
+		 ((0x7000 <= (_reg)) && ((_reg) < 0x8000))))
+
+#define SWAPREG(_ah, _reg, _val) \
+	(IS_SWAPPED(_ah, _reg) ? cpu_to_le32(_val) : (_val))
 
 /*
  * The register accesses are done using target-specific functions when
  * debugging is enabled (AH_DEBUG) or it's explicitly requested for the target.
- *
- * The hardware registers use little-endian byte order natively.  Big-endian
- * systems are configured by HAL to enable hardware byte-swap of register reads
- * and writes at reset.  This avoid the need to byte-swap the data in software.
- * However, the registers in a certain area from 0x4000 to 0x4fff (PCI clock
- * domain registers) are not byte swapped!
- *
- * Since Linux I/O primitives default to little-endian operations, we only
- * need to suppress byte-swapping on big-endian systems outside the area used
- * by the PCI clock domain registers.
  */
-#if (AH_BYTE_ORDER == AH_BIG_ENDIAN)
-#define is_reg_le(__reg) ((0x4000 <= (__reg) && (__reg) < 0x5000))
-#else
-#define is_reg_le(__reg) 1
-#endif
-
-#if LINUX_VERSION_CODE >= KERNEL_VERSION(2,6,12)
-#define _OS_REG_WRITE(_ah, _reg, _val) do {			\
-	 is_reg_le(_reg) ?					\
-	 iowrite32((_val), (_ah)->ah_sh + (_reg)) :		\
-	 iowrite32be((_val), (_ah)->ah_sh + (_reg));		\
-	} while (0)
-#define _OS_REG_READ(_ah, _reg)					\
-	(is_reg_le(_reg) ?					\
-	 ioread32((_ah)->ah_sh + (_reg)) :			\
-	 ioread32be((_ah)->ah_sh + (_reg)))
-#else
 #define _OS_REG_WRITE(_ah, _reg, _val) do {			\
-	 writel(is_reg_le(_reg) ? 				\
-	 	(_val) : cpu_to_le32(_val), 			\
-		(_ah)->ah_sh + (_reg));				\
-	} while (0)
+	 __raw_writel(SWAPREG(_ah, _reg, _val), (_ah)->ah_sh + (_reg));		\
+} while (0)
 #define _OS_REG_READ(_ah, _reg)					\
-	(is_reg_le(_reg) ?					\
-	 readl((_ah)->ah_sh + (_reg)) :				\
-	 cpu_to_le32(readl((_ah)->ah_sh + (_reg))))
-#endif				/* KERNEL_VERSION(2,6,12) */
+	 SWAPREG(_ah, _reg, __raw_readl((_ah)->ah_sh + (_reg)))
 
 /*
  * The functions in this section are not intended to be invoked by MadWifi
