#!/bin/sh /etc/rc.common
START=50

stop() {
	killall br2684ctl 2>/dev/null >/dev/null
	sleep 1
	rmmod br2684
}

start_daemon() {
	local cfg="$1"
	config_get atmdev "$cfg" atmdev
	config_get unit "$cfg" unit
	config_get vpi "$cfg" vpi
	config_get vci "$cfg" vci
	config_get encaps "$cfg" encaps
	config_get payload "$cfg" payload
	case "$encaps" in
		1|vc) encaps=1;;
		*) encaps=0;;
	esac
        case "$payload" in
                0|routed) payload=0;;
                *) payload=1;;
        esac
	br2684ctl -b -c "$unit" -e "$encaps" -p "$payload" -a "${atmdev:+$atmdev.}${vpi:-8}.${vci:-35}"	
}

start() {
	insmod br2684 >/dev/null 2>/dev/null
	config_load network
	config_foreach start_daemon atm-bridge
}
