I'm not sure if this is necessary, but the original driver did it and
apparently also many other drivers do it, so it should not be completely
wrong to do it.

Signed-off-by: Phil Sutter <n0-1@freewrt.org>
---
 drivers/net/korina.c |    2 ++
 1 files changed, 2 insertions(+), 0 deletions(-)

diff --git a/drivers/net/korina.c b/drivers/net/korina.c
index 75010ca..56b4db2 100644
--- a/drivers/net/korina.c
+++ b/drivers/net/korina.c
@@ -419,6 +419,7 @@ static int korina_rx(struct net_device *dev, int limit)
 			/* 16 bit align */
 			skb_reserve(skb_new, 2);
 
+			skb_new->dev = dev;
 			lp->rx_skb[lp->rx_next_done] = skb_new;
 		}
 
@@ -763,6 +764,7 @@ static void korina_alloc_ring(struct net_device *dev)
 		if (!skb)
 			break;
 		skb_reserve(skb, 2);
+		skb->dev = dev;
 		lp->rx_skb[i] = skb;
 		lp->rd_ring[i].control = DMA_DESC_IOD |
 				DMA_COUNT(KORINA_RBSIZE);
-- 
1.5.6.4


