RB_CONFIG="$(grep "RedBoot config" /proc/mtd | cut -d: -f1)"

for npe in eth0 eth1 eth2
do
	if [ "$(ifconfig $npe 2>/dev/null | grep -c 00:00:00:00:00:00)" == "1" ]; then
		ifconfig $npe hw ether $(fconfig -s -r -d /dev/$RB_CONFIG -n npe_"$npe"_esa)
	fi
done

# Some developers should be shot on sight at Zcom/Netgear
# -- Fixup for the WG302v1, need someone with a WAG302v1 to fix that, too

if [ "$(ifconfig eth0 2>/dev/null | grep -c 00:00:00:00:00:00)" == "1" ]; then
		ifconfig eth0 hw ether $(fconfig -s -r -d /dev/$RB_CONFIG -n zcom_npe_esa)
fi
