--- a/ath/if_ath.c
+++ b/ath/if_ath.c
@@ -8862,8 +8862,7 @@ ath_chan_set(struct ath_softc *sc, struc
 		 * needed to do the reset with chanchange = AH_FALSE in order
 		 * to receive traffic when peforming high velocity channel
 		 * changes. */
-		if (!ath_hal_reset(ah, sc->sc_opmode, &hchan, AH_TRUE, &status)   ||
-		    !ath_hal_reset(ah, sc->sc_opmode, &hchan, AH_FALSE, &status)) {
+		if (!ath_hal_reset(ah, sc->sc_opmode, &hchan, AH_TRUE, &status)) {
 			EPRINTF(sc, "Unable to reset channel %u (%u MHz) "
 				"flags 0x%x '%s' (HAL status %u)\n",
 				ieee80211_chan2ieee(ic, chan), chan->ic_freq,
