--- a/drivers/spi/Kconfig
+++ b/drivers/spi/Kconfig
@@ -100,6 +100,11 @@ config SPI_BUTTERFLY
 	  inexpensive battery powered microcontroller evaluation board.
 	  This same cable can be used to flash new firmware.
 
+config SPI_GPIO
+	tristate "GPIO API based bitbanging SPI controller"
+	depends on SPI_MASTER && GENERIC_GPIO && EXPERIMENTAL
+	select SPI_BITBANG
+
 config SPI_IMX
 	tristate "Freescale iMX SPI controller"
 	depends on SPI_MASTER && ARCH_IMX && EXPERIMENTAL
--- a/drivers/spi/Makefile
+++ b/drivers/spi/Makefile
@@ -16,6 +16,7 @@ obj-$(CONFIG_SPI_BFIN)			+= spi_bfin5xx.
 obj-$(CONFIG_SPI_BITBANG)		+= spi_bitbang.o
 obj-$(CONFIG_SPI_AU1550)		+= au1550_spi.o
 obj-$(CONFIG_SPI_BUTTERFLY)		+= spi_butterfly.o
+obj-$(CONFIG_SPI_GPIO)			+= spi_gpio.o
 obj-$(CONFIG_SPI_IMX)			+= spi_imx.o
 obj-$(CONFIG_SPI_LM70_LLP)		+= spi_lm70llp.o
 obj-$(CONFIG_SPI_PXA2XX)		+= pxa2xx_spi.o
