--- a/arch/arm/mach-orion5x/wnr854t-setup.c
+++ b/arch/arm/mach-orion5x/wnr854t-setup.c
@@ -15,6 +15,7 @@
 #include <linux/mtd/physmap.h>
 #include <linux/mv643xx_eth.h>
 #include <linux/ethtool.h>
+#include <net/dsa.h>
 #include <asm/mach-types.h>
 #include <asm/gpio.h>
 #include <asm/mach/arch.h>
@@ -97,6 +98,15 @@ static struct mv643xx_eth_platform_data 
 	.duplex		= DUPLEX_FULL,
 };
 
+static struct dsa_platform_data wnr854t_switch_data = {
+	.port_names[0] = "lan3",
+	.port_names[1] = "lan4",
+	.port_names[2] = "wan",
+	.port_names[3] = "cpu",
+	.port_names[5] = "lan1",
+	.port_names[7] = "lan2",
+};
+
 static void __init wnr854t_init(void)
 {
 	/*
@@ -110,6 +120,7 @@ static void __init wnr854t_init(void)
 	 * Configure peripherals.
 	 */
 	orion5x_eth_init(&wnr854t_eth_data);
+	orion5x_eth_switch_init(&wnr854t_switch_data, NO_IRQ);
 	orion5x_uart0_init();
 
 	orion5x_setup_dev_boot_win(WNR854T_NOR_BOOT_BASE,
