--- a/drivers/mmc/host/sdhci.c
+++ b/drivers/mmc/host/sdhci.c
@@ -481,16 +481,16 @@ static void sdhci_finish_data(struct sdh
 	 * Controller doesn't count down when in single block mode.
 	 */
 	if (data->blocks == 1)
-		blocks = (data->error == MMC_ERR_NONE) ? 0 : 1;
+		blocks = (data->error == 0) ? 0 : 1;
 	else
 		blocks = readw(host->ioaddr + SDHCI_BLOCK_COUNT);
 	data->bytes_xfered = data->blksz * (data->blocks - blocks);
 
-	if ((data->error == MMC_ERR_NONE) && blocks) {
+	if (!data->error && blocks) {
 		printk(KERN_ERR "%s: Controller signalled completion even "
 			"though there were blocks left.\n",
 			mmc_hostname(host->mmc));
-		data->error = MMC_ERR_FAILED;
+		data->error = -EIO;
 	}
 
 	if (data->stop) {
@@ -498,7 +498,7 @@ static void sdhci_finish_data(struct sdh
 		 * The controller needs a reset of internal state machines
 		 * upon error conditions.
 		 */
-		if (data->error != MMC_ERR_NONE) {
+		if (data->error) {
 			sdhci_reset(host, SDHCI_RESET_CMD);
 			sdhci_reset(host, SDHCI_RESET_DATA);
 		}
@@ -533,7 +533,7 @@ static void sdhci_send_command(struct sd
 			printk(KERN_ERR "%s: Controller never released "
 				"inhibit bit(s).\n", mmc_hostname(host->mmc));
 			sdhci_dumpregs(host);
-			cmd->error = MMC_ERR_FAILED;
+			cmd->error = -EIO;
 			tasklet_schedule(&host->finish_tasklet);
 			return;
 		}
@@ -554,7 +554,7 @@ static void sdhci_send_command(struct sd
 	if ((cmd->flags & MMC_RSP_136) && (cmd->flags & MMC_RSP_BUSY)) {
 		printk(KERN_ERR "%s: Unsupported response type!\n",
 			mmc_hostname(host->mmc));
-		cmd->error = MMC_ERR_INVALID;
+		cmd->error = -EINVAL;
 		tasklet_schedule(&host->finish_tasklet);
 		return;
 	}
@@ -601,7 +601,7 @@ static void sdhci_finish_command(struct 
 		}
 	}
 
-	host->cmd->error = MMC_ERR_NONE;
+	host->cmd->error = 0;
 
 	if (host->data && host->data_early)
 		sdhci_finish_data(host);
@@ -722,7 +722,7 @@ static void sdhci_request(struct mmc_hos
 	host->mrq = mrq;
 
 	if (!(readl(host->ioaddr + SDHCI_PRESENT_STATE) & SDHCI_CARD_PRESENT)) {
-		host->mrq->cmd->error = MMC_ERR_TIMEOUT;
+		host->mrq->cmd->error = -ENOMEDIUM;
 		tasklet_schedule(&host->finish_tasklet);
 	} else
 		sdhci_send_command(host, mrq->cmd);
@@ -831,7 +831,7 @@ static void sdhci_tasklet_card(unsigned 
 			sdhci_reset(host, SDHCI_RESET_CMD);
 			sdhci_reset(host, SDHCI_RESET_DATA);
 
-			host->mrq->cmd->error = MMC_ERR_FAILED;
+			host->mrq->cmd->error = -ENOMEDIUM;
 			tasklet_schedule(&host->finish_tasklet);
 		}
 	}
@@ -859,9 +859,9 @@ static void sdhci_tasklet_finish(unsigne
 	 * The controller needs a reset of internal state machines
 	 * upon error conditions.
 	 */
-	if ((mrq->cmd->error != MMC_ERR_NONE) ||
-		(mrq->data && ((mrq->data->error != MMC_ERR_NONE) ||
-		(mrq->data->stop && (mrq->data->stop->error != MMC_ERR_NONE))))) {
+	if (mrq->cmd->error ||
+		(mrq->data && (mrq->data->error ||
+		(mrq->data->stop && mrq->data->stop->error)))) {
 
 		/* Some controllers need this kick or reset won't work here */
 		if (host->chip->quirks & SDHCI_QUIRK_CLOCK_BEFORE_RESET) {
@@ -906,13 +906,13 @@ static void sdhci_timeout_timer(unsigned
 		sdhci_dumpregs(host);
 
 		if (host->data) {
-			host->data->error = MMC_ERR_TIMEOUT;
+			host->data->error = -ETIMEDOUT;
 			sdhci_finish_data(host);
 		} else {
 			if (host->cmd)
-				host->cmd->error = MMC_ERR_TIMEOUT;
+				host->cmd->error = -ETIMEDOUT;
 			else
-				host->mrq->cmd->error = MMC_ERR_TIMEOUT;
+				host->mrq->cmd->error = -ETIMEDOUT;
 
 			tasklet_schedule(&host->finish_tasklet);
 		}
@@ -941,13 +941,12 @@ static void sdhci_cmd_irq(struct sdhci_h
 	}
 
 	if (intmask & SDHCI_INT_TIMEOUT)
-		host->cmd->error = MMC_ERR_TIMEOUT;
-	else if (intmask & SDHCI_INT_CRC)
-		host->cmd->error = MMC_ERR_BADCRC;
-	else if (intmask & (SDHCI_INT_END_BIT | SDHCI_INT_INDEX))
-		host->cmd->error = MMC_ERR_FAILED;
+		host->cmd->error = -ETIMEDOUT;
+	else if (intmask & (SDHCI_INT_CRC | SDHCI_INT_END_BIT |
+			SDHCI_INT_INDEX))
+		host->cmd->error = -EILSEQ;
 
-	if (host->cmd->error != MMC_ERR_NONE)
+	if (host->cmd->error)
 		tasklet_schedule(&host->finish_tasklet);
 	else if (intmask & SDHCI_INT_RESPONSE)
 		sdhci_finish_command(host);
@@ -974,13 +973,11 @@ static void sdhci_data_irq(struct sdhci_
 	}
 
 	if (intmask & SDHCI_INT_DATA_TIMEOUT)
-		host->data->error = MMC_ERR_TIMEOUT;
-	else if (intmask & SDHCI_INT_DATA_CRC)
-		host->data->error = MMC_ERR_BADCRC;
-	else if (intmask & SDHCI_INT_DATA_END_BIT)
-		host->data->error = MMC_ERR_FAILED;
+		host->data->error = -ETIMEDOUT;
+	else if (intmask & (SDHCI_INT_DATA_CRC | SDHCI_INT_DATA_END_BIT))
+		host->data->error = -EILSEQ;
 
-	if (host->data->error != MMC_ERR_NONE)
+	if (host->data->error)
 		sdhci_finish_data(host);
 	else {
 		if (intmask & (SDHCI_INT_DATA_AVAIL | SDHCI_INT_SPACE_AVAIL))
@@ -1312,7 +1309,7 @@ static int __devinit sdhci_probe_slot(st
 	mmc->ops = &sdhci_ops;
 	mmc->f_min = host->max_clk / 256;
 	mmc->f_max = host->max_clk;
-	mmc->caps = MMC_CAP_4_BIT_DATA | MMC_CAP_MULTIWRITE | MMC_CAP_BYTEBLOCK;
+	mmc->caps = MMC_CAP_4_BIT_DATA | MMC_CAP_MULTIWRITE;
 
 	if (caps & SDHCI_CAN_DO_HISPD)
 		mmc->caps |= MMC_CAP_SD_HIGHSPEED;
