From ce7273c31fadb3143fc80c96a72a42adc19c2757 Mon Sep 17 00:00:00 2001
From: "Russell King (Oracle)" <rmk+kernel@armlinux.org.uk>
Date: Fri, 24 Nov 2023 12:28:24 +0000
Subject: [PATCH 4/7] net: phylink: pass PHY into phylink_validate_one()

Pass the phy (if any) into phylink_validate_one() so that we can
validate each interface with its rate matching setting.

Tested-by: Luo Jie <quic_luoj@quicinc.com>
Signed-off-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Link: https://lore.kernel.org/r/E1r6VIG-00DDLx-Cb@rmk-PC.armlinux.org.uk
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/phy/phylink.c | 7 +++++--
 1 file changed, 5 insertions(+), 2 deletions(-)

--- a/drivers/net/phy/phylink.c
+++ b/drivers/net/phy/phylink.c
@@ -724,7 +724,7 @@ static int phylink_validate_mac_and_pcs(
 	return phylink_is_empty_linkmode(supported) ? -EINVAL : 0;
 }
 
-static void phylink_validate_one(struct phylink *pl,
+static void phylink_validate_one(struct phylink *pl, struct phy_device *phy,
 				 const unsigned long *supported,
 				 const struct phylink_link_state *state,
 				 phy_interface_t interface,
@@ -739,6 +739,9 @@ static void phylink_validate_one(struct
 	tmp_state = *state;
 	tmp_state.interface = interface;
 
+	if (phy)
+		tmp_state.rate_matching = phy_get_rate_matching(phy, interface);
+
 	if (!phylink_validate_mac_and_pcs(pl, tmp_supported, &tmp_state)) {
 		phylink_dbg(pl, " interface %u (%s) rate match %s supports %*pbl\n",
 			    interface, phy_modes(interface),
@@ -760,7 +763,7 @@ static int phylink_validate_mask(struct
 	int interface;
 
 	for_each_set_bit(interface, interfaces, PHY_INTERFACE_MODE_MAX)
-		phylink_validate_one(pl, supported, state, interface,
+		phylink_validate_one(pl, NULL, supported, state, interface,
 				     all_s, all_adv);
 
 	linkmode_copy(supported, all_s);
