From b299ea0069284186b0d3d54aebe87f0d195d457a Mon Sep 17 00:00:00 2001
From: Heiner Kallweit <hkallweit1@gmail.com>
Date: Fri, 13 Dec 2024 20:01:41 +0100
Subject: [PATCH] r8169: adjust version numbering for RTL8126

Adjust version numbering for RTL8126, so that it doesn't overlap with
new RTL8125 versions.

Signed-off-by: Heiner Kallweit <hkallweit1@gmail.com>
Reviewed-by: Simon Horman <horms@kernel.org>
Link: https://patch.msgid.link/6a354364-20e9-48ad-a198-468264288757@gmail.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/realtek/r8169.h          |  4 +-
 drivers/net/ethernet/realtek/r8169_main.c     | 62 +++++++++----------
 .../net/ethernet/realtek/r8169_phy_config.c   |  4 +-
 3 files changed, 35 insertions(+), 35 deletions(-)

--- a/drivers/net/ethernet/realtek/r8169.h
+++ b/drivers/net/ethernet/realtek/r8169.h
@@ -69,8 +69,8 @@ enum mac_version {
 	RTL_GIGA_MAC_VER_61,
 	RTL_GIGA_MAC_VER_63,
 	RTL_GIGA_MAC_VER_64,
-	RTL_GIGA_MAC_VER_65,
-	RTL_GIGA_MAC_VER_66,
+	RTL_GIGA_MAC_VER_70,
+	RTL_GIGA_MAC_VER_71,
 	RTL_GIGA_MAC_NONE
 };
 
--- a/drivers/net/ethernet/realtek/r8169_main.c
+++ b/drivers/net/ethernet/realtek/r8169_main.c
@@ -139,8 +139,8 @@ static const struct {
 	/* reserve 62 for CFG_METHOD_4 in the vendor driver */
 	[RTL_GIGA_MAC_VER_63] = {"RTL8125B",		FIRMWARE_8125B_2},
 	[RTL_GIGA_MAC_VER_64] = {"RTL8125D",		FIRMWARE_8125D_1},
-	[RTL_GIGA_MAC_VER_65] = {"RTL8126A",		FIRMWARE_8126A_2},
-	[RTL_GIGA_MAC_VER_66] = {"RTL8126A",		FIRMWARE_8126A_3},
+	[RTL_GIGA_MAC_VER_70] = {"RTL8126A",		FIRMWARE_8126A_2},
+	[RTL_GIGA_MAC_VER_71] = {"RTL8126A",		FIRMWARE_8126A_3},
 };
 
 static const struct pci_device_id rtl8169_pci_tbl[] = {
@@ -1227,7 +1227,7 @@ static void rtl_writephy(struct rtl8169_
 	case RTL_GIGA_MAC_VER_31:
 		r8168dp_2_mdio_write(tp, location, val);
 		break;
-	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_71:
 		r8168g_mdio_write(tp, location, val);
 		break;
 	default:
@@ -1242,7 +1242,7 @@ static int rtl_readphy(struct rtl8169_pr
 	case RTL_GIGA_MAC_VER_28:
 	case RTL_GIGA_MAC_VER_31:
 		return r8168dp_2_mdio_read(tp, location);
-	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_71:
 		return r8168g_mdio_read(tp, location);
 	default:
 		return r8169_mdio_read(tp, location);
@@ -1573,7 +1573,7 @@ static void __rtl8169_set_wol(struct rtl
 		break;
 	case RTL_GIGA_MAC_VER_34:
 	case RTL_GIGA_MAC_VER_37:
-	case RTL_GIGA_MAC_VER_39 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_39 ... RTL_GIGA_MAC_VER_71:
 		r8169_mod_reg8_cond(tp, Config2, PME_SIGNAL, wolopts);
 		break;
 	default:
@@ -2046,7 +2046,7 @@ static void rtl_set_eee_txidle_timer(str
 		tp->tx_lpi_timer = timer_val;
 		r8168_mac_ocp_write(tp, 0xe048, timer_val);
 		break;
-	case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_71:
 		tp->tx_lpi_timer = timer_val;
 		RTL_W16(tp, EEE_TXIDLE_TIMER_8125, timer_val);
 		break;
@@ -2254,8 +2254,8 @@ static enum mac_version rtl8169_get_mac_
 		enum mac_version ver;
 	} mac_info[] = {
 		/* 8126A family. */
-		{ 0x7cf, 0x64a,	RTL_GIGA_MAC_VER_66 },
-		{ 0x7cf, 0x649,	RTL_GIGA_MAC_VER_65 },
+		{ 0x7cf, 0x64a,	RTL_GIGA_MAC_VER_71 },
+		{ 0x7cf, 0x649,	RTL_GIGA_MAC_VER_70 },
 
 		/* 8125D family. */
 		{ 0x7cf, 0x688,	RTL_GIGA_MAC_VER_64 },
@@ -2525,7 +2525,7 @@ static void rtl_init_rxcfg(struct rtl816
 	case RTL_GIGA_MAC_VER_61:
 		RTL_W32(tp, RxConfig, RX_FETCH_DFLT_8125 | RX_DMA_BURST);
 		break;
-	case RTL_GIGA_MAC_VER_63 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_63 ... RTL_GIGA_MAC_VER_71:
 		RTL_W32(tp, RxConfig, RX_FETCH_DFLT_8125 | RX_DMA_BURST |
 			RX_PAUSE_SLOT_ON);
 		break;
@@ -2657,7 +2657,7 @@ static void rtl_wait_txrx_fifo_empty(str
 	case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_61:
 		rtl_loop_wait_high(tp, &rtl_rxtx_empty_cond, 100, 42);
 		break;
-	case RTL_GIGA_MAC_VER_63 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_63 ... RTL_GIGA_MAC_VER_71:
 		RTL_W8(tp, ChipCmd, RTL_R8(tp, ChipCmd) | StopReq);
 		rtl_loop_wait_high(tp, &rtl_rxtx_empty_cond, 100, 42);
 		rtl_loop_wait_high(tp, &rtl_rxtx_empty_cond_2, 100, 42);
@@ -2926,7 +2926,7 @@ static void rtl_enable_exit_l1(struct rt
 	case RTL_GIGA_MAC_VER_37 ... RTL_GIGA_MAC_VER_38:
 		rtl_eri_set_bits(tp, 0xd4, 0x0c00);
 		break;
-	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_71:
 		r8168_mac_ocp_modify(tp, 0xc0ac, 0, 0x1f80);
 		break;
 	default:
@@ -2940,7 +2940,7 @@ static void rtl_disable_exit_l1(struct r
 	case RTL_GIGA_MAC_VER_34 ... RTL_GIGA_MAC_VER_38:
 		rtl_eri_clear_bits(tp, 0xd4, 0x1f00);
 		break;
-	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_71:
 		r8168_mac_ocp_modify(tp, 0xc0ac, 0x1f80, 0);
 		break;
 	default:
@@ -2966,8 +2966,8 @@ static void rtl_hw_aspm_clkreq_enable(st
 
 		rtl_mod_config5(tp, 0, ASPM_en);
 		switch (tp->mac_version) {
-		case RTL_GIGA_MAC_VER_65:
-		case RTL_GIGA_MAC_VER_66:
+		case RTL_GIGA_MAC_VER_70:
+		case RTL_GIGA_MAC_VER_71:
 			val8 = RTL_R8(tp, INT_CFG0_8125) | INT_CFG0_CLKREQEN;
 			RTL_W8(tp, INT_CFG0_8125, val8);
 			break;
@@ -2978,7 +2978,7 @@ static void rtl_hw_aspm_clkreq_enable(st
 
 		switch (tp->mac_version) {
 		case RTL_GIGA_MAC_VER_46 ... RTL_GIGA_MAC_VER_48:
-		case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_66:
+		case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_71:
 			/* reset ephy tx/rx disable timer */
 			r8168_mac_ocp_modify(tp, 0xe094, 0xff00, 0);
 			/* chip can trigger L1.2 */
@@ -2990,7 +2990,7 @@ static void rtl_hw_aspm_clkreq_enable(st
 	} else {
 		switch (tp->mac_version) {
 		case RTL_GIGA_MAC_VER_46 ... RTL_GIGA_MAC_VER_48:
-		case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_66:
+		case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_71:
 			r8168_mac_ocp_modify(tp, 0xe092, 0x00ff, 0);
 			break;
 		default:
@@ -2998,8 +2998,8 @@ static void rtl_hw_aspm_clkreq_enable(st
 		}
 
 		switch (tp->mac_version) {
-		case RTL_GIGA_MAC_VER_65:
-		case RTL_GIGA_MAC_VER_66:
+		case RTL_GIGA_MAC_VER_70:
+		case RTL_GIGA_MAC_VER_71:
 			val8 = RTL_R8(tp, INT_CFG0_8125) & ~INT_CFG0_CLKREQEN;
 			RTL_W8(tp, INT_CFG0_8125, val8);
 			break;
@@ -3719,12 +3719,12 @@ static void rtl_hw_start_8125_common(str
 	/* disable new tx descriptor format */
 	r8168_mac_ocp_modify(tp, 0xeb58, 0x0001, 0x0000);
 
-	if (tp->mac_version == RTL_GIGA_MAC_VER_65 ||
-	    tp->mac_version == RTL_GIGA_MAC_VER_66)
+	if (tp->mac_version == RTL_GIGA_MAC_VER_70 ||
+	    tp->mac_version == RTL_GIGA_MAC_VER_71)
 		RTL_W8(tp, 0xD8, RTL_R8(tp, 0xD8) & ~0x02);
 
-	if (tp->mac_version == RTL_GIGA_MAC_VER_65 ||
-	    tp->mac_version == RTL_GIGA_MAC_VER_66)
+	if (tp->mac_version == RTL_GIGA_MAC_VER_70 ||
+	    tp->mac_version == RTL_GIGA_MAC_VER_71)
 		r8168_mac_ocp_modify(tp, 0xe614, 0x0700, 0x0400);
 	else if (tp->mac_version == RTL_GIGA_MAC_VER_63)
 		r8168_mac_ocp_modify(tp, 0xe614, 0x0700, 0x0200);
@@ -3742,8 +3742,8 @@ static void rtl_hw_start_8125_common(str
 	r8168_mac_ocp_modify(tp, 0xe056, 0x00f0, 0x0030);
 	r8168_mac_ocp_modify(tp, 0xe040, 0x1000, 0x0000);
 	r8168_mac_ocp_modify(tp, 0xea1c, 0x0003, 0x0001);
-	if (tp->mac_version == RTL_GIGA_MAC_VER_65 ||
-	    tp->mac_version == RTL_GIGA_MAC_VER_66)
+	if (tp->mac_version == RTL_GIGA_MAC_VER_70 ||
+	    tp->mac_version == RTL_GIGA_MAC_VER_71)
 		r8168_mac_ocp_modify(tp, 0xea1c, 0x0300, 0x0000);
 	else
 		r8168_mac_ocp_modify(tp, 0xea1c, 0x0004, 0x0000);
@@ -3863,8 +3863,8 @@ static void rtl_hw_config(struct rtl8169
 		[RTL_GIGA_MAC_VER_61] = rtl_hw_start_8125a_2,
 		[RTL_GIGA_MAC_VER_63] = rtl_hw_start_8125b,
 		[RTL_GIGA_MAC_VER_64] = rtl_hw_start_8125d,
-		[RTL_GIGA_MAC_VER_65] = rtl_hw_start_8126a,
-		[RTL_GIGA_MAC_VER_66] = rtl_hw_start_8126a,
+		[RTL_GIGA_MAC_VER_70] = rtl_hw_start_8126a,
+		[RTL_GIGA_MAC_VER_71] = rtl_hw_start_8126a,
 	};
 
 	if (hw_configs[tp->mac_version])
@@ -3885,8 +3885,8 @@ static void rtl_hw_start_8125(struct rtl
 			RTL_W32(tp, i, 0);
 		break;
 	case RTL_GIGA_MAC_VER_63:
-	case RTL_GIGA_MAC_VER_65:
-	case RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_70:
+	case RTL_GIGA_MAC_VER_71:
 		for (i = 0xa00; i < 0xa80; i += 4)
 			RTL_W32(tp, i, 0);
 		RTL_W16(tp, INT_CFG1_8125, 0x0000);
@@ -4118,7 +4118,7 @@ static void rtl8169_cleanup(struct rtl81
 		RTL_W8(tp, ChipCmd, RTL_R8(tp, ChipCmd) | StopReq);
 		rtl_loop_wait_high(tp, &rtl_txcfg_empty_cond, 100, 666);
 		break;
-	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_71:
 		rtl_enable_rxdvgate(tp);
 		fsleep(2000);
 		break;
@@ -4275,7 +4275,7 @@ static unsigned int rtl_quirk_packet_pad
 
 	switch (tp->mac_version) {
 	case RTL_GIGA_MAC_VER_34:
-	case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_71:
 		padto = max_t(unsigned int, padto, ETH_ZLEN);
 		break;
 	default:
@@ -5294,7 +5294,7 @@ static void rtl_hw_initialize(struct rtl
 	case RTL_GIGA_MAC_VER_40 ... RTL_GIGA_MAC_VER_48:
 		rtl_hw_init_8168g(tp);
 		break;
-	case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_66:
+	case RTL_GIGA_MAC_VER_61 ... RTL_GIGA_MAC_VER_71:
 		rtl_hw_init_8125(tp);
 		break;
 	default:
--- a/drivers/net/ethernet/realtek/r8169_phy_config.c
+++ b/drivers/net/ethernet/realtek/r8169_phy_config.c
@@ -1162,8 +1162,8 @@ void r8169_hw_phy_config(struct rtl8169_
 		[RTL_GIGA_MAC_VER_61] = rtl8125a_2_hw_phy_config,
 		[RTL_GIGA_MAC_VER_63] = rtl8125b_hw_phy_config,
 		[RTL_GIGA_MAC_VER_64] = rtl8125d_hw_phy_config,
-		[RTL_GIGA_MAC_VER_65] = rtl8126a_hw_phy_config,
-		[RTL_GIGA_MAC_VER_66] = rtl8126a_hw_phy_config,
+		[RTL_GIGA_MAC_VER_70] = rtl8126a_hw_phy_config,
+		[RTL_GIGA_MAC_VER_71] = rtl8126a_hw_phy_config,
 	};
 
 	if (phy_configs[ver])
