#include "qcom-ipq8064-v2.0-smb208.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "TP-Link Archer VR2600v";
	compatible = "tplink,vr2600v", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	aliases {
		mdio-gpio0 = &mdio0;

		led-boot = &power;
		led-failsafe = &general;
		led-running = &power;
		led-upgrade = &general;
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		wifi {
			label = "wifi";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
			debounce-interval = <60>;
			wakeup-source;
		};

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 64 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};

		dect {
			label = "dect";
			gpios = <&qcom_pinmux 67 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_PHONE>;
			debounce-interval = <60>;
			wakeup-source;
		};

		ledswitch {
			label = "ledswitch";
			gpios = <&qcom_pinmux 68 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_LIGHTS_TOGGLE>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		dsl {
			label = "white:dsl";
			gpios = <&qcom_pinmux 7 GPIO_ACTIVE_HIGH>;
		};

		usb {
			function = LED_FUNCTION_USB;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&qcom_pinmux 8 GPIO_ACTIVE_HIGH>;
		};

		lan {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&qcom_pinmux 9 GPIO_ACTIVE_HIGH>;
		};

		wlan2g {
			label = "white:wlan2g";
			gpios = <&qcom_pinmux 16 GPIO_ACTIVE_HIGH>;
		};

		wlan5g {
			label = "white:wlan5g";
			gpios = <&qcom_pinmux 17 GPIO_ACTIVE_HIGH>;
		};

		power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&qcom_pinmux 26 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};

		phone {
			label = "white:phone";
			gpios = <&qcom_pinmux 53 GPIO_ACTIVE_HIGH>;
		};

		wan {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&qcom_pinmux 56 GPIO_ACTIVE_HIGH>;
		};

		general: general {
			label = "white:general";
			gpios = <&qcom_pinmux 66 GPIO_ACTIVE_HIGH>;
		};
	};
};

&qcom_pinmux {
	led_pins: led_pins {
		mux {
			pins = "gpio7", "gpio8", "gpio9", "gpio16", "gpio17",
				"gpio26", "gpio53", "gpio56", "gpio66";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	button_pins: button_pins {
		mux {
			pins = "gpio54", "gpio64", "gpio65", "gpio67", "gpio68";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	spi_pins: spi-state {
		/delete-property/ pins;
		/delete-property/ function;
		/delete-property/ drive-strength;
		/delete-property/ bias-disable;

		mux {
			pins = "gpio18", "gpio19", "gpio21";
			function = "gsbi5";
			bias-pull-down;
		};

		data {
			pins = "gpio18", "gpio19";
			drive-strength = <10>;
		};

		cs {
			pins = "gpio20";
			drive-strength = <10>;
			bias-pull-up;
		};

		clk {
			pins = "gpio21";
			drive-strength = <12>;
		};
	};
};

&gsbi5 {
	qcom,mode = <GSBI_PROT_SPI>;
	status = "okay";

	spi4: spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_LOW>;

		flash@0 {
			compatible = "jedec,spi-nor";
			#address-cells = <1>;
			#size-cells = <1>;
			spi-max-frequency = <50000000>;
			reg = <0>;

			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				partition@0 {
					label = "SBL1";
					reg = <0x0 0x20000>;
					read-only;
				};

				partition@20000 {
					label = "MIBIB";
					reg = <0x20000 0x20000>;
					read-only;
				};

				partition@40000 {
					label = "SBL2";
					reg = <0x40000 0x40000>;
					read-only;
				};

				partition@80000 {
					label = "SBL3";
					reg = <0x80000 0x80000>;
					read-only;
				};

				partition@100000 {
					label = "DDRCONFIG";
					reg = <0x100000 0x10000>;
					read-only;
				};

				partition@110000 {
					label = "SSD";
					reg = <0x110000 0x10000>;
					read-only;
				};

				partition@120000 {
					label = "TZ";
					reg = <0x120000 0x80000>;
					read-only;
				};

				partition@1a0000 {
					label = "RPM";
					reg = <0x1a0000 0x80000>;
					read-only;
				};

				partition@220000 {
					label = "APPSBL";
					reg = <0x220000 0x80000>;
					read-only;
				};

				partition@2a0000 {
					label = "APPSBLENV";
					reg = <0x2a0000 0x40000>;
					read-only;
				};

				partition@2e0000 {
					label = "OLDART";
					reg = <0x2e0000 0x40000>;
					read-only;
				};

				partition@320000 {
					label = "firmware";
					reg = <0x320000 0xc60000>;
					compatible = "openwrt,uimage";
					openwrt,offset = <512>; /* account for pad-extra 512 */
				};

				/* hole 0xf80000 - 0xfaf100 */

				partition@faf100 {
					label = "default-mac";
					reg = <0xfaf100 0x00200>;
					read-only;

					nvmem-layout {
						compatible = "fixed-layout";
						#address-cells = <1>;
						#size-cells = <1>;

						macaddr_defaultmac_0: macaddr@0 {
							compatible = "mac-base";
							reg = <0x0 0x6>;
							#nvmem-cell-cells = <1>;
						};
					};
				};

				partition@fc0000 {
					label = "ART";
					reg = <0xfc0000 0x40000>;
					read-only;

					nvmem-layout {
						compatible = "fixed-layout";
						#address-cells = <1>;
						#size-cells = <1>;

						precal_ART_1000: precal@1000 {
							reg = <0x1000 0x2f20>;
						};

						precal_ART_5000: precal@5000 {
							reg = <0x5000 0x2f20>;
						};
					};
				};
			};
		};
	};
};

&hs_phy_0 {
	status = "okay";
};

&ss_phy_0 {
	status = "okay";
};

&usb3_0 {
	status = "okay";
};

&hs_phy_1 {
	status = "okay";
};

&ss_phy_1 {
	status = "okay";
};

&usb3_1 {
	status = "okay";
};

&pcie0 {
	status = "okay";
};

&pcie_bridge0 {
	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x00010000 0 0 0 0>;
		nvmem-cells = <&macaddr_defaultmac_0 (-1)>, <&precal_ART_1000>;
		nvmem-cell-names = "mac-address", "pre-calibration";
	};
};

&pcie1 {
	status = "okay";
	max-link-speed = <1>;
};

&pcie_bridge1 {
	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x00010000 0 0 0 0>;
		nvmem-cells = <&macaddr_defaultmac_0 0>, <&precal_ART_5000>;
		nvmem-cell-names = "mac-address", "pre-calibration";
	};
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	switch@10 {
		compatible = "qca,qca8337";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x10>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "cpu";
				ethernet = <&gmac1>;
				phy-mode = "rgmii";
				tx-internal-delay-ps = <1000>;
				rx-internal-delay-ps = <1000>;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};

			port@1 {
				reg = <1>;
				label = "lan4";
				phy-mode = "internal";
				phy-handle = <&phy_port1>;
			};

			port@2 {
				reg = <2>;
				label = "lan3";
				phy-mode = "internal";
				phy-handle = <&phy_port2>;
			};

			port@3 {
				reg = <3>;
				label = "lan2";
				phy-mode = "internal";
				phy-handle = <&phy_port3>;
			};

			port@4 {
				reg = <4>;
				label = "lan1";
				phy-mode = "internal";
				phy-handle = <&phy_port4>;
			};

			port@5 {
				reg = <5>;
				label = "wan";
				phy-mode = "internal";
				phy-handle = <&phy_port5>;
			};

			port@6 {
				reg = <6>;
				label = "cpu";
				ethernet = <&gmac2>;
				phy-mode = "sgmii";
				qca,sgmii-enable-pll;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};

		mdio {
			#address-cells = <1>;
			#size-cells = <0>;

			phy_port1: phy@0 {
				reg = <0>;
			};

			phy_port2: phy@1 {
				reg = <1>;
			};

			phy_port3: phy@2 {
				reg = <2>;
			};

			phy_port4: phy@3 {
				reg = <3>;
			};

			phy_port5: phy@4 {
				reg = <4>;
			};
		};
	};
};

&gmac1 {
	status = "okay";
	phy-mode = "rgmii";
	qcom,id = <1>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	nvmem-cells = <&macaddr_defaultmac_0 1>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";
	phy-mode = "sgmii";
	qcom,id = <2>;

	nvmem-cells = <&macaddr_defaultmac_0 0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&adm_dma {
	status = "okay";
};
