(footprint "0908SQ-23N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.5 -2 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ff5069db-971e-4012-a8fe-79a0beeecba2")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "0908SQ-23N"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c788aafb-994d-4f0d-a772-19139ed4b02a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.coilcraft.com/getmedia/b4a6ff85-4c1f-448e-aea7-541369538706/sq_spring.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "69f6b539-b4d8-480f-bee6-8714df5845b6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Square Air Core Inductor 24 nH, Q>120, I_rms=4.4 A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cbff2ecb-ae54-4bf8-ad5c-7f89f71cb09b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.5 -1.4)
		(end 0.5 -1.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "89716351-aa68-45c5-9c3e-57a3f007a040")
	)
	(fp_line
		(start -0.5 1.4)
		(end -0.5 1.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "cea89c5b-1ac2-48fe-a52f-4eaaf0b14cf0")
	)
	(fp_line
		(start -0.5 1.4)
		(end 0.5 1.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1d3ae979-5ae2-473f-8263-c0f541358936")
	)
	(fp_rect
		(start -1.3 -1.4)
		(end 1.3 1.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "2381b2f1-d50e-475d-b21e-9824096947db")
	)
	(fp_line
		(start -1.2 -1.3)
		(end -1.2 1.3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "4ebbb063-9f45-469d-9765-d35393b51da2")
	)
	(fp_line
		(start -1.2 -1.3)
		(end 1.2 -1.3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a13d60b6-8e9f-4ab4-8d58-b542c5386432")
	)
	(fp_line
		(start -1.2 1.3)
		(end 1.2 1.3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "26a9057f-9cb3-4820-8fb7-a169dafbc550")
	)
	(fp_line
		(start 1.2 1.3)
		(end 1.2 -1.3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0895da63-d22e-4748-bfb3-4df06a7f00db")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d81c5e90-a27e-4bbc-94be-a0bf45dfe818")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.95 0)
		(size 0.64 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "1835b1b7-3832-4dc2-9517-716f0ba370c6")
	)
	(pad "2" smd roundrect
		(at 0.95 0)
		(size 0.64 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "cf1fda8d-d25a-4927-a438-7274d4ea4823")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/parts/parts.3dshapes/Coilcraft-0908SQ-23N.step"
		(offset
			(xyz -1 -0.9 0.15)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
