(footprint "Connector_SMA_4x10mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMA THT connector used in the Retevis C62 radio")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "80102fe9-2f24-4f9f-af06-d957a2339c3f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "SMA 4x10mm"
		(at 0 2.2 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a34d2d62-0765-4da1-ac9b-635ed076b59b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "48f94bd9-c136-4e26-9877-e2fb97835e49")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "905148bf-d207-4ac9-b1d9-6ecfe4380d18")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -5 -8.1)
		(end 5 -8.1)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "18f6e088-da08-4668-8d80-c7d79016a9fc")
	)
	(fp_line
		(start -5 -5.95)
		(end -5 -8.1)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fa4fe366-408f-40d3-9128-0e4577149e01")
	)
	(fp_line
		(start -4.5 -13.2)
		(end 4.5 -13.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "badf7925-5582-499b-9c06-d9bc6933b1fc")
	)
	(fp_line
		(start -4.5 -8.15)
		(end -4.5 -13.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "27cdc8fc-256e-4503-a5d1-d81e2654d22c")
	)
	(fp_line
		(start -4.5 -4.1)
		(end -4.5 -2.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "957f27b0-d499-4157-a0c2-493d05066f58")
	)
	(fp_line
		(start -4.5 -2.1)
		(end 4.5 -2.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9dba7657-71b2-4a08-baa6-15373c45aee6")
	)
	(fp_line
		(start -1.3 -0.4)
		(end -1.3 -2.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "669a12b8-52ee-481c-9e87-5e167ef06e28")
	)
	(fp_line
		(start 1.3 -0.4)
		(end 1.3 -2.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "433ca06d-cd4f-40a0-9f39-38c104bc18b2")
	)
	(fp_line
		(start 3 -4.1)
		(end -3 -4.1)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2d8c67bf-57cd-4c7b-b11b-0b9090a11228")
	)
	(fp_line
		(start 4.5 -13.2)
		(end 4.5 -8.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "abb8244f-ffa0-46ce-8187-a7e74a5c6a09")
	)
	(fp_line
		(start 4.5 -2.1)
		(end 4.5 -4.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b506e301-9ea3-460a-beda-b6c8179b844e")
	)
	(fp_line
		(start 5 -8.1)
		(end 5 -5.95)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "bca821a7-5e69-45e2-8cd9-19084b97066c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 3.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a9b10697-3ad2-4023-8a79-ffea0bd057da")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.54 2.54)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6f2a2976-cd88-4bc1-adce-86ec51a01457")
	)
	(pad "2" thru_hole circle
		(at -3.75 -5.3)
		(size 2.54 2.54)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c109aca4-9b17-4cf4-8b80-1351643c20e9")
	)
	(pad "2" thru_hole circle
		(at 3.75 -5.3)
		(size 2.54 2.54)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f95e716f-1f15-4a03-b50c-54d6f9b32a3b")
	)
	(embedded_fonts no)
)
