(footprint "TSLP-6-4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "9a3aa994-7536-4476-8bbd-9288fdef0981")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "TSLP-6-4"
		(at 0 4 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "554a6a3a-c5b5-44b5-9b8a-9c3f9aa95e65")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "722e2fa2-2250-459c-86f5-8a3b3ae214ff")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0d1bb7dc-584f-4382-80d5-b23565a514a9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.6 -0.4)
		(end -0.6 0.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3d37ef7f-8599-4bf9-9c8c-91e87602fec8")
	)
	(fp_line
		(start -0.6 0.4)
		(end 0.6 0.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a33bb430-f018-4354-81a7-2feb19fc6c4d")
	)
	(fp_line
		(start 0.6 -0.4)
		(end -0.6 -0.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6206b217-745f-41b5-8927-3a6521fbca39")
	)
	(fp_line
		(start 0.6 0.4)
		(end 0.6 -0.4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2c0478b5-8d08-406f-b948-308850df27d6")
	)
	(fp_circle
		(center -0.4 0.6)
		(end -0.35 0.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "209f785e-4e73-40e1-99b2-22eef1dbf8a5")
	)
	(fp_rect
		(start -0.6 -0.4)
		(end 0.6 0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "397f203a-b7bb-4093-bf45-a70ef770ea73")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "6b57fcbd-de44-426a-9b74-0e06d8ac28b7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -0.4 0.2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "798dc9c6-aeb5-4fd3-ba28-4c7976b067a9")
	)
	(pad "2" smd rect
		(at 0 0.2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "61bddb5c-6543-4ce9-965d-5375577ea6a7")
	)
	(pad "3" smd rect
		(at 0.4 0.2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "96cb11f3-a07b-44e4-938a-aaa5e43318f4")
	)
	(pad "4" smd rect
		(at 0.4 -0.2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "cb640787-be88-4c19-b745-6e4c1e49220c")
	)
	(pad "5" smd rect
		(at 0 -0.2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "77135aea-84e9-4862-88e7-9f369b2819b4")
	)
	(pad "6" smd rect
		(at -0.4 -0.2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c75de03e-2563-4420-890d-efbd9af79182")
	)
	(embedded_fonts no)
)
