(footprint "LG77L"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint of the Quectel LG77L GNSS module")
	(property "Reference" "REF**"
		(at -2.6 -4.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5a4a5c43-0705-4e50-a7d4-086544a98c0e")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "LG77L"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f118f25f-baa0-401f-bc89-ad33a73892ae")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d2c786e6-4cab-4760-950d-efcc0684fb4e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Footprint of the Quectel LG77L GNSS module"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d71725b2-61d6-4d32-adb0-a029871e94f4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.7 -3.7)
		(end -3.15 -3.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "998a6c69-d629-4dc8-96a8-f738f45ebe67")
	)
	(fp_line
		(start -3.7 -3.35)
		(end -3.35 -3.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1273686e-e3e6-4fc8-9308-84fb6efca4df")
	)
	(fp_line
		(start -3.7 -3.15)
		(end -3.7 -3.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6e1c00a2-8509-4454-ac10-f4b5b854a1dc")
	)
	(fp_line
		(start -3.5 -3.5)
		(end 3.5 -3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4fd4c71a-3ee3-42ae-b2d7-1945f1aae112")
	)
	(fp_line
		(start -3.5 3.5)
		(end -3.5 -3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7aae71df-5d86-4554-af04-60abf87632d0")
	)
	(fp_line
		(start -3.5 3.5)
		(end 3.5 3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "48996a6c-9adf-4ef1-8aa5-214cf10145a8")
	)
	(fp_line
		(start 3.5 3.5)
		(end 3.5 -3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "039ccfb8-4512-4397-944d-6c63f82aebe9")
	)
	(fp_rect
		(start -3.7 -3.7)
		(end 3.7 3.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "a42469c2-6809-4336-b217-97a467bf35e0")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "8c8aca7e-4089-4f4a-bd9e-86cba41b2b05")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -3.15 -2.6)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "8434dda3-042d-4d5f-9e27-84b5860c5093")
	)
	(pad "2" smd rect
		(at -3.15 -1.95)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "c0a13736-a7a3-4fe6-8385-080d9328e44c")
	)
	(pad "3" smd rect
		(at -3.15 -1.3)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "ce1e8130-2d7a-470e-a56d-e6951d72f81c")
	)
	(pad "4" smd rect
		(at -3.15 -0.65)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "d76a556c-d202-4abc-8cf1-f38b2a758bec")
	)
	(pad "5" smd rect
		(at -3.15 0)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "05396c81-0ffc-46e4-944e-9a25178566e9")
	)
	(pad "6" smd rect
		(at -3.15 0.65)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "407ee700-8dcf-4120-9e66-f763afbc5ead")
	)
	(pad "7" smd rect
		(at -3.15 1.3)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "4579ae85-a8d3-4772-9415-0569937fcdda")
	)
	(pad "8" smd rect
		(at -3.15 1.95)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "047fa1e4-514b-42ba-85c1-02c289eb6e90")
	)
	(pad "9" smd rect
		(at -3.15 2.6)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "58b7dda1-8943-4a42-9800-e08f86b4ef9c")
	)
	(pad "10" smd rect
		(at -2.6 3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "50a02efc-846c-4881-8f8c-ca92ff96d451")
	)
	(pad "11" smd rect
		(at -1.95 3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "f4b4525b-28e1-4f80-ae49-2029f055bea0")
	)
	(pad "12" smd rect
		(at -1.3 3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "64d2a0d3-495a-4414-8c8c-1ba56a807045")
	)
	(pad "13" smd rect
		(at -0.65 3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "bb66b982-d048-48e4-9453-a1c3e7267812")
	)
	(pad "14" smd rect
		(at 0 3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "a4ddce47-348e-49ce-bffb-65afb37d16b7")
	)
	(pad "15" smd rect
		(at 0.65 3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "7035dbbc-981d-41ad-84c6-0c3c676a5e5d")
	)
	(pad "16" smd rect
		(at 1.3 3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "37acf533-9106-4968-a12e-5a5f08605f42")
	)
	(pad "17" smd rect
		(at 1.95 3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "e2ec9451-a34b-4910-93c0-fb3b88a0b35d")
	)
	(pad "18" smd rect
		(at 2.6 3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "21d1a3e3-b919-4d59-9641-4f5da2962429")
	)
	(pad "19" smd rect
		(at 3.15 2.6)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "47bc0a58-f13a-4868-a995-85758b92e88e")
	)
	(pad "20" smd rect
		(at 3.15 1.95)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "f41feb9f-7549-429f-8019-f3e7ecccf621")
	)
	(pad "21" smd rect
		(at 3.15 1.3)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "2b09dd2e-bf6c-45d9-a069-b5a2fefa906d")
	)
	(pad "22" smd rect
		(at 3.15 0.65)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "d1ec8d28-096e-480e-94fa-f5a8845d0318")
	)
	(pad "23" smd rect
		(at 3.15 0)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "ec875793-5a2b-40bf-9420-61bc489ad12f")
	)
	(pad "24" smd rect
		(at 3.15 -0.65)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "a97d1315-d260-46cf-8244-ff5eb24204da")
	)
	(pad "25" smd rect
		(at 3.15 -1.3)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "28019ec8-b73a-443f-ba70-a61f82c73447")
	)
	(pad "26" smd rect
		(at 3.15 -1.95)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "58ab1220-483d-45fe-9383-468e81974f43")
	)
	(pad "27" smd rect
		(at 3.15 -2.6)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "18bba525-ac4c-40ac-97af-7ebdf52dac0a")
	)
	(pad "28" smd rect
		(at 2.6 -3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "541b85a6-f955-4be8-aa6e-4e5dce3401c8")
	)
	(pad "29" smd rect
		(at 1.95 -3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "2d4cfb5d-b913-4dc5-8c06-371feb1d4bbc")
	)
	(pad "30" smd rect
		(at 1.3 -3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "29987e7e-274e-49a3-8817-b8378febf272")
	)
	(pad "31" smd rect
		(at 0.65 -3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "d7fd6692-c079-4646-abff-75f2e7df79b9")
	)
	(pad "32" smd rect
		(at 0 -3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "3596584a-a93b-4ad5-a2f2-a73afbe7dbea")
	)
	(pad "33" smd rect
		(at -0.65 -3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "eeab4309-eb26-45db-a549-dfd3690125d3")
	)
	(pad "34" smd rect
		(at -1.3 -3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "6e376d9d-099a-49a4-81f2-5344d7e3cd27")
	)
	(pad "35" smd rect
		(at -1.95 -3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "813acad6-3d64-4053-a12b-80ebb2298b7c")
	)
	(pad "36" smd rect
		(at -2.6 -3.15 90)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "f13c26d2-baef-4b84-9a2d-32df5705f1f8")
	)
	(pad "37" smd rect
		(at -1.3 -1.3)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "b6275dd6-7d9e-42a1-81b8-fd408bebb21a")
	)
	(pad "38" smd rect
		(at 0 -1.3)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "d8a54cb3-569a-4560-8ab4-9f43260d88ad")
	)
	(pad "39" smd rect
		(at -1.3 0)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "7eb9a52c-4fbb-49c3-b036-dfdcc2b61134")
	)
	(pad "40" smd rect
		(at 0 0)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "a3da43f2-323c-423e-befa-222fb4d903ce")
	)
	(pad "41" smd rect
		(at -1.3 1.3)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "a2c16c35-2246-48ef-8721-736d46cf2d53")
	)
	(pad "42" smd rect
		(at 0 1.3)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "5f77703a-3395-4a33-8d43-c8e48a729fa2")
	)
	(pad "43" smd rect
		(at 1.3 1.3)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(uuid "1713a5bf-e34d-421f-8fd8-c1467d39d23f")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/parts/parts.3dshapes/LG77L.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
