(footprint "Jack_2.5mm_PJ-204_nodrill_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TRS 2.5mm, horizontal, through-hole, https://www.jbl-ec.com/pj-204-audio-jack-2-5mm-dip-5pin-dc12v-1a-right-angle-stereo-jack-product/")
	(tags "TRS audio jack stereo horizontal")
	(property "Reference" "REF**"
		(at 0 -0.9 0)
		(layer "F.SilkS")
		(uuid "1add7dcf-a760-4acf-a8df-7191842316d8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Jack_2.5mm_PJ-204_nodrill_Horizontal"
		(at 0 -10 0)
		(layer "F.Fab")
		(uuid "6612f225-863e-4980-926d-c81f7a4c0ba5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "87b43f88-e722-4fe0-a9f0-7872afe98c67")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fcc3ef8c-8425-4c05-ab28-aa0bbbe4a25a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -5 0)
		(end -5 9.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c78b5373-444d-46df-a7ff-7918695524aa")
	)
	(fp_line
		(start -5 0)
		(end 5 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "37df54e5-cc8c-41e4-84e7-55d2f9716bba")
	)
	(fp_line
		(start -5 9.5)
		(end 5 9.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c90c2cac-c094-4a44-8573-9eade1ac1d10")
	)
	(fp_line
		(start -2.5 9.5)
		(end -2.5 12)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "24e7a552-df83-426c-b60f-fe2f1fbc809e")
	)
	(fp_line
		(start -2.5 12)
		(end 2.5 12)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "94f970ba-e83e-49a0-b986-74fd1ecd5c78")
	)
	(fp_line
		(start 2.5 12)
		(end 2.5 9.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f29f4406-918d-48c2-9b74-351874647dc4")
	)
	(fp_line
		(start 5 0)
		(end 5 9.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fb781b1e-c884-42ea-9fa8-fe7a1786fd68")
	)
	(fp_line
		(start -5.2 10.2)
		(end -2.8 10.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "1f9968e1-0eee-4dd9-9f60-e366337fcb8a")
	)
	(fp_line
		(start -2.8 9.5)
		(end -2.8 10.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "c31c5813-442f-4ad2-960c-3f73d806ce53")
	)
	(fp_line
		(start -2.5 9.2)
		(end 2.5 9.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "dbb57839-1d85-4f3a-9ffc-784b41399dbf")
	)
	(fp_line
		(start 2.8 9.5)
		(end 2.8 10.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "86375f01-fc12-4053-b820-79f7aa5c8146")
	)
	(fp_line
		(start 2.8 10.2)
		(end 5.2 10.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "978a124b-c077-4e1d-a7de-ec1e47637e18")
	)
	(fp_arc
		(start -2.8 9.5)
		(mid -2.712132 9.287868)
		(end -2.5 9.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "dbde7e21-8636-4297-9d29-cd1d0d9efbd0")
	)
	(fp_arc
		(start 2.5 9.2)
		(mid 2.712132 9.287868)
		(end 2.8 9.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "65bc386a-a6e4-4a0e-84da-1422f63a936a")
	)
	(fp_line
		(start -5.2 -0.2)
		(end 5.2 -0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "97966214-2210-4448-a880-744d95a73b87")
	)
	(fp_line
		(start -5.2 9.7)
		(end -5.2 -0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1f6ed11b-79cd-45f6-959e-7f2fbf90f69a")
	)
	(fp_line
		(start -2.7 9.7)
		(end -5.2 9.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b74f1fa6-5829-409a-b994-da1bf9a13516")
	)
	(fp_line
		(start -2.7 12.2)
		(end -2.7 9.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c3ca5317-fc50-4144-9d59-8647b18b887e")
	)
	(fp_line
		(start 2.7 9.7)
		(end 2.7 12.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "308ca0d3-88bf-4641-a81c-63b2cb244e99")
	)
	(fp_line
		(start 2.7 12.2)
		(end -2.7 12.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cdbf1a26-9172-42d0-8e5f-d28b5324d8c7")
	)
	(fp_line
		(start 5.2 -0.2)
		(end 5.2 9.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e89ed8b8-dbbf-45a7-b867-1502c7286eb3")
	)
	(fp_line
		(start 5.2 9.7)
		(end 2.7 9.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bf50228b-3ef5-443b-87fe-7d588817c57b")
	)
	(fp_text user "PCB edge"
		(at 0 8.2 0)
		(unlocked yes)
		(layer "Dwgs.User")
		(uuid "280aa230-a25f-414c-9d84-47f182621149")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0.1 0.9 0)
		(layer "F.Fab")
		(uuid "085988cb-9879-4ac3-a25a-5a2bd7285627")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "R" thru_hole oval
		(at -4 5 90)
		(size 1.8 1)
		(drill oval 1.1 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5aecb324-b167-40b9-a41d-67a6469e1fa6")
	)
	(pad "RN" thru_hole circle
		(at -4 7)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "565d8018-5776-4af4-939a-4fc9b4a6d31a")
	)
	(pad "S" thru_hole oval
		(at 2 7.1 90)
		(size 1.8 1)
		(drill oval 1.1 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2a9c9215-8df3-4b75-b688-d6e63cc11eab")
	)
	(pad "T" thru_hole oval
		(at 4 6 90)
		(size 1.8 1)
		(drill oval 1.1 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "90bc0af0-53b1-40e6-82a5-896c9d0526e7")
	)
	(pad "TN" thru_hole circle
		(at 4 4)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5a3cd8fb-44ec-4d5b-9655-c80e908a60e3")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/parts/parts.3dshapes/PJ-204.STEP"
		(offset
			(xyz 0 -4.7 2.51)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
