(footprint "Fuse_1812L200"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "16V 2A 100A 4A 20mΩ 1812 PTC Resettable Fuses")
	(property "Reference" "REF**"
		(at 0 -2.05 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "af2fd0fe-a6b0-4ede-99e9-afca1a15eabe")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.15)
				(bold yes)
			)
		)
	)
	(property "Value" "1812L200"
		(at 0 2.4 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c2b87a99-99c0-4a9a-92c4-2df3f5800af5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c084fba9-c381-4ee9-9f09-3125d2a42c7b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "16V 2A 100A 4A 20mΩ 1812 PTC Resettable Fuses"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2deff168-1cff-4a8b-8de0-8c1c73a28161")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.3 -1.5)
		(end 1.3 -1.5)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "80f3575f-ad24-4bef-8c93-21539d1c40ae")
	)
	(fp_line
		(start 1.3 1.5)
		(end -1.3 1.5)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e795d725-0e38-471c-9559-6d528f447fae")
	)
	(fp_rect
		(start -3.35 -1.7)
		(end 3.35 1.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "c6a858da-55df-47c9-afc8-8a6ceb14ddf0")
	)
	(fp_rect
		(start -2.25 -1.55)
		(end 2.25 1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "269c2f99-0ae4-4b3e-9260-e2fe6830033e")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7d52f6eb-3607-49d7-b956-aba6f75e540b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.2 0)
		(size 1.6 3.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "1596402f-1968-4744-8536-4d34377fd0f1")
	)
	(pad "2" smd roundrect
		(at 2.2 0)
		(size 1.6 3.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "4f990784-974c-4158-9f6c-1dc006e80997")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/parts/parts.3dshapes/F1812_L4.5-W3.2-H1.0.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
