{
	"ifname": "test1",
	"enabled": true,
	"status": "running",
	"ssid": "iopsysWrt-44D43771B810",
	"bssid": "44:d4:37:71:b8:1f",
	"security": "WPA2PSK",
	"encryption": "CCMP",
	"channel": 36,
	"bandwidth": 80,
	"standard": "802.11a/n/ac/ax",
	"num_stations": 1,
	"max_stations": 64,
	"utilization": 6,
	"adm_capacity": 0,
	"hidden": false,
	"supp_security": [
		"NONE",
		"WEP64",
		"WEP128",
		"WPAPSK",
		"WPA2PSK",
		"WPA3PSK",
		"WPAPSK+WPA2PSK",
		"WPA2PSK+WPA3PSK",
		"WPA",
		"WPA2",
		"WPA3",
		"WPA+WPA2",
		"WPA2+WPA3",
		"WPA3PSK+FT",
		"WPA2PSK+FT"
	],
	"capabilities": {
		"wmm": true,
		"apsd": true,
		"shortslot": false,
		"dot11h": true,
		"2040coex": false,
		"psmp": false,
		"proxy_arp": false,
		"dot11v_btm": true,
		"dot11n": {
			"dot11n_ldpc": true,
			"dot11n_40": true,
			"dot11n_ps": true,
			"dot11n_sgi20": true,
			"dot11n_sgi40": true,
			"dot11n_tx_stbc": false,
			"dot11n_rx_stbc": false,
			"dot11n_supp_max_mcs": 31
		},
		"dot11ac": {
			"dot11ac_160": false,
			"dot11ac_8080": false,
			"dot11ac_mpdu_max": 7991,
			"dot11ac_sgi80": true,
			"dot11ac_sgi160": false,
			"dot11ac_rx_ldpc": true,
			"dot11ac_tx_stbc": false,
			"dot11ac_rx_stbc_1ss": false,
			"dot11ac_rx_stbc_2ss": false,
			"dot11ac_rx_stbc_3ss": false,
			"dot11ac_rx_stbc_4ss": false,
			"dot11ac_su_beamformer": true,
			"dot11ac_su_beamformee": false,
			"dot11ac_mu_beamformer": true,
			"dot11ac_mu_beamformee": false,
			"dot11ac_supp_max_rx_mcs": 9,
			"dot11ac_supp_max_rx_nss": 4,
			"dot11ac_supp_max_tx_mcs": 9,
			"dot11ac_supp_max_tx_nss": 4
		},
		"dot11ax": {
			"dot11ax_twt_requester": false,
			"dot11ax_twt_responder": true,
			"dot11ax_all_ack": false,
			"dot11ax_trs": false,
			"dot11ax_bsr": true,
			"dot11ax_twt_bcast": false,
			"dot11ax_ba_32bit": false,
			"dot11ax_om_control": true,
			"dot11ax_ofdma_ra": false,
			"dot11ax_amsdu_frag": true,
			"dot11ax_twt_flexible": false,
			"dot11ax_qtp": false,
			"dot11ax_bqr": false,
			"dot11ax_srp_responder": false,
			"dot11ax_ops": false,
			"dot11ax_amsdu_in_ampdu": false,
			"dot11ax_dynamic_smps": false,
			"dot11ax_2g_40": false,
			"dot11ax_5g_4080": true,
			"dot11ax_5g_160": false,
			"dot11ax_5g_160_and_8080": false,
			"dot11ax_2g_242ru": false,
			"dot11ax_5g_242ru": false,
			"dot11ax_ldpc_payload": true,
			"dot11ax_tx_stbc_80": false,
			"dot11ax_rx_stbc_80": false,
			"dot11ax_ul_mumimo_full": false,
			"dot11ax_ul_mumimo_partial": false,
			"dot11ax_su_beamformer": true,
			"dot11ax_su_beamformee": true,
			"dot11ax_mu_beamformer": true,
			"dot11ax_supp_max_rx_mcs_80": 11,
			"dot11ax_supp_max_rx_nss_80": 4,
			"dot11ax_supp_max_tx_mcs_80": 11,
			"dot11ax_supp_max_tx_nss_80": 4
		},
		"dot11k": {
			"dot11k_link_meas": true,
			"dot11k_nbr_report": true,
			"dot11k_bcn_passive": true,
			"dot11k_bcn_active": true,
			"dot11k_bcn_table": true,
			"dot11k_rcpi": false,
			"dot11k_rsni": false
		}
	},
	"wmm_params": [
		{
			"ac": "BE",
			"aifsn": 3,
			"cwmin": 4,
			"cwmax": 10,
			"txop": 0
		},
		{
			"ac": "BK",
			"aifsn": 7,
			"cwmin": 4,
			"cwmax": 10,
			"txop": 0
		},
		{
			"ac": "VI",
			"aifsn": 2,
			"cwmin": 3,
			"cwmax": 4,
			"txop": 94
		},
		{
			"ac": "VO",
			"aifsn": 2,
			"cwmin": 2,
			"cwmax": 3,
			"txop": 47
		}
	]
}
