{
	"radio": "test2",
	"macaddr": "44:d4:37:71:b8:1e",
	"firmware": "test2: Aug 31 2021 22:20:08 version 17.10.157.2805 (r796514 WLTEST)",
	"vendor_id": "0x14e4",
	"device_id": "0xf6ca",
	"isup": true,
	"band": "2.4GHz",
	"standard": "802.11g/n/ax",
	"num_iface": 1,
	"iface": [
		{
			"name": "test2",
			"mode": "ap"
		}
	],
	"opclass": 81,
	"channel": 11,
	"bandwidth": 20,
	"channel_ext": "none",
	"tx_streams": 2,
	"rx_streams": 2,
	"noise": -83,
	"guard_int": "Auto",
	"maxrate": 286,
	"supp_bands": [
		"2.4GHz"
	],
	"supp_std": [
		"11b",
		"11g",
		"11n",
		"11ac",
		"11ax"
	],
	"supp_bw": [
		"20MHz",
		"40MHz"
	],
	"supp_rates": [
		
	],
	"basic_rates": [
		
	],
	"supp_channels": [
		{
			"opclass": 81,
			"bandwidth": 20,
			"txpower": 20,
			"channels": [
				1,
				2,
				3,
				4,
				5,
				6,
				7,
				8,
				9,
				10,
				11,
				12,
				13
			]
		},
		{
			"opclass": 83,
			"bandwidth": 40,
			"txpower": 20,
			"channels": [
				1,
				2,
				3,
				4,
				5,
				6,
				7,
				8,
				9
			]
		},
		{
			"opclass": 84,
			"bandwidth": 40,
			"txpower": 20,
			"channels": [
				5,
				6,
				7,
				8,
				9,
				10,
				11,
				12,
				13
			]
		}
	],
	"txpower_dbm": 31,
	"txpower": 100,
	"dot11h_capable": false,
	"dot11h_enabled": false,
	"regdomain": "DE",
	"beacon_int": 100,
	"dtim_period": 2,
	"preamble": "short",
	"short_retry_limit": 7,
	"long_retry_limit": 4,
	"frag_threshold": -1,
	"rts_threshold": -1,
	"aggr_enabled": false,
	"stats": {
		"tx_bytes": 117108,
		"tx_packets": 1100,
		"tx_error_packets": 5,
		"tx_dropped_packets": 0,
		"rx_bytes": 0,
		"rx_packets": 0,
		"rx_error_packets": 0,
		"rx_dropped_packets": 0,
		"rx_plcp_error_packets": 0,
		"rx_fcs_error_packets": 75038,
		"rx_mac_error_packets": 0,
		"rx_unknown_packets": 0
	},
	"diagnostics": {
		"channel_busy": 0,
		"tx_airtime": 10000,
		"rx_airtime": 0,
		"obss_airtime": 0,
		"cca_time": 1000000,
		"false_cca_count": 16
	}
}
