
config globals 'globals'
	option enabled '1'

config defaults
	option syn_flood '1'
	option input 'ACCEPT'
	option output 'ACCEPT'
	option forward 'REJECT'

config zone 'lan'
	option name 'lan'
	list network 'lan'
	option input 'ACCEPT'
	option output 'ACCEPT'
	option forward 'ACCEPT'

config zone 'wan'
	option name 'wan'
	list network 'wan'
	list network 'wan6'
	option input 'REJECT'
	option output 'ACCEPT'
	option forward 'REJECT'
	option masq '1'
	option mtu_fix '1'

config forwarding 'default_fwd_1'
	option src 'lan'
	option dest 'wan'

config rule 'default_rule_1'
	option name 'Allow-DHCP-Renew'
	option src 'wan'
	option proto 'udp'
	option dest_port '68'
	option target 'ACCEPT'
	option family 'ipv4'

config rule 'default_rule_2'
	option name 'Allow-Ping'
	option src 'wan'
	option proto 'icmp'
	option icmp_type 'echo-request'
	option family 'ipv4'
	option target 'ACCEPT'

config rule 'default_rule_3'
	option name 'Allow-IGMP'
	option src 'wan'
	option proto 'igmp'
	option family 'ipv4'
	option target 'ACCEPT'

config rule 'default_rule_4'
	option name 'Allow-DHCPv6'
	option src 'wan'
	option proto 'udp'
	option src_ip 'fc00::/6'
	option dest_ip 'fc00::/6'
	option dest_port '546'
	option family 'ipv6'
	option target 'ACCEPT'

config rule 'default_rule_5'
	option name 'Allow-MLD'
	option src 'wan'
	option proto 'icmp'
	option src_ip 'fe80::/10'
	list icmp_type '130/0'
	list icmp_type '131/0'
	list icmp_type '132/0'
	list icmp_type '143/0'
	option family 'ipv6'
	option target 'ACCEPT'

config rule 'default_rule_6'
	option name 'Allow-ICMPv6-Input'
	option src 'wan'
	option proto 'icmp'
	list icmp_type 'echo-request'
	list icmp_type 'echo-reply'
	list icmp_type 'destination-unreachable'
	list icmp_type 'packet-too-big'
	list icmp_type 'time-exceeded'
	list icmp_type 'bad-header'
	list icmp_type 'unknown-header-type'
	list icmp_type 'router-solicitation'
	list icmp_type 'neighbour-solicitation'
	list icmp_type 'router-advertisement'
	list icmp_type 'neighbour-advertisement'
	option limit '1000/sec'
	option family 'ipv6'
	option target 'ACCEPT'

config rule 'default_rule_7'
	option name 'Allow-ICMPv6-Forward'
	option src 'wan'
	option dest '*'
	option proto 'icmp'
	list icmp_type 'echo-request'
	list icmp_type 'echo-reply'
	list icmp_type 'destination-unreachable'
	list icmp_type 'packet-too-big'
	list icmp_type 'time-exceeded'
	list icmp_type 'bad-header'
	list icmp_type 'unknown-header-type'
	option limit '1000/sec'
	option family 'ipv6'
	option target 'ACCEPT'

config rule 'default_rule_8'
	option name 'Allow-IPSec-ESP'
	option src 'wan'
	option dest 'lan'
	option proto 'esp'
	option target 'ACCEPT'

config rule 'default_rule_9'
	option name 'Allow-ISAKMP'
	option src 'wan'
	option dest 'lan'
	option dest_port '500'
	option proto 'udp'
	option target 'ACCEPT'

config rule 'default_rule_10'
	option name 'Support-UDP-Traceroute'
	option src 'wan'
	option dest_port '33434:33689'
	option proto 'udp'
	option family 'ipv4'
	option target 'REJECT'
	option enabled 'false'

config dmz 'dmz'
	option enabled '0'
	option exclude_ports '5060 7547'

config include
	option path '/etc/firewall.user'
	option reload '1'

config include 'ddos'
	option path '/etc/firewall.ddos'
	option reload '1'

config include 'parental'
	option path '/etc/firewall.parental'
	option reload '1'

config include 'qos'
	option path '/etc/firewall.qos'
	option reload '1'

config include 'cwmp'
	option path '/etc/firewall.cwmp'
	option reload '1'

config include 'miniupnpd'
	option type 'script'
	option path '/usr/share/miniupnpd/firewall.include'
	option family 'any'
	option reload '1'

config include 'sip'
	option path '/etc/firewall.sip'
	option reload '1'

config include 'dmzhost'
	option path '/etc/firewall.dmz'
	option reload '1'

config redirect 'port_mapping_1'
	option enabled '1'
	option src 'wan'
	option dest 'lan'
	option target 'DNAT'
	option reflection '1'
	option name 'test'
	option proto 'tcp'
	option dest_ip 'wan'
	option src_dport '192.168.3.45'
	option src_dport '50:60'
	option dest_port '44'
