config controller 'controller'
	option enabled '1'	# may be modified by other package start-up scripts (i.e. map-agent)
	option profile '3'
	option registrar '2 5 6'
	option debug '2'
	option bcn_metrics_max_num '10'
	option initial_channel_scan '0'
	option enable_ts '0'
	option primary_vid '1'
	option primary_pcp '0'
	option stale_sta_timeout '30d'
	option de_collect_interval '60'
	list plugin 'zerotouch'

config sta_steering 'sta_steering'
	option enable_sta_steer '1'
	option enable_bsta_steer '1'
	option rcpi_threshold_2g '70'
	option rcpi_threshold_5g '86'
	option rcpi_threshold_6g '86'
	option report_rcpi_threshold_2g '80'
	option report_rcpi_threshold_5g '96'
	option report_rcpi_threshold_6g '96'
	option plugins_enabled '1'
	option plugins_policy 'any'
	list plugins 'rcpi'
	list plugins 'rate'
	list plugins 'bsteer'

config channel_plan 'channel_plan'
	option preclear_dfs '0'
	option acs '0'

###################
# Default AP sections credentials will by updated
# by uci-defaults script 99-mapcntlr
###################

config ap
	option band '2'
	option ssid '$WIFI_FH_2G_SSID'
	option encryption '$WIFI_FH_2G_ENCRYPTION'
	option key '$WIFI_FH_2G_KEY'
	option vid '1'
	option type 'fronthaul'
	option mld_id '1'

config ap
	option band '5'
	option ssid '$WIFI_FH_5G_SSID'
	option encryption '$WIFI_FH_5G_ENCRYPTION'
	option key '$WIFI_FH_5G_KEY'
	option vid '1'
	option type 'fronthaul'
	option mld_id '1'

config ap
	option band '6'
	option ssid '$WIFI_FH_6G_SSID'
	option encryption '$WIFI_FH_6G_ENCRYPTION'
	option key '$WIFI_FH_6G_KEY'
	option vid '1'
	option type 'fronthaul'
	option mld_id '1'

config ap
	option band '2'
	option ssid 'MAP-$BASEMAC_ADDR-BH'
	option encryption 'sae'
	option key '$WIFI_BH_KEY'
	option type 'backhaul'
	option vid '1'
	option mld_id '2'

config ap
	option band '5'
	option ssid 'MAP-$BASEMAC_ADDR-BH'
	option encryption 'sae'
	option key '$WIFI_BH_KEY'
	option type 'backhaul'
	option vid '1'
	option mld_id '2'

config ap
	option band '6'
	option ssid 'MAP-$BASEMAC_ADDR-BH'
	option encryption 'sae'
	option key '$WIFI_BH_KEY'
	option type 'backhaul'
	option vid '1'
	option mld_id '2'

config mld
	option id '1'
	option ssid '$WIFI_FH_ALL_SSID'
	option key '$WIFI_FH_ALL_KEY'
#	option vid '1'
	option type 'fronthaul'

config mld
	option id '2'
	option ssid 'MAP-$BASEMAC_ADDR-BH'
	option key '$WIFI_BH_KEY'
#	option vid '1'
	option type 'backhaul'

# node and radio sections (per node) are auto
# generated per Multi-AP Agent in the network
#
#config node 'node_0a1b2c3d4e50'
#	option agent_id '0a:1b:2c:3d:4e:50'
# following values use default values after onboarding if not explicitly set
#	option backhaul_ul_macaddr '00:00:00:00:00:00'
#	option backhaul_dl_macaddr '00:00:00:00:00:00'
#	option backhaul_type 'none'
#	option report_sta_assocfails '0'
#	option report_sta_assocfails_rate '0'
#	option report_metric_periodic '0'
#	option report_scan '0'
#	list steer_exclude 'e0:d4:e8:79:c4:ee'
#	list steer_exclude_btm 'e0:d4:e8:79:c4:11'
#	option steer_disallow '0'
#	option coordinated_cac '0'
#	option traffic_separation '0'
#	option sta_steer '0'

#config radio 'radio_0a1b2c3d4e53'
#	option agent_id '0a:1b:2c:3d:4e:50'
#	option macaddr '0a:1b:2c:3d:4e:53'
#	option band '2'
# following values use default values after onboarding if not explicitly set
#	option steer_policy '0'
#	option util_threshold '0'
#	option rcpi_threshold '70'
#	option report_rcpi_threshold '80'
#	option report_util_threshold '0'
#	option report_rcpi_hysteresis_margin '0'
#	option include_sta_stats '1'
#	option include_sta_metric '1'

#config radio 'radio_0a1b2c3d4e54'
#	option agent_id '0a:1b:2c:3d:4e:50'
#	option macaddr '0a:1b:2c:3d:4e:54'
#	option band '5'
# following values use default values after onboarding if not explicitly set
#	option steer_policy '0'
#	option util_threshold '0'
#	option rcpi_threshold '86'
#	option report_rcpi_threshold '96'
#	option report_util_threshold '0'
#	option report_rcpi_hysteresis_margin '0'
#	option include_sta_stats '1'
#	option include_sta_metric '1'

#config node 'node_3fb1c2d3e460'
#	option agent_id '3f:b1:c2:d3:e4:60'
# following values use default values after onboarding if not explicitly set
#	option backhaul_ul_macaddr '00:00:00:00:00:00'
#	option backhaul_dl_macaddr '00:00:00:00:00:00'
#	option backhaul_type 'none'
#	option primary_vid '1'
#	option primary_pcp '0'
#	option report_sta_assocfails '0'
#	option report_sta_assocfails_rate '0'
#	option report_metric_periodic '0'
#	option report_scan '0'
#	list steer_exclude 'e0:d4:e8:79:c4:ee'
#	list steer_exclude_btm 'e0:d4:e8:79:c4:11'
#	option steer_disallow '0'
#	option coordinated_cac '0'
#	option traffic_separation '0'
#	option sta_steer '0'

#config radio 'radio_3fb1c2d3e463'
#	option agent_id '3f:b1:c2:d3:e4:60'
#	option macaddr '3f:b1:c2:d3:e4:63'
#	option band '2'
# following values use default values after onboarding if not explicitly set
#	option steer_policy '0'
#	option util_threshold '0'
#	option rcpi_threshold '70'
#	option report_rcpi_threshold '80'
#	option report_util_threshold '0'
#	option report_rcpi_hysteresis_margin '0'
#	option include_sta_stats '1'
#	option include_sta_metric '1'

#config radio 'radio_3fb1c2d3e464'
#	option agent_id '3f:b1:c2:d3:e4:60'
#	option macaddr '3f:b1:c2:d3:e4:64'
#	option band '5'
# following values use default values after onboarding if not explicitly set
#	option steer_policy '0'
#	option util_threshold '0'
#	option rcpi_threshold '86'
#	option report_rcpi_threshold '96'
#	option report_util_threshold '0'
#	option report_rcpi_hysteresis_margin '0'
#	option include_sta_stats '1'
#	option include_sta_metric '1'
