config agent 'agent'
	option enabled '1'
	option debug '0'
	option profile '3'
	option al_bridge 'br-lan'
	option island_prevention '1'
	option eth_onboards_wifi_bhs '1'
	option scan_on_boot_only '0'
	option chan_ch_relay_mcast '0'
	option guest_isolation '1'
	option partial_wifi_reload '0'
	list map_port 'all'
#	option controller_macaddr '0a:1b:2c:3d:4e:50'

config dynamic_backhaul
	option missing_bh_timer '60'
	option missing_bh_reconfig_timer '1800'

config controller_select
	option mode 'auto'
	option probe_int '20'
	option retry_int '9'
	option autostart '1'
	option local '0'

#config radio
#	option device 'phy0'
#	option band '2'
# options below are auto-generated during onboarding
#	option steer_policy '0'
#	option util_threshold '0'
#	option rcpi_threshold '70'
#	option report_rcpi_threshold '80'
#	option rcpi_hysteresis_margin '0'
#	option report_util_threshold '0'
#	option include_sta_stats '1'
#	option include_sta_metric '1'

#config radio
#	option device 'phy1'
#	option band '5'
# options below are auto-generated during onboarding
#	option steer_policy '0'
#	option util_threshold '0'
#	option rcpi_threshold '86'
#	option report_rcpi_threshold '96'
#	option rcpi_hysteresis_margin '0'
#	option report_util_threshold '0'
#	option include_sta_stats '1'
#	option include_sta_metric '1'

#config bsta
#	option enabled '1'
#	option ifname 'wlan0'
#	option band '2'
#	option device 'phy0'
#	option priority '2'
# options below are auto-generated during onboarding
#	option ssid 'MAP-BH-2.4GHz'
#	option encryption 'sae-mixed'
#	option key '0123456789abcdefghijklmnopqrstuvwxyzABCDEFGHIJKLMNOPQRSTUVWZYZ0'
#	option onboarded '1'
#	option bssid '0a:1b:2c:3d:4e:53'
#	option vid '1'

#config bsta
#	option enabled '1'
#	option ifname 'wlan1'
#	option band '5'
#	option device 'phy1'
#	option priority '0'
# options below are auto-generated during onboarding
#	option ssid 'MAP-BH-5GHz'
#	option encryption 'sae-mixed'
#	option key '0123456789abcdefghijklmnopqrstuvwxyzABCDEFGHIJKLMNOPQRSTUVWZYZ0'
#	option onboarded '1'
#	option bssid '0a:1b:2c:3d:4e:54'
#	option vid '1'

# ap sections and policy section are
# auto-generated during onboarding
#
#config ap
#	option enabled '1'
#	option ifname 'wlan0-1'
#	option band '2'
#	option device 'phy0'
#	option type 'fronthaul'
#	option ssid 'IOWRT-2.4GHz'
#	option encryption 'sae-mixed+aes'
#	option key '1234567890'
#	option vid '1'

#config ap
#	option enabled '1'
#	option ifname 'wlan0-2'
#	option band '2'
#	option device 'phy0'
#	option type 'backhaul'
#	option ssid 'MAP-BH-2.4GHz'
#	option encryption 'sae+aes'
#	option key '0123456789abcdefghijklmnopqrstuvwxyzABCDEFGHIJKLMNOPQRSTUVWZYZ0'
#	option disallow_bsta '0'
#	option vid '1'

#config ap
#	option enabled '1'
#	option ifname 'wlan1-1'
#	option band '5'
#	option device 'phy1'
#	option type 'fronthaul'
#	option ssid 'IOWRT-5GHz'
#	option encryption 'sae-mixed+aes'
#	option key '1234567890'
#	option vid '1'

#config ap
#	option enabled '1'
#	option ifname 'wlan1-2'
#	option band '5'
#	option device 'phy1'
#	option type 'backhaul'
#	option ssid 'MAP-BH-5GHz'
#	option encryption 'sae+aes'
#	option key '0123456789abcdefghijklmnopqrstuvwxyzABCDEFGHIJKLMNOPQRSTUVWZYZ0'
#	option disallow_bsta '0'
#	option vid '1'

#config policy
#	option report_interval '0'
#	option pvid '1'
#	option pcp_default '0'
#	option report_scan '0'
#	option report_sta_assocfails '0'
#	option report_sta_assocfails_rate '0'

