--- a/drivers/char/Makefile
+++ b/drivers/char/Makefile
@@ -110,6 +110,10 @@ obj-$(CONFIG_PS3_FLASH)		+= ps3flash.o
 obj-$(CONFIG_JS_RTC)		+= js-rtc.o
 js-rtc-y = rtc.o
 
+obj-$(CONFIG_IFXMIPS_SSC)  += ifxmips_ssc.o
+obj-$(CONFIG_IFXMIPS_EEPROM)   += ifxmips_eeprom.o
+obj-$(CONFIG_IFXMIPS_MEI)  += ifxmips_mei_core.o
+
 # Files generated that shall be removed upon make clean
 clean-files := consolemap_deftbl.c defkeymap.c
 
--- a/drivers/mtd/maps/Makefile
+++ b/drivers/mtd/maps/Makefile
@@ -52,6 +52,7 @@ obj-$(CONFIG_MTD_NETtel)	+= nettel.o
 obj-$(CONFIG_MTD_SCB2_FLASH)	+= scb2_flash.o
 obj-$(CONFIG_MTD_H720X)		+= h720x-flash.o
 obj-$(CONFIG_MTD_SBC8240)	+= sbc8240.o
+obj-$(CONFIG_MTD_IFXMIPS)	+= ifxmips.o
 obj-$(CONFIG_MTD_IXP4XX)	+= ixp4xx.o
 obj-$(CONFIG_MTD_IXP2000)	+= ixp2000.o
 obj-$(CONFIG_MTD_WRSBC8260)	+= wr_sbc82xx_flash.o
--- a/drivers/net/Kconfig
+++ b/drivers/net/Kconfig
@@ -343,6 +343,12 @@ config MACB
 
 source "drivers/net/arm/Kconfig"
 
+config IFXMIPS_MII0
+	tristate "Infineon IFXMips eth0 driver"
+	depends on IFXMIPS
+	help
+	  Support for the MII0 inside the IFXMips SOC
+
 config AX88796
 	tristate "ASIX AX88796 NE2000 clone support"
 	depends on ARM || MIPS || SUPERH
--- a/drivers/serial/Kconfig
+++ b/drivers/serial/Kconfig
@@ -1304,6 +1304,14 @@ config SERIAL_OF_PLATFORM
 	  Currently, only 8250 compatible ports are supported, but
 	  others can easily be added.
 
+config SERIAL_IFXMIPS
+	bool "IFXMips serial driver"
+	depends on IFXMIPS
+	select SERIAL_CORE
+	select SERIAL_CORE_CONSOLE
+	help
+	  Driver for the ifxmipss built in ASC hardware
+
 config SERIAL_QE
 	tristate "Freescale QUICC Engine serial port support"
 	depends on QUICC_ENGINE
--- a/drivers/serial/Makefile
+++ b/drivers/serial/Makefile
@@ -73,3 +73,4 @@ obj-$(CONFIG_SERIAL_OF_PLATFORM) += of_s
 obj-$(CONFIG_SERIAL_KS8695) += serial_ks8695.o
 obj-$(CONFIG_KGDB_SERIAL_CONSOLE) += kgdboc.o
 obj-$(CONFIG_SERIAL_QE) += ucc_uart.o
+obj-$(CONFIG_SERIAL_IFXMIPS) += ifxmips_asc.o
--- a/drivers/watchdog/Makefile
+++ b/drivers/watchdog/Makefile
@@ -106,6 +106,7 @@ obj-$(CONFIG_WDT_RM9K_GPI) += rm9k_wdt.o
 obj-$(CONFIG_SIBYTE_WDOG) += sb_wdog.o
 obj-$(CONFIG_AR7_WDT) += ar7_wdt.o
 obj-$(CONFIG_TXX9_WDT) += txx9wdt.o
+obj-$(CONFIG_IFXMIPS_WDT) += ifxmips_wdt.o
 
 # PARISC Architecture
 
--- a/drivers/net/Makefile
+++ b/drivers/net/Makefile
@@ -262,4 +262,4 @@ obj-$(CONFIG_NETXEN_NIC) += netxen/
 obj-$(CONFIG_NIU) += niu.o
 obj-$(CONFIG_VIRTIO_NET) += virtio_net.o
 obj-$(CONFIG_SFC) += sfc/
-
+obj-$(CONFIG_IFXMIPS_MII0) += ifxmips_mii0.o
--- a/drivers/crypto/Kconfig
+++ b/drivers/crypto/Kconfig
@@ -9,6 +9,9 @@ menuconfig CRYPTO_HW
 	  If you say N, all options in this submenu will be skipped and disabled.
 
 if CRYPTO_HW
+config CRYPTO_DEV_IFXMIPS
+	tristate "Support for IFXMIPS Data Encryption Unit"
+	depends on IFXMIPS
 
 config CRYPTO_DEV_PADLOCK
 	tristate "Support for VIA PadLock ACE"
--- a/drivers/crypto/Makefile
+++ b/drivers/crypto/Makefile
@@ -4,3 +4,4 @@ obj-$(CONFIG_CRYPTO_DEV_GEODE) += geode-
 obj-$(CONFIG_CRYPTO_DEV_HIFN_795X) += hifn_795x.o
 obj-$(CONFIG_CRYPTO_DEV_TALITOS) += talitos.o
 obj-$(CONFIG_CRYPTO_DEV_IXP4XX) += ixp4xx_crypto.o
+obj-$(CONFIG_CRYPTO_DEV_IFXMIPS) += ifxdeu-aes.o ifxdeu-des.o ifxdeu-dma.o ifxdeu-generic.o ifxdeu-md5.o ifxdeu-sha1.o
--- a/drivers/usb/host/Kconfig
+++ b/drivers/usb/host/Kconfig
@@ -321,3 +321,10 @@ config USB_HWA_HCD
 
 	  To compile this driver a module, choose M here: the module
 	  will be called "hwa-hc".
+
+config USB_DWC_HCD
+	tristate "IFXMIPS USB Host Controller Driver"
+	depends on USB && IFXMIPS
+	default y
+	help
+       Danube USB Host Controller
--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -171,6 +171,12 @@ config LEDS_DA903X
 	  This option enables support for on-chip LED drivers found
 	  on Dialog Semiconductor DA9030/DA9034 PMICs.
 
+config LEDS_IFXMIPS
+	tristate "LED Support for IFXMIPS LEDs"
+	depends on LEDS_CLASS && IFXMIPS
+	help
+	  This option enables support for the IFXMIPS LEDs.
+
 comment "LED Triggers"
 
 config LEDS_TRIGGERS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -24,6 +24,7 @@ obj-$(CONFIG_LEDS_FSG)			+= leds-fsg.o
 obj-$(CONFIG_LEDS_PCA955X)		+= leds-pca955x.o
 obj-$(CONFIG_LEDS_DA903X)		+= leds-da903x.o
 obj-$(CONFIG_LEDS_HP_DISK)		+= leds-hp-disk.o
+obj-$(CONFIG_LEDS_IFXMIPS)		+= leds-ifxmips.o
 
 # LED Triggers
 obj-$(CONFIG_LEDS_TRIGGER_TIMER)	+= ledtrig-timer.o
--- a/drivers/watchdog/Kconfig
+++ b/drivers/watchdog/Kconfig
@@ -747,6 +747,12 @@ config TXX9_WDT
 	help
 	  Hardware driver for the built-in watchdog timer on TXx9 MIPS SoCs.
 
+config IFXMIPS_WDT
+	bool "IFXMips watchdog"
+	depends on IFXMIPS
+	help
+	  Hardware driver for the IFXMIPS Watchdog Timer.
+
 # PARISC Architecture
 
 # POWERPC Architecture
