--- linux-2.6.28.9/arch/mips/Kconfig	2009-04-17 10:43:28.000000000 +0200
+++ linux-2.6.28.9.new/arch/mips/Kconfig	2009-04-17 10:43:51.000000000 +0200
@@ -56,7 +56,6 @@
 	select SSB_B43_PCI_BRIDGE if PCI
 	select SSB_PCICORE_HOSTMODE if PCI
 	select GENERIC_GPIO
-	select SYS_HAS_EARLY_PRINTK
 	select CFE
 	help
 	 Support for BCM47XX based boards
