--- a/lib/ipfix_FOKUS_IEs.txt
+++ b/lib/ipfix_FOKUS_IEs.txt
@@ -39,3 +39,41 @@
 313, IPFIX_FT_OWDVARMIN_NSEC,       4, IPFIX_CODING_INT, "owdvarmin_nsec", "FOKUS minimum owd variance in ns"
 314, IPFIX_FT_OWDVARMAX_NSEC,       4, IPFIX_CODING_INT, "owdvarmax_nsec", "FOKUS maximum ow variance in ns"
 
+315, IPFIX_FT_WPROBE_NOISE_AVG, 4, IPFIX_CODING_FLOAT, "global_noise_avg", "wprobe global noice floor - Average"
+316, IPFIX_FT_WPROBE_NOISE_STDEV, 4, IPFIX_CODING_FLOAT, "global_noise_stdev", "wprobe global noice floor - Standard deviation"
+317, IPFIX_FT_WPROBE_NOISE_N, 4, IPFIX_CODING_UINT, "global_noise_n", "wprobe global noice floor - Number of samples"
+318, IPFIX_FT_WPROBE_PHY_BUSY_AVG, 4, IPFIX_CODING_FLOAT, "global_phy_busy_avg", "wprobe global airtime total - Average"
+319, IPFIX_FT_WPROBE_PHY_BUSY_STDEV, 4, IPFIX_CODING_FLOAT, "global_phy_busy_stdev", "wprobe global airtime total - Standard deviation"
+320, IPFIX_FT_WPROBE_PHY_BUSY_N, 4, IPFIX_CODING_UINT, "global_phy_busy_n", "wprobe global airtime total - Number of samples"
+321, IPFIX_FT_WPROBE_PHY_RX_AVG, 4, IPFIX_CODING_FLOAT, "global_phy_rx_avg", "wprobe global airtime total from rx-frame - Average"
+322, IPFIX_FT_WPROBE_PHY_RX_STDEV, 4, IPFIX_CODING_FLOAT, "global_phy_rx_stdev", "wprobe global airtime total from rx-frame - Standard deviation"
+323, IPFIX_FT_WPROBE_PHY_RX_N, 4, IPFIX_CODING_UINT, "global_phy_rx_n", "wprobe global airtime total from rx-frame - Number of samples"
+324, IPFIX_FT_WPROBE_PHY_TX_AVG, 4, IPFIX_CODING_FLOAT, "global_phy_tx_avg", "wprobe global airtime total from tx-frame - Average"
+325, IPFIX_FT_WPROBE_PHY_TX_STDEV, 4, IPFIX_CODING_FLOAT, "global_phy_tx_stdev", "wprobe global airtime total from tx-frame - Standard deviation"
+326, IPFIX_FT_WPROBE_PHY_TX_N, 4, IPFIX_CODING_UINT, "global_phy_tx_n", "wprobe global airtime total from tx-frame - Number of samples"
+327, IPFIX_FT_WPROBE_RSSI_AVG, 4, IPFIX_CODING_FLOAT, "link_rssi_avg", "wprobe link received signal strength indication - Average"
+328, IPFIX_FT_WPROBE_RSSI_STDEV, 4, IPFIX_CODING_FLOAT, "link_rssi_stdev", "wprobe link received signal strength indication - Standard deviation"
+329, IPFIX_FT_WPROBE_RSSI_N, 4, IPFIX_CODING_UINT, "link_rssi_n", "wprobe link received signal strength indication - Number of samples"
+330, IPFIX_FT_WPROBE_SIGNAL_AVG, 4, IPFIX_CODING_FLOAT, "link_signal_avg", "wprobe link signal strength in dB - Average"
+331, IPFIX_FT_WPROBE_SIGNAL_STDEV, 4, IPFIX_CODING_FLOAT, "link_signal_stdev", "wprobe link signal strength in dB - Standard deviation"
+332, IPFIX_FT_WPROBE_SIGNAL_N, 4, IPFIX_CODING_UINT, "link_signal_n", "wprobe link signal strength in dB - Number of samples"
+333, IPFIX_FT_WPROBE_IEEE_RX_RATE_AVG, 4, IPFIX_CODING_FLOAT, "link_ieee_rx_rate_avg", "wprobe link IEEE 802.11 RX data rate - Average"
+334, IPFIX_FT_WPROBE_IEEE_RX_RATE_STDEV, 4, IPFIX_CODING_FLOAT, "link_ieee_rx_rate_stdev", "wprobe link IEEE 802.11 RX data rate - Standard deviation"
+335, IPFIX_FT_WPROBE_IEEE_RX_RATE_N, 4, IPFIX_CODING_UINT, "link_ieee_rx_rate_n", "wprobe link IEEE 802.11 RX data rate - Number of samples"
+336, IPFIX_FT_WPROBE_IEEE_TX_RATE_AVG, 4, IPFIX_CODING_FLOAT, "link_ieee_tx_rate_avg", "wprobe link IEEE 802.11 TX data rate - Average"
+337, IPFIX_FT_WPROBE_IEEE_TX_RATE_STDEV, 4, IPFIX_CODING_FLOAT, "link_ieee_tx_rate_stdev", "wprobe link IEEE 802.11 TX data rate - Standard deviation"
+338, IPFIX_FT_WPROBE_IEEE_TX_RATE_N, 4, IPFIX_CODING_UINT, "link_ieee_tx_rate_n", "wprobe link IEEE 802.11 TX data rate - Number of samples"
+339, IPFIX_FT_WPROBE_RETRANSMIT_200_AVG, 4, IPFIX_CODING_FLOAT, "link_retransmit_200_avg", "wprobe link total retransmissions per packet - <200 bytes - Average"
+340, IPFIX_FT_WPROBE_RETRANSMIT_200_STDEV, 4, IPFIX_CODING_FLOAT, "link_retransmit_200_stdev", "wprobe link total retransmissions per packet - <200 bytes - Standard deviation"
+341, IPFIX_FT_WPROBE_RETRANSMIT_200_N, 4, IPFIX_CODING_UINT, "link_retransmit_200_n", "wprobe link total retransmissions per packet - <200 bytes - Number of samples"
+342, IPFIX_FT_WPROBE_RETRANSMIT_400_AVG, 4, IPFIX_CODING_FLOAT, "link_retransmit_400_avg", "wprobe link total retransmissions per packet - <400 bytes - Average"
+343, IPFIX_FT_WPROBE_RETRANSMIT_400_STDEV, 4, IPFIX_CODING_FLOAT, "link_retransmit_400_stdev", "wprobe link total retransmissions per packet - <400 bytes - Standard deviation"
+344, IPFIX_FT_WPROBE_RETRANSMIT_400_N, 4, IPFIX_CODING_UINT, "link_retransmit_400_n", "wprobe link total retransmissions per packet - <400 bytes - Number of samples"
+345, IPFIX_FT_WPROBE_RETRANSMIT_800_AVG, 4, IPFIX_CODING_FLOAT, "link_retransmit_800_avg", "wprobe link total retransmissions per packet - <800 bytes - Average"
+346, IPFIX_FT_WPROBE_RETRANSMIT_800_STDEV, 4, IPFIX_CODING_FLOAT, "link_retransmit_800_stdev", "wprobe link total retransmissions per packet - <800 bytes - Standard deviation"
+347, IPFIX_FT_WPROBE_RETRANSMIT_800_N, 4, IPFIX_CODING_UINT, "link_retransmit_800_n", "wprobe link total retransmissions per packet - <800 bytes - Number of samples"
+348, IPFIX_FT_WPROBE_RETRANSMIT_1600_AVG, 4, IPFIX_CODING_FLOAT, "link_retransmit_1600_avg", "wprobe link total retransmissions per packet - >800 bytes - Average"
+349, IPFIX_FT_WPROBE_RETRANSMIT_1600_STDEV, 4, IPFIX_CODING_FLOAT, "link_retransmit_1600_stdev", "wprobe link total retransmissions per packet - >800 bytes - Standard deviation"
+350, IPFIX_FT_WPROBE_RETRANSMIT_1600_N, 4, IPFIX_CODING_UINT, "link_retransmit_1600_n", "wprobe link total retransmissions per packet - >800 bytes - Number of samples"
+351, IPFIX_FT_WPROBE_FRAMES, 4, IPFIX_CODING_UINT, "global_frames", "wprobe global number of 802.11 frames seen"
+352, IPFIX_FT_WPROBE_PROBEREQ, 4, IPFIX_CODING_UINT, "global_probereq", "wprobe global number of 802.11 probe requests seen"
