Index: linux-2.6.25.16/arch/cris/arch-v10/drivers/ds1302.c
===================================================================
--- linux-2.6.25.16.o/arch/cris/arch-v10/drivers/ds1302.c	2008-10-26 15:54:02.000000000 +0100
+++ linux-2.6.25.16/arch/cris/arch-v10/drivers/ds1302.c	2008-10-26 15:59:37.000000000 +0100
@@ -21,6 +21,7 @@
 #include <linux/delay.h>
 #include <linux/bcd.h>
 #include <linux/capability.h>
+#include <linux/device.h>
 
 #include <asm/uaccess.h>
 #include <asm/system.h>
@@ -489,6 +490,10 @@
 	return 0;
 }
 
+#ifdef CONFIG_SYSFS
+static struct class *rtc_class;
+#endif
+
 static int __init ds1302_register(void)
 {
 	ds1302_init();
@@ -497,6 +502,12 @@
 		       ds1302_name, RTC_MAJOR_NR);
 		return -1;
 	}
+	#ifdef CONFIG_SYSFS
+	rtc_class = class_create(THIS_MODULE, "rtc");
+	class_device_create(rtc_class, NULL, MKDEV(RTC_MAJOR_NR, 0),
+		NULL, "rtc");
+	#endif
+
         return 0;
 
 }
Index: linux-2.6.25.16/arch/cris/arch-v10/drivers/gpio.c
===================================================================
--- linux-2.6.25.16.o/arch/cris/arch-v10/drivers/gpio.c	2008-10-26 15:56:28.000000000 +0100
+++ linux-2.6.25.16/arch/cris/arch-v10/drivers/gpio.c	2008-10-26 15:57:41.000000000 +0100
@@ -20,6 +20,7 @@
 #include <linux/poll.h>
 #include <linux/init.h>
 #include <linux/interrupt.h>
+#include <linux/device.h>
 
 #include <asm/etraxgpio.h>
 #include <asm/arch/svinto.h>
@@ -768,6 +769,10 @@
 
 /* main driver initialization routine, called from mem.c */
 
+#ifdef CONFIG_SYSFS
+static struct class *gpio_class;
+#endif
+
 static int __init gpio_init(void)
 {
 	int res;
@@ -781,6 +786,13 @@
 		return res;
 	}
 
+#ifdef CONFIG_SYSFS
+	gpio_class = class_create(THIS_MODULE, "gpio");
+	class_device_create(gpio_class, NULL, MKDEV(GPIO_MAJOR, 0), NULL, "gpioa");
+	class_device_create(gpio_class, NULL, MKDEV(GPIO_MAJOR, 1), NULL, "gpiob");
+	class_device_create(gpio_class, NULL, MKDEV(GPIO_MAJOR, 2), NULL, "leds");
+	class_device_create(gpio_class, NULL, MKDEV(GPIO_MAJOR, 3), NULL, "gpiog");
+#endif
 	/* Clear all leds */
 #if defined (CONFIG_ETRAX_CSP0_LEDS) ||  defined (CONFIG_ETRAX_PA_LEDS) || defined (CONFIG_ETRAX_PB_LEDS)
 	CRIS_LED_NETWORK_SET(0);

