Index: linux-2.4.35.4/drivers/mtd/devices/Config.in
===================================================================
--- linux-2.4.35.4.orig/drivers/mtd/devices/Config.in
+++ linux-2.4.35.4/drivers/mtd/devices/Config.in
@@ -5,6 +5,7 @@
 mainmenu_option next_comment
 
 comment 'Self-contained MTD device drivers'
+bool '  Broadcom Chipcommon Serial Flash support' CONFIG_MTD_SFLASH
 dep_tristate '  Ramix PMC551 PCI Mezzanine RAM card support' CONFIG_MTD_PMC551 $CONFIG_MTD $CONFIG_PCI
 if [ "$CONFIG_MTD_PMC551" = "y" -o  "$CONFIG_MTD_PMC551" = "m" ]; then
    bool '    PMC551 256M DRAM Bugfix' CONFIG_MTD_PMC551_BUGFIX
Index: linux-2.4.35.4/drivers/mtd/devices/Makefile
===================================================================
--- linux-2.4.35.4.orig/drivers/mtd/devices/Makefile
+++ linux-2.4.35.4/drivers/mtd/devices/Makefile
@@ -3,6 +3,8 @@
 #
 # $Id: Makefile,v 1.4 2001/06/26 21:10:05 spse Exp $
 
+EXTRA_CFLAGS := -I$(TOPDIR)/arch/mips/bcm947xx/include
+
 O_TARGET	:= devlink.o
 
 #                       *** BIG UGLY NOTE ***
@@ -12,6 +14,7 @@ O_TARGET	:= devlink.o
 # here where previously there was none.  We now have to ensure that
 # doc200[01].o are linked before docprobe.o
 
+obj-$(CONFIG_MTD_SFLASH)	+= sflash.o
 obj-$(CONFIG_MTD_DOC1000)	+= doc1000.o
 obj-$(CONFIG_MTD_DOC2000)	+= doc2000.o
 obj-$(CONFIG_MTD_DOC2001)	+= doc2001.o
Index: linux-2.4.35.4/drivers/mtd/maps/Config.in
===================================================================
--- linux-2.4.35.4.orig/drivers/mtd/maps/Config.in
+++ linux-2.4.35.4/drivers/mtd/maps/Config.in
@@ -48,6 +48,7 @@ if [ "$CONFIG_PPC" = "y" ]; then
 fi
 
 if [ "$CONFIG_MIPS" = "y" ]; then
+   dep_tristate '  CFI Flash device mapped on Broadcom BCM947XX boards' CONFIG_MTD_BCM947XX $CONFIG_MTD_CFI
    dep_tristate '  Pb1000 MTD support' CONFIG_MTD_PB1000 $CONFIG_MIPS_PB1000
    dep_tristate '  Pb1500 MTD support' CONFIG_MTD_PB1500 $CONFIG_MIPS_PB1500
    dep_tristate '  Pb1100 MTD support' CONFIG_MTD_PB1100 $CONFIG_MIPS_PB1100
Index: linux-2.4.35.4/drivers/mtd/maps/Makefile
===================================================================
--- linux-2.4.35.4.orig/drivers/mtd/maps/Makefile
+++ linux-2.4.35.4/drivers/mtd/maps/Makefile
@@ -3,6 +3,8 @@
 #
 # $Id: Makefile,v 1.37 2003/01/24 14:26:38 dwmw2 Exp $
 
+EXTRA_CFLAGS := -I$(TOPDIR)/arch/mips/bcm947xx/include
+
 BELOW25		:= $(shell echo $(PATCHLEVEL) | sed s/[1234]/y/)
 
 ifeq ($(BELOW25),y)
@@ -10,6 +12,7 @@ O_TARGET	:= mapslink.o
 endif
 
 # Chip mappings
+obj-$(CONFIG_MTD_BCM947XX)	+= bcm947xx-flash.o
 obj-$(CONFIG_MTD_CDB89712)	+= cdb89712.o
 obj-$(CONFIG_MTD_ARM_INTEGRATOR)+= integrator-flash.o
 obj-$(CONFIG_MTD_CFI_FLAGADM)	+= cfi_flagadm.o
