Index: linux-2.4.35.4/include/linux/skbuff.h
===================================================================
--- linux-2.4.35.4.orig/include/linux/skbuff.h
+++ linux-2.4.35.4/include/linux/skbuff.h
@@ -912,6 +912,49 @@ static inline void skb_reserve(struct sk
 	skb->tail+=len;
 }
 
+/*
+ * CPUs often take a performance hit when accessing unaligned memory
+ * locations. The actual performance hit varies, it can be small if the
+ * hardware handles it or large if we have to take an exception and fix it
+ * in software.
+ *
+ * Since an ethernet header is 14 bytes network drivers often end up with
+ * the IP header at an unaligned offset. The IP header can be aligned by
+ * shifting the start of the packet by 2 bytes. Drivers should do this
+ * with:
+ *
+ * skb_reserve(NET_IP_ALIGN);
+ *
+ * The downside to this alignment of the IP header is that the DMA is now
+ * unaligned. On some architectures the cost of an unaligned DMA is high
+ * and this cost outweighs the gains made by aligning the IP header.
+ * 
+ * Since this trade off varies between architectures, we allow NET_IP_ALIGN
+ * to be overridden.
+ */
+#ifndef NET_IP_ALIGN
+#define NET_IP_ALIGN    2
+#endif
+
+/*
+ * The networking layer reserves some headroom in skb data (via
+ * dev_alloc_skb). This is used to avoid having to reallocate skb data when
+ * the header has to grow. In the default case, if the header has to grow
+ * 16 bytes or less we avoid the reallocation.
+ *
+ * Unfortunately this headroom changes the DMA alignment of the resulting
+ * network packet. As for NET_IP_ALIGN, this unaligned DMA is expensive
+ * on some architectures. An architecture can override this value,
+ * perhaps setting it to a cacheline in size (since that will maintain
+ * cacheline alignment of the DMA). It must be a power of 2.
+ *
+ * Various parts of the networking layer expect at least 16 bytes of
+ * headroom, you should not reduce this.
+ */
+#ifndef NET_SKB_PAD
+#define NET_SKB_PAD     16
+#endif
+ 
 extern int ___pskb_trim(struct sk_buff *skb, unsigned int len, int realloc);
 
 static inline void __skb_trim(struct sk_buff *skb, unsigned int len)
Index: linux-2.4.35.4/drivers/net/tun.c
===================================================================
--- linux-2.4.35.4.orig/drivers/net/tun.c
+++ linux-2.4.35.4/drivers/net/tun.c
@@ -185,22 +185,31 @@ static __inline__ ssize_t tun_get_user(s
 {
 	struct tun_pi pi = { 0, __constant_htons(ETH_P_IP) };
 	struct sk_buff *skb;
-	size_t len = count;
+	size_t len = count, align = 0;
 
 	if (!(tun->flags & TUN_NO_PI)) {
 		if ((len -= sizeof(pi)) > count)
 			return -EINVAL;
 
-		memcpy_fromiovec((void *)&pi, iv, sizeof(pi));
+ 		if(memcpy_fromiovec((void *)&pi, iv, sizeof(pi)))
+ 			return -EFAULT;
 	}
- 
-	if (!(skb = alloc_skb(len + 2, GFP_KERNEL))) {
+
+	if ((tun->flags & TUN_TYPE_MASK) == TUN_TAP_DEV)
+		align = NET_IP_ALIGN;
+  
+	if (!(skb = alloc_skb(len + align, GFP_KERNEL))) {
 		tun->stats.rx_dropped++;
 		return -ENOMEM;
 	}
 
-	skb_reserve(skb, 2);
-	memcpy_fromiovec(skb_put(skb, len), iv, len);
+	if (align)
+		skb_reserve(skb, align);
+ 	if (memcpy_fromiovec(skb_put(skb, len), iv, len)) {
+		tun->stats.rx_dropped++;
+		kfree_skb(skb);
+ 		return -EFAULT;
+	}
 
 	skb->dev = &tun->dev;
 	switch (tun->flags & TUN_TYPE_MASK) {
@@ -271,7 +280,8 @@ static __inline__ ssize_t tun_put_user(s
 			pi.flags |= TUN_PKT_STRIP;
 		}
  
-		memcpy_toiovec(iv, (void *) &pi, sizeof(pi));
+		if(memcpy_toiovec(iv, (void *) &pi, sizeof(pi)))
+			return -EFAULT;
 		total += sizeof(pi);
 	}       
 
