--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -150,4 +150,11 @@ config LEDS_TRIGGER_DEFAULT_ON
 	  This allows LEDs to be initialised in the ON state.
 	  If unsure, say Y.
 
+config LEDS_TRIGGER_NETDEV
+	tristate "LED Netdev Trigger"
+	depends on LEDS_TRIGGERS
+	help
+		This allows LEDs to be controlled by network device activity.
+		If unsure, say Y.
+
 endif # NEW_LEDS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -25,3 +25,4 @@ obj-$(CONFIG_LEDS_TRIGGER_IDE_DISK)	+= l
 obj-$(CONFIG_LEDS_TRIGGER_HEARTBEAT)	+= ledtrig-heartbeat.o
 obj-$(CONFIG_LEDS_TRIGGER_MORSE)	+= ledtrig-morse.o
 obj-$(CONFIG_LEDS_TRIGGER_DEFAULT_ON)	+= ledtrig-default-on.o
+obj-$(CONFIG_LEDS_TRIGGER_NETDEV)		+= ledtrig-netdev.o
