Index: linux-2.4.35.4/include/linux/netfilter_ipv4/ip_nat.h
===================================================================
--- linux-2.4.35.4.orig/include/linux/netfilter_ipv4/ip_nat.h
+++ linux-2.4.35.4/include/linux/netfilter_ipv4/ip_nat.h
@@ -121,5 +121,13 @@ extern int ip_nat_used_tuple(const struc
 extern u_int16_t ip_nat_cheat_check(u_int32_t oldvalinv,
 				    u_int32_t newval,
 				    u_int16_t oldcheck);
+
+/* Call input routing for SNAT-ed traffic */
+extern unsigned int ip_nat_route_input(unsigned int hooknum,
+				       struct sk_buff **pskb,
+				       const struct net_device *in,
+				       const struct net_device *out,
+				       int (*okfn)(struct sk_buff *));
+
 #endif /*__KERNEL__*/
 #endif
Index: linux-2.4.35.4/include/linux/rtnetlink.h
===================================================================
--- linux-2.4.35.4.orig/include/linux/rtnetlink.h
+++ linux-2.4.35.4/include/linux/rtnetlink.h
@@ -234,6 +234,8 @@ struct rtnexthop
 #define RTNH_F_DEAD		1	/* Nexthop is dead (used by multipath)	*/
 #define RTNH_F_PERVASIVE	2	/* Do recursive gateway lookup	*/
 #define RTNH_F_ONLINK		4	/* Gateway is forced on link	*/
+#define RTNH_F_SUSPECT		8	/* We don't know the real state	*/
+#define RTNH_F_BADSTATE		(RTNH_F_DEAD | RTNH_F_SUSPECT)
 
 /* Macros to handle hexthops */
 
Index: linux-2.4.35.4/include/net/ip_fib.h
===================================================================
--- linux-2.4.35.4.orig/include/net/ip_fib.h
+++ linux-2.4.35.4/include/net/ip_fib.h
@@ -162,7 +162,8 @@ static inline int fib_lookup(const struc
 
 static inline void fib_select_default(const struct rt_key *key, struct fib_result *res)
 {
-	if (FIB_RES_GW(*res) && FIB_RES_NH(*res).nh_scope == RT_SCOPE_LINK)
+	if ((FIB_RES_GW(*res) && FIB_RES_NH(*res).nh_scope == RT_SCOPE_LINK) ||
+	    FIB_RES_NH(*res).nh_scope == RT_SCOPE_HOST)
 		main_table->tb_select_default(main_table, key, res);
 }
 
@@ -174,6 +175,7 @@ extern struct fib_table * fib_tables[RT_
 extern int fib_lookup(const struct rt_key *key, struct fib_result *res);
 extern struct fib_table *__fib_new_table(int id);
 extern void fib_rule_put(struct fib_rule *r);
+extern int fib_result_table(struct fib_result *res);
 
 static inline struct fib_table *fib_get_table(int id)
 {
@@ -275,5 +277,6 @@ static inline void fib_res_put(struct fi
 #endif
 }
 
+extern rwlock_t fib_nhflags_lock;
 
 #endif  /* _NET_FIB_H */
Index: linux-2.4.35.4/include/net/route.h
===================================================================
--- linux-2.4.35.4.orig/include/net/route.h
+++ linux-2.4.35.4/include/net/route.h
@@ -49,6 +49,8 @@ struct rt_key
 {
 	__u32			dst;
 	__u32			src;
+	__u32			lsrc;
+	__u32			gw;
 	int			iif;
 	int			oif;
 #ifdef CONFIG_IP_ROUTE_FWMARK
@@ -128,6 +130,7 @@ extern void		ip_rt_advice(struct rtable 
 extern void		rt_cache_flush(int how);
 extern int		ip_route_output_key(struct rtable **, const struct rt_key *key);
 extern int		ip_route_input(struct sk_buff*, u32 dst, u32 src, u8 tos, struct net_device *devin);
+extern int		ip_route_input_lookup(struct sk_buff*, u32 dst, u32 src, u8 tos, struct net_device *devin, u32 lsrc);
 extern unsigned short	ip_rt_frag_needed(struct iphdr *iph, unsigned short new_mtu);
 extern void		ip_rt_update_pmtu(struct dst_entry *dst, unsigned mtu);
 extern void		ip_rt_send_redirect(struct sk_buff *skb);
@@ -148,6 +151,15 @@ static inline int ip_route_output(struct
 }
 
 
+static inline int
+ip_route_output_lookup(struct rtable **rp,
+		       u32 daddr, u32 saddr, u32 tos, int oif, u32 gw)
+{
+	struct rt_key key = { dst:daddr, src:saddr, gw:gw, oif:oif, tos:tos };
+
+	return ip_route_output_key(rp, &key);
+}
+
 static inline void ip_rt_put(struct rtable * rt)
 {
 	if (rt)
Index: linux-2.4.35.4/net/ipv4/fib_frontend.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/fib_frontend.c
+++ linux-2.4.35.4/net/ipv4/fib_frontend.c
@@ -54,6 +54,8 @@
 struct fib_table *local_table;
 struct fib_table *main_table;
 
+#define FIB_RES_TABLE(r) (RT_TABLE_MAIN)
+
 #else
 
 #define RT_TABLE_MIN 1
@@ -71,6 +73,7 @@ struct fib_table *__fib_new_table(int id
 	return tb;
 }
 
+#define FIB_RES_TABLE(r) (fib_result_table(r))
 
 #endif /* CONFIG_IP_MULTIPLE_TABLES */
 
@@ -209,6 +212,9 @@ int fib_validate_source(u32 src, u32 dst
 	struct in_device *in_dev;
 	struct rt_key key;
 	struct fib_result res;
+	int table;
+	unsigned char prefixlen;
+	unsigned char scope;
 	int no_addr, rpf;
 	int ret;
 
@@ -216,6 +222,7 @@ int fib_validate_source(u32 src, u32 dst
 	key.src = dst;
 	key.tos = tos;
 	key.oif = 0;
+	key.gw	= 0;
 	key.iif = oif;
 	key.scope = RT_SCOPE_UNIVERSE;
 
@@ -237,31 +244,35 @@ int fib_validate_source(u32 src, u32 dst
 		goto e_inval_res;
 	*spec_dst = FIB_RES_PREFSRC(res);
 	fib_combine_itag(itag, &res);
-#ifdef CONFIG_IP_ROUTE_MULTIPATH
-	if (FIB_RES_DEV(res) == dev || res.fi->fib_nhs > 1)
-#else
 	if (FIB_RES_DEV(res) == dev)
-#endif
 	{
 		ret = FIB_RES_NH(res).nh_scope >= RT_SCOPE_HOST;
 		fib_res_put(&res);
 		return ret;
 	}
+	table = FIB_RES_TABLE(&res);
+	prefixlen = res.prefixlen;
+	scope = res.scope;
 	fib_res_put(&res);
 	if (no_addr)
 		goto last_resort;
-	if (rpf)
-		goto e_inval;
 	key.oif = dev->ifindex;
 
 	ret = 0;
 	if (fib_lookup(&key, &res) == 0) {
-		if (res.type == RTN_UNICAST) {
+		if (res.type == RTN_UNICAST &&
+		    ((table == FIB_RES_TABLE(&res) &&
+		      res.prefixlen >= prefixlen && res.scope >= scope) ||
+		     !rpf)) {
 			*spec_dst = FIB_RES_PREFSRC(res);
 			ret = FIB_RES_NH(res).nh_scope >= RT_SCOPE_HOST;
+			fib_res_put(&res);
+			return ret;
 		}
 		fib_res_put(&res);
 	}
+	if (rpf)
+		goto e_inval;
 	return ret;
 
 last_resort:
@@ -579,9 +590,7 @@ static int fib_inetaddr_event(struct not
 	switch (event) {
 	case NETDEV_UP:
 		fib_add_ifaddr(ifa);
-#ifdef CONFIG_IP_ROUTE_MULTIPATH
 		fib_sync_up(ifa->ifa_dev->dev);
-#endif
 		rt_cache_flush(-1);
 		break;
 	case NETDEV_DOWN:
@@ -617,9 +626,7 @@ static int fib_netdev_event(struct notif
 		for_ifa(in_dev) {
 			fib_add_ifaddr(ifa);
 		} endfor_ifa(in_dev);
-#ifdef CONFIG_IP_ROUTE_MULTIPATH
 		fib_sync_up(dev);
-#endif
 		rt_cache_flush(-1);
 		break;
 	case NETDEV_DOWN:
Index: linux-2.4.35.4/net/ipv4/fib_hash.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/fib_hash.c
+++ linux-2.4.35.4/net/ipv4/fib_hash.c
@@ -71,6 +71,7 @@ struct fib_node
 	struct fib_info		*fn_info;
 #define FIB_INFO(f)	((f)->fn_info)
 	fn_key_t		fn_key;
+	int			fn_last_dflt;
 	u8			fn_tos;
 	u8			fn_type;
 	u8			fn_scope;
@@ -336,72 +337,123 @@ out:
 	return err;
 }
 
-static int fn_hash_last_dflt=-1;
-
-static int fib_detect_death(struct fib_info *fi, int order,
-			    struct fib_info **last_resort, int *last_idx)
+static int fib_detect_death(struct fib_info *fi, int order, int last_dflt,
+			    struct fib_info **last_resort, int *last_idx,
+			    int *last_nhsel, const struct rt_key *key)
 {
 	struct neighbour *n;
-	int state = NUD_NONE;
+	int nhsel;
+	int state;
+	struct fib_nh * nh;
+	u32 dst;
+	int flag, dead = 1;
+
+	/* change_nexthops(fi) { */
+	for (nhsel = 0, nh = fi->fib_nh; nhsel < fi->fib_nhs; nh++, nhsel++) {
+		if (key->oif && key->oif != nh->nh_oif)
+			continue;
+		if (key->gw && key->gw != nh->nh_gw && nh->nh_gw &&
+		    nh->nh_scope == RT_SCOPE_LINK)
+			continue;
+		if (nh->nh_flags & RTNH_F_DEAD)
+			continue;
 
-	n = neigh_lookup(&arp_tbl, &fi->fib_nh[0].nh_gw, fi->fib_dev);
-	if (n) {
-		state = n->nud_state;
-		neigh_release(n);
+		flag = 0;
+		if (nh->nh_dev->flags & IFF_NOARP) {
+			dead = 0;
+			goto setfl;
+		}
+
+		dst = nh->nh_gw;
+		if (!nh->nh_gw || nh->nh_scope != RT_SCOPE_LINK)
+			dst = key->dst;
+
+		state = NUD_NONE;
+		n = neigh_lookup(&arp_tbl, &dst, nh->nh_dev);
+		if (n) {
+			state = n->nud_state;
+			neigh_release(n);
+		}
+		if (state==NUD_REACHABLE ||
+			((state&NUD_VALID) && order != last_dflt)) {
+			dead = 0;
+			goto setfl;
+		}
+		if (!(state&NUD_VALID))
+			flag = 1;
+		if (!dead)
+			goto setfl;
+		if ((state&NUD_VALID) ||
+		    (*last_idx<0 && order >= last_dflt)) {
+			*last_resort = fi;
+			*last_idx = order;
+			*last_nhsel = nhsel;
+		}
+
+		setfl:
+
+		read_lock_bh(&fib_nhflags_lock);
+		if (flag)
+			nh->nh_flags |= RTNH_F_SUSPECT;
+		else
+			nh->nh_flags &= ~RTNH_F_SUSPECT;
+		read_unlock_bh(&fib_nhflags_lock);
 	}
-	if (state==NUD_REACHABLE)
-		return 0;
-	if ((state&NUD_VALID) && order != fn_hash_last_dflt)
-		return 0;
-	if ((state&NUD_VALID) ||
-	    (*last_idx<0 && order > fn_hash_last_dflt)) {
-		*last_resort = fi;
-		*last_idx = order;
-	}
-	return 1;
+	/* } endfor_nexthops(fi) */
+
+	return dead;
 }
 
 static void
 fn_hash_select_default(struct fib_table *tb, const struct rt_key *key, struct fib_result *res)
 {
-	int order, last_idx;
-	struct fib_node *f;
+	int order, last_idx, last_dflt, last_nhsel;
+	struct fib_node *f, *first_node;
 	struct fib_info *fi = NULL;
 	struct fib_info *last_resort;
 	struct fn_hash *t = (struct fn_hash*)tb->tb_data;
-	struct fn_zone *fz = t->fn_zones[0];
+	struct fn_zone *fz = t->fn_zones[res->prefixlen];
+	fn_key_t k;
 
 	if (fz == NULL)
 		return;
 
+	k = fz_key(key->dst, fz);
+	last_dflt = -2;
+	first_node = NULL;
 	last_idx = -1;
 	last_resort = NULL;
+	last_nhsel = 0;
 	order = -1;
 
 	read_lock(&fib_hash_lock);
-	for (f = fz->fz_hash[0]; f; f = f->fn_next) {
+	for (f = fz_chain(k, fz); f; f = f->fn_next) {
 		struct fib_info *next_fi = FIB_INFO(f);
 
-		if ((f->fn_state&FN_S_ZOMBIE) ||
+		if (!fn_key_eq(k, f->fn_key) ||
+		    (f->fn_state&FN_S_ZOMBIE) ||
 		    f->fn_scope != res->scope ||
+#ifdef CONFIG_IP_ROUTE_TOS
+		    (f->fn_tos && f->fn_tos != key->tos) ||
+#endif
 		    f->fn_type != RTN_UNICAST)
 			continue;
 
 		if (next_fi->fib_priority > res->fi->fib_priority)
 			break;
-		if (!next_fi->fib_nh[0].nh_gw || next_fi->fib_nh[0].nh_scope != RT_SCOPE_LINK)
-			continue;
 		f->fn_state |= FN_S_ACCESSED;
 
-		if (fi == NULL) {
-			if (next_fi != res->fi)
-				break;
-		} else if (!fib_detect_death(fi, order, &last_resort, &last_idx)) {
+		if (!first_node) {
+			last_dflt = f->fn_last_dflt;
+			first_node = f;
+		}
+		if (fi && !fib_detect_death(fi, order, last_dflt,
+				&last_resort, &last_idx, &last_nhsel, key)) {
 			if (res->fi)
 				fib_info_put(res->fi);
 			res->fi = fi;
 			atomic_inc(&fi->fib_clntref);
-			fn_hash_last_dflt = order;
+			first_node->fn_last_dflt = order;
 			goto out;
 		}
 		fi = next_fi;
@@ -409,16 +461,25 @@ fn_hash_select_default(struct fib_table 
 	}
 
 	if (order<=0 || fi==NULL) {
-		fn_hash_last_dflt = -1;
+		if (fi && fi->fib_nhs > 1 &&
+		    fib_detect_death(fi, order, last_dflt,
+			&last_resort, &last_idx, &last_nhsel, key) &&
+		    last_resort == fi) {
+			read_lock_bh(&fib_nhflags_lock);
+			fi->fib_nh[last_nhsel].nh_flags &= ~RTNH_F_SUSPECT;
+			read_unlock_bh(&fib_nhflags_lock);
+		}
+		if (first_node) first_node->fn_last_dflt = -1;
 		goto out;
 	}
 
-	if (!fib_detect_death(fi, order, &last_resort, &last_idx)) {
+	if (!fib_detect_death(fi, order, last_dflt, &last_resort, &last_idx,
+			      &last_nhsel, key)) {
 		if (res->fi)
 			fib_info_put(res->fi);
 		res->fi = fi;
 		atomic_inc(&fi->fib_clntref);
-		fn_hash_last_dflt = order;
+		first_node->fn_last_dflt = order;
 		goto out;
 	}
 
@@ -428,8 +489,11 @@ fn_hash_select_default(struct fib_table 
 		res->fi = last_resort;
 		if (last_resort)
 			atomic_inc(&last_resort->fib_clntref);
+		read_lock_bh(&fib_nhflags_lock);
+		last_resort->fib_nh[last_nhsel].nh_flags &= ~RTNH_F_SUSPECT;
+		read_unlock_bh(&fib_nhflags_lock);
+		first_node->fn_last_dflt = last_idx;
 	}
-	fn_hash_last_dflt = last_idx;
 out:
 	read_unlock(&fib_hash_lock);
 }
@@ -589,6 +653,7 @@ replace:
 
 	memset(new_f, 0, sizeof(struct fib_node));
 
+	new_f->fn_last_dflt = -1;
 	new_f->fn_key = key;
 #ifdef CONFIG_IP_ROUTE_TOS
 	new_f->fn_tos = tos;
Index: linux-2.4.35.4/net/ipv4/fib_rules.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/fib_rules.c
+++ linux-2.4.35.4/net/ipv4/fib_rules.c
@@ -307,6 +307,11 @@ static void fib_rules_attach(struct net_
 	}
 }
 
+int fib_result_table(struct fib_result *res)
+{
+	return res->r->r_table;
+}
+
 int fib_lookup(const struct rt_key *key, struct fib_result *res)
 {
 	int err;
@@ -371,8 +376,10 @@ FRprintk("FAILURE\n");
 
 void fib_select_default(const struct rt_key *key, struct fib_result *res)
 {
-	if (res->r && res->r->r_action == RTN_UNICAST &&
-	    FIB_RES_GW(*res) && FIB_RES_NH(*res).nh_scope == RT_SCOPE_LINK) {
+	if (res->r &&
+	    (res->r->r_action == RTN_UNICAST || res->r->r_action == RTN_NAT) &&
+	    ((FIB_RES_GW(*res) && FIB_RES_NH(*res).nh_scope == RT_SCOPE_LINK) ||
+	     FIB_RES_NH(*res).nh_scope == RT_SCOPE_HOST)) {
 		struct fib_table *tb;
 		if ((tb = fib_get_table(res->r->r_table)) != NULL)
 			tb->tb_select_default(tb, key, res);
Index: linux-2.4.35.4/net/ipv4/fib_semantics.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/fib_semantics.c
+++ linux-2.4.35.4/net/ipv4/fib_semantics.c
@@ -48,6 +48,7 @@
 static struct fib_info 	*fib_info_list;
 static rwlock_t fib_info_lock = RW_LOCK_UNLOCKED;
 int fib_info_cnt;
+rwlock_t fib_nhflags_lock = RW_LOCK_UNLOCKED;
 
 #define for_fib_info() { struct fib_info *fi; \
 	for (fi = fib_info_list; fi; fi = fi->fib_next)
@@ -150,7 +151,7 @@ static __inline__ int nh_comp(const stru
 #ifdef CONFIG_NET_CLS_ROUTE
 		    nh->nh_tclassid != onh->nh_tclassid ||
 #endif
-		    ((nh->nh_flags^onh->nh_flags)&~RTNH_F_DEAD))
+		    ((nh->nh_flags^onh->nh_flags)&~RTNH_F_BADSTATE))
 			return -1;
 		onh++;
 	} endfor_nexthops(fi);
@@ -166,7 +167,7 @@ static __inline__ struct fib_info * fib_
 		    nfi->fib_prefsrc == fi->fib_prefsrc &&
 		    nfi->fib_priority == fi->fib_priority &&
 		    memcmp(nfi->fib_metrics, fi->fib_metrics, sizeof(fi->fib_metrics)) == 0 &&
-		    ((nfi->fib_flags^fi->fib_flags)&~RTNH_F_DEAD) == 0 &&
+		    ((nfi->fib_flags^fi->fib_flags)&~RTNH_F_BADSTATE) == 0 &&
 		    (nfi->fib_nhs == 0 || nh_comp(fi, nfi) == 0))
 			return fi;
 	} endfor_fib_info();
@@ -365,8 +366,11 @@ static int fib_check_nh(const struct rtm
 				return -EINVAL;
 			if ((dev = __dev_get_by_index(nh->nh_oif)) == NULL)
 				return -ENODEV;
-			if (!(dev->flags&IFF_UP))
-				return -ENETDOWN;
+			if (!(dev->flags&IFF_UP)) {
+				if (fi->fib_protocol != RTPROT_STATIC)
+					return -ENETDOWN;
+				nh->nh_flags |= RTNH_F_DEAD;
+			}
 			nh->nh_dev = dev;
 			dev_hold(dev);
 			nh->nh_scope = RT_SCOPE_LINK;
@@ -380,23 +384,48 @@ static int fib_check_nh(const struct rtm
 		/* It is not necessary, but requires a bit of thinking */
 		if (key.scope < RT_SCOPE_LINK)
 			key.scope = RT_SCOPE_LINK;
-		if ((err = fib_lookup(&key, &res)) != 0)
-			return err;
-		err = -EINVAL;
-		if (res.type != RTN_UNICAST && res.type != RTN_LOCAL)
-			goto out;
-		nh->nh_scope = res.scope;
-		nh->nh_oif = FIB_RES_OIF(res);
-		if ((nh->nh_dev = FIB_RES_DEV(res)) == NULL)
-			goto out;
-		dev_hold(nh->nh_dev);
-		err = -ENETDOWN;
-		if (!(nh->nh_dev->flags & IFF_UP))
-			goto out;
-		err = 0;
+
+		err = fib_lookup(&key, &res);
+		if (err) {
+			struct in_device *in_dev;
+
+			if (err != -ENETUNREACH ||
+			    fi->fib_protocol != RTPROT_STATIC)
+				return err;
+
+			in_dev = inetdev_by_index(nh->nh_oif);
+			if (in_dev == NULL ||
+			    in_dev->dev->flags & IFF_UP) {
+				if (in_dev)
+					in_dev_put(in_dev);
+				return err;
+			}
+			nh->nh_flags |= RTNH_F_DEAD;
+			nh->nh_scope = RT_SCOPE_LINK;
+			nh->nh_dev = in_dev->dev;
+			dev_hold(nh->nh_dev);
+			in_dev_put(in_dev);
+		} else {
+			err = -EINVAL;
+			if (res.type != RTN_UNICAST && res.type != RTN_LOCAL)
+				goto out;
+			nh->nh_scope = res.scope;
+			nh->nh_oif = FIB_RES_OIF(res);
+			if ((nh->nh_dev = FIB_RES_DEV(res)) == NULL)
+				goto out;
+			dev_hold(nh->nh_dev);
+			if (!(nh->nh_dev->flags & IFF_UP)) {
+				if (fi->fib_protocol != RTPROT_STATIC) {
+					err = -ENETDOWN;
+					goto out;
+				}
+				nh->nh_flags |= RTNH_F_DEAD;
+			}
+			err = 0;
 out:
-		fib_res_put(&res);
-		return err;
+			fib_res_put(&res);
+			return err;
+		}
 	} else {
 		struct in_device *in_dev;
 
@@ -407,8 +436,11 @@ out:
 		if (in_dev == NULL)
 			return -ENODEV;
 		if (!(in_dev->dev->flags&IFF_UP)) {
-			in_dev_put(in_dev);
-			return -ENETDOWN;
+			if (fi->fib_protocol != RTPROT_STATIC) {
+				in_dev_put(in_dev);
+				return -ENETDOWN;
+			}
+			nh->nh_flags |= RTNH_F_DEAD;
 		}
 		nh->nh_dev = in_dev->dev;
 		dev_hold(nh->nh_dev);
@@ -606,8 +638,12 @@ fib_semantic_match(int type, struct fib_
 			for_nexthops(fi) {
 				if (nh->nh_flags&RTNH_F_DEAD)
 					continue;
-				if (!key->oif || key->oif == nh->nh_oif)
-					break;
+				if (key->oif && key->oif != nh->nh_oif)
+					continue;
+				if (key->gw && key->gw != nh->nh_gw &&
+				    nh->nh_gw && nh->nh_scope == RT_SCOPE_LINK)
+					continue;
+				break;
 			}
 #ifdef CONFIG_IP_ROUTE_MULTIPATH
 			if (nhsel < fi->fib_nhs) {
@@ -873,22 +909,35 @@ int fib_sync_down(u32 local, struct net_
 		if (local && fi->fib_prefsrc == local) {
 			fi->fib_flags |= RTNH_F_DEAD;
 			ret++;
-		} else if (dev && fi->fib_nhs) {
+		} else if (fi->fib_nhs) {
 			int dead = 0;
 
 			change_nexthops(fi) {
-				if (nh->nh_flags&RTNH_F_DEAD)
-					dead++;
-				else if (nh->nh_dev == dev &&
-					 nh->nh_scope != scope) {
-					nh->nh_flags |= RTNH_F_DEAD;
+				if (nh->nh_flags&RTNH_F_DEAD) {
+					if (fi->fib_protocol!=RTPROT_STATIC ||
+					    nh->nh_dev == NULL ||
+					    !__in_dev_get(nh->nh_dev) ||
+					    nh->nh_dev->flags&IFF_UP)
+						dead++;
+				} else if ((nh->nh_dev == dev && dev &&
+					    nh->nh_scope != scope) ||
+					    (local == nh->nh_gw && local &&
+					     nh->nh_oif)) {
+					write_lock_bh(&fib_nhflags_lock);
 #ifdef CONFIG_IP_ROUTE_MULTIPATH
-					spin_lock_bh(&fib_multipath_lock);
+					spin_lock(&fib_multipath_lock);
+					nh->nh_flags |= RTNH_F_DEAD;
 					fi->fib_power -= nh->nh_power;
 					nh->nh_power = 0;
-					spin_unlock_bh(&fib_multipath_lock);
+					spin_unlock(&fib_multipath_lock);
+#else
+					nh->nh_flags |= RTNH_F_DEAD;
 #endif
-					dead++;
+					write_unlock_bh(&fib_nhflags_lock);
+					if (fi->fib_protocol!=RTPROT_STATIC ||
+					    force ||
+					    (dev && __in_dev_get(dev) == NULL))
+						dead++;
 				}
 #ifdef CONFIG_IP_ROUTE_MULTIPATH
 				if (force > 1 && nh->nh_dev == dev) {
@@ -906,37 +955,55 @@ int fib_sync_down(u32 local, struct net_
 	return ret;
 }
 
-#ifdef CONFIG_IP_ROUTE_MULTIPATH
-
 /*
-   Dead device goes up. We wake up dead nexthops.
-   It takes sense only on multipath routes.
+   Dead device goes up or new address is added. We wake up dead nexthops.
  */
 
 int fib_sync_up(struct net_device *dev)
 {
-	int ret = 0;
+	struct rt_key key;
+	struct fib_result res;
+	int ret, rep;
 
+repeat:
 	if (!(dev->flags&IFF_UP))
 		return 0;
 
+	ret = 0;
+	rep = 0;
 	for_fib_info() {
 		int alive = 0;
 
 		change_nexthops(fi) {
-			if (!(nh->nh_flags&RTNH_F_DEAD)) {
-				alive++;
+			if (!(nh->nh_flags&RTNH_F_DEAD))
 				continue;
-			}
 			if (nh->nh_dev == NULL || !(nh->nh_dev->flags&IFF_UP))
 				continue;
 			if (nh->nh_dev != dev || __in_dev_get(dev) == NULL)
 				continue;
+			if (nh->nh_gw && fi->fib_protocol == RTPROT_STATIC) {
+				memset(&key, 0, sizeof(key));
+				key.dst = nh->nh_gw;
+				key.oif = nh->nh_oif;
+				key.scope = nh->nh_scope;
+				if (fib_lookup(&key, &res) != 0)
+					continue;
+				if (res.type != RTN_UNICAST &&
+				    res.type != RTN_LOCAL) {
+					fib_res_put(&res);
+					continue;
+				}
+				nh->nh_scope = res.scope;
+				fib_res_put(&res);
+				rep = 1;
+			}
 			alive++;
+#ifdef CONFIG_IP_ROUTE_MULTIPATH
 			spin_lock_bh(&fib_multipath_lock);
 			nh->nh_power = 0;
 			nh->nh_flags &= ~RTNH_F_DEAD;
 			spin_unlock_bh(&fib_multipath_lock);
+#endif
 		} endfor_nexthops(fi)
 
 		if (alive > 0) {
@@ -944,9 +1011,13 @@ int fib_sync_up(struct net_device *dev)
 			ret++;
 		}
 	} endfor_fib_info();
+	if (rep)
+		goto repeat;
 	return ret;
 }
 
+#ifdef CONFIG_IP_ROUTE_MULTIPATH
+
 /*
    The algorithm is suboptimal, but it provides really
    fair weighted route distribution.
@@ -955,24 +1026,45 @@ int fib_sync_up(struct net_device *dev)
 void fib_select_multipath(const struct rt_key *key, struct fib_result *res)
 {
 	struct fib_info *fi = res->fi;
-	int w;
+	int w, alive;
 
 	spin_lock_bh(&fib_multipath_lock);
+	if (key->oif) {
+		int sel = -1;
+		w = -1;
+		change_nexthops(fi) {
+			if (key->oif != nh->nh_oif)
+				continue;
+			if (key->gw && key->gw != nh->nh_gw &&
+			    nh->nh_gw && nh->nh_scope == RT_SCOPE_LINK)
+				continue;
+			if (!(nh->nh_flags&RTNH_F_BADSTATE)) {
+				if (nh->nh_power > w) {
+					w = nh->nh_power;
+					sel = nhsel;
+				}
+			}
+		} endfor_nexthops(fi);
+		if (sel >= 0) {
+			spin_unlock_bh(&fib_multipath_lock);
+			res->nh_sel = sel;
+			return;
+		}
+		goto last_resort;
+	}
+
+repeat:
 	if (fi->fib_power <= 0) {
 		int power = 0;
 		change_nexthops(fi) {
-			if (!(nh->nh_flags&RTNH_F_DEAD)) {
+			if (!(nh->nh_flags&RTNH_F_BADSTATE)) {
 				power += nh->nh_weight;
 				nh->nh_power = nh->nh_weight;
 			}
 		} endfor_nexthops(fi);
 		fi->fib_power = power;
-		if (power <= 0) {
-			spin_unlock_bh(&fib_multipath_lock);
-			/* Race condition: route has just become dead. */
-			res->nh_sel = 0;
-			return;
-		}
+		if (power <= 0)
+			goto last_resort;
 	}
 
 
@@ -982,20 +1074,40 @@ void fib_select_multipath(const struct r
 
 	w = jiffies % fi->fib_power;
 
+	alive = 0;
 	change_nexthops(fi) {
-		if (!(nh->nh_flags&RTNH_F_DEAD) && nh->nh_power) {
+		if (!(nh->nh_flags&RTNH_F_BADSTATE) && nh->nh_power) {
 			if ((w -= nh->nh_power) <= 0) {
 				nh->nh_power--;
 				fi->fib_power--;
-				res->nh_sel = nhsel;
 				spin_unlock_bh(&fib_multipath_lock);
+				res->nh_sel = nhsel;
 				return;
 			}
+			alive = 1;
+		}
+	} endfor_nexthops(fi);
+	if (alive) {
+		fi->fib_power = 0;
+		goto repeat;
+	}
+
+last_resort:
+
+	for_nexthops(fi) {
+		if (!(nh->nh_flags&RTNH_F_DEAD)) {
+			if (key->oif && key->oif != nh->nh_oif)
+				continue;
+			if (key->gw && key->gw != nh->nh_gw &&
+			    nh->nh_gw && nh->nh_scope == RT_SCOPE_LINK)
+				continue;
+			spin_unlock_bh(&fib_multipath_lock);
+			res->nh_sel = nhsel;
+			return;
 		}
 	} endfor_nexthops(fi);
 
 	/* Race condition: route has just become dead. */
-	res->nh_sel = 0;
 	spin_unlock_bh(&fib_multipath_lock);
 }
 #endif
Index: linux-2.4.35.4/net/ipv4/ip_nat_dumb.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/ip_nat_dumb.c
+++ linux-2.4.35.4/net/ipv4/ip_nat_dumb.c
@@ -124,6 +124,7 @@ ip_do_nat(struct sk_buff *skb)
 					key.dst = ciph->saddr;
 					key.iif = skb->dev->ifindex;
 					key.oif = 0;
+					key.gw	= 0;
 #ifdef CONFIG_IP_ROUTE_TOS
 					key.tos = RT_TOS(ciph->tos);
 #endif
Index: linux-2.4.35.4/net/ipv4/netfilter/ip_fw_compat_masq.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/netfilter/ip_fw_compat_masq.c
+++ linux-2.4.35.4/net/ipv4/netfilter/ip_fw_compat_masq.c
@@ -41,6 +41,10 @@ do_masquerade(struct sk_buff **pskb, con
 	enum ip_conntrack_info ctinfo;
 	struct ip_conntrack *ct;
 	unsigned int ret;
+	struct rtable *rt, *skb_rt;
+	struct net_device *skb_dev;
+	__u32 saddr;
+	int new;
 
 	/* Sorry, only ICMP, TCP and UDP. */
 	if (iph->protocol != IPPROTO_ICMP
@@ -64,22 +68,28 @@ do_masquerade(struct sk_buff **pskb, con
 	}
 
 	info = &ct->nat.info;
+	iph = (*pskb)->nh.iph;
+	saddr = iph->saddr;
+	new = 0;
 
 	WRITE_LOCK(&ip_nat_lock);
 	/* Setup the masquerade, if not already */
 	if (!info->initialized) {
 		u_int32_t newsrc;
-		struct rtable *rt;
 		struct ip_nat_multi_range range;
 
+		skb_rt = (struct rtable *) (*pskb)->dst;
+		skb_dev = skb_rt->u.dst.dev;
 		/* Pass 0 instead of saddr, since it's going to be changed
 		   anyway. */
-		if (ip_route_output(&rt, iph->daddr, 0, 0, 0) != 0) {
+		if (ip_route_output_lookup(&rt, iph->daddr, 0, RT_TOS(iph->tos),
+		    skb_dev? skb_dev->ifindex : 0,
+		    skb_dev? skb_rt->rt_gateway : 0) != 0) {
+			WRITE_UNLOCK(&ip_nat_lock);
 			DEBUGP("ipnat_rule_masquerade: Can't reroute.\n");
 			return NF_DROP;
 		}
-		newsrc = inet_select_addr(rt->u.dst.dev, rt->rt_gateway,
-					  RT_SCOPE_UNIVERSE);
+		newsrc = rt->rt_src;
 		ip_rt_put(rt);
 		range = ((struct ip_nat_multi_range)
 			 { 1,
@@ -92,11 +102,31 @@ do_masquerade(struct sk_buff **pskb, con
 			WRITE_UNLOCK(&ip_nat_lock);
 			return ret;
 		}
+		new = 1;
 	} else
 		DEBUGP("Masquerading already done on this conn.\n");
 	WRITE_UNLOCK(&ip_nat_lock);
 
-	return do_bindings(ct, ctinfo, info, NF_IP_POST_ROUTING, pskb);
+	ret = do_bindings(ct, ctinfo, info, NF_IP_POST_ROUTING, pskb);
+	if (ret != NF_ACCEPT || saddr == (*pskb)->nh.iph->saddr || new)
+		return ret;
+
+	iph = (*pskb)->nh.iph;
+	if (ip_route_output(&rt, iph->daddr, iph->saddr, RT_TOS(iph->tos), 0) != 0)
+		return NF_DROP;
+	
+	skb_rt = (struct rtable *) (*pskb)->dst;
+	skb_dev = skb_rt->u.dst.dev;
+	if (skb_dev != rt->u.dst.dev || rt->rt_gateway != skb_rt->rt_gateway) {
+		if (skb_dev != rt->u.dst.dev) {
+			/* TODO: check the new mtu and reply FRAG_NEEDED */
+		}
+		dst_release((*pskb)->dst);
+		(*pskb)->dst = &rt->u.dst;
+	} else {
+		ip_rt_put(rt);
+	}
+	return NF_ACCEPT;
 }
 
 void
Index: linux-2.4.35.4/net/ipv4/netfilter/ip_nat_core.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/netfilter/ip_nat_core.c
+++ linux-2.4.35.4/net/ipv4/netfilter/ip_nat_core.c
@@ -994,6 +994,60 @@ icmp_reply_translation(struct sk_buff *s
 	return NF_ACCEPT;
 }
 
+unsigned int
+ip_nat_route_input(unsigned int hooknum,
+		struct sk_buff **pskb,
+		const struct net_device *in,
+		const struct net_device *out,
+		int (*okfn)(struct sk_buff *))
+{
+	struct sk_buff *skb = *pskb;
+	struct iphdr *iph;
+	struct ip_conntrack *ct;
+	enum ip_conntrack_info ctinfo;
+	struct ip_nat_info *info;
+	enum ip_conntrack_dir dir;
+	__u32 saddr;
+	int i;
+
+	if (!(ct = ip_conntrack_get(skb, &ctinfo)))
+		return NF_ACCEPT;
+
+	info = &ct->nat.info;
+	if (!info->initialized)
+		return NF_ACCEPT;
+
+	if (skb->dst)
+		return NF_ACCEPT;
+
+	if (skb->len < sizeof(struct iphdr))
+		return NF_ACCEPT;
+
+	iph = skb->nh.iph;
+	saddr = iph->saddr;
+	hooknum = NF_IP_POST_ROUTING;
+	dir = CTINFO2DIR(ctinfo);
+
+	READ_LOCK(&ip_nat_lock);
+	for (i = 0; i < info->num_manips; i++) {
+		if (info->manips[i].direction == dir
+		    && info->manips[i].hooknum == hooknum
+		    && info->manips[i].maniptype == IP_NAT_MANIP_SRC) {
+			saddr = info->manips[i].manip.ip;
+		}
+	}
+	READ_UNLOCK(&ip_nat_lock);
+
+	if (saddr == iph->saddr)
+		return NF_ACCEPT;
+
+	if (ip_route_input_lookup(skb, iph->daddr, iph->saddr, iph->tos,
+	    skb->dev, saddr))
+		return NF_DROP;
+
+	return NF_ACCEPT;
+}
+
 int __init ip_nat_init(void)
 {
 	size_t i;
Index: linux-2.4.35.4/net/ipv4/netfilter/ip_nat_standalone.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/netfilter/ip_nat_standalone.c
+++ linux-2.4.35.4/net/ipv4/netfilter/ip_nat_standalone.c
@@ -245,6 +245,9 @@ ip_nat_local_fn(unsigned int hooknum,
 /* Before packet filtering, change destination */
 static struct nf_hook_ops ip_nat_in_ops
 = { { NULL, NULL }, ip_nat_in, PF_INET, NF_IP_PRE_ROUTING, NF_IP_PRI_NAT_DST };
+/* Before routing, route before mangling */
+static struct nf_hook_ops ip_nat_inr_ops
+= { { NULL, NULL }, ip_nat_route_input, PF_INET, NF_IP_PRE_ROUTING, NF_IP_PRI_LAST-1 };
 /* After packet filtering, change source */
 static struct nf_hook_ops ip_nat_out_ops
 = { { NULL, NULL }, ip_nat_out, PF_INET, NF_IP_POST_ROUTING, NF_IP_PRI_NAT_SRC};
@@ -313,10 +316,15 @@ static int init_or_cleanup(int init)
 		printk("ip_nat_init: can't register in hook.\n");
 		goto cleanup_nat;
 	}
+	ret = nf_register_hook(&ip_nat_inr_ops);
+	if (ret < 0) {
+		printk("ip_nat_init: can't register inr hook.\n");
+		goto cleanup_inops;
+	}
 	ret = nf_register_hook(&ip_nat_out_ops);
 	if (ret < 0) {
 		printk("ip_nat_init: can't register out hook.\n");
-		goto cleanup_inops;
+		goto cleanup_inrops;
 	}
 	ret = nf_register_hook(&ip_nat_local_out_ops);
 	if (ret < 0) {
@@ -336,6 +344,8 @@ static int init_or_cleanup(int init)
 	nf_unregister_hook(&ip_nat_local_out_ops);
  cleanup_outops:
 	nf_unregister_hook(&ip_nat_out_ops);
+ cleanup_inrops:
+	nf_unregister_hook(&ip_nat_inr_ops);
  cleanup_inops:
 	nf_unregister_hook(&ip_nat_in_ops);
  cleanup_nat:
Index: linux-2.4.35.4/net/ipv4/netfilter/ipt_MASQUERADE.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/netfilter/ipt_MASQUERADE.c
+++ linux-2.4.35.4/net/ipv4/netfilter/ipt_MASQUERADE.c
@@ -87,7 +87,8 @@ masquerade_target(struct sk_buff **pskb,
 	key.dst = (*pskb)->nh.iph->daddr;
 	key.src = 0; /* Unknown: that's what we're trying to establish */
 	key.tos = RT_TOS((*pskb)->nh.iph->tos)|RTO_CONN;
-	key.oif = 0;
+	key.oif = out->ifindex;
+	key.gw	= ((struct rtable *) (*pskb)->dst)->rt_gateway;
 #ifdef CONFIG_IP_ROUTE_FWMARK
 	key.fwmark = (*pskb)->nfmark;
 #endif
@@ -98,13 +99,6 @@ masquerade_target(struct sk_buff **pskb,
                                " No route: Rusty's brain broke!\n");
                 return NF_DROP;
         }
-        if (rt->u.dst.dev != out) {
-                if (net_ratelimit())
-                        printk("MASQUERADE:"
-                               " Route sent us somewhere else.\n");
-			ip_rt_put(rt);
-		return NF_DROP;
-	}
 
 	newsrc = rt->rt_src;
 	DEBUGP("newsrc = %u.%u.%u.%u\n", NIPQUAD(newsrc));
Index: linux-2.4.35.4/net/ipv4/route.c
===================================================================
--- linux-2.4.35.4.orig/net/ipv4/route.c
+++ linux-2.4.35.4/net/ipv4/route.c
@@ -919,6 +919,7 @@ void ip_rt_redirect(u32 old_gw, u32 dadd
 
 				/* Gateway is different ... */
 				rt->rt_gateway		= new_gw;
+				if (rt->key.gw) rt->key.gw = new_gw;
 
 				/* Redirect received -> path was valid */
 				dst_confirm(&rth->u.dst);
@@ -1343,6 +1344,7 @@ static int ip_route_input_mc(struct sk_b
 	rth->key.fwmark	= skb->nfmark;
 #endif
 	rth->key.src	= saddr;
+	rth->key.lsrc	= 0;
 	rth->rt_src	= saddr;
 #ifdef CONFIG_IP_ROUTE_NAT
 	rth->rt_dst_map	= daddr;
@@ -1356,6 +1358,7 @@ static int ip_route_input_mc(struct sk_b
 	rth->u.dst.dev	= &loopback_dev;
 	dev_hold(rth->u.dst.dev);
 	rth->key.oif	= 0;
+	rth->key.gw	= 0;
 	rth->rt_gateway	= daddr;
 	rth->rt_spec_dst= spec_dst;
 	rth->rt_type	= RTN_MULTICAST;
@@ -1395,7 +1398,7 @@ e_inval:
  */
 
 int ip_route_input_slow(struct sk_buff *skb, u32 daddr, u32 saddr,
-			u8 tos, struct net_device *dev)
+			u8 tos, struct net_device *dev, u32 lsrc)
 {
 	struct rt_key	key;
 	struct fib_result res;
@@ -1415,16 +1418,17 @@ int ip_route_input_slow(struct sk_buff *
 		goto out;
 
 	key.dst		= daddr;
-	key.src		= saddr;
+	key.src		= lsrc? : saddr;
 	key.tos		= tos;
 #ifdef CONFIG_IP_ROUTE_FWMARK
 	key.fwmark	= skb->nfmark;
 #endif
-	key.iif		= dev->ifindex;
+	key.iif		= lsrc? loopback_dev.ifindex : dev->ifindex;
 	key.oif		= 0;
+	key.gw		= 0;
 	key.scope	= RT_SCOPE_UNIVERSE;
 
-	hash = rt_hash_code(daddr, saddr ^ (key.iif << 5), tos);
+	hash = rt_hash_code(daddr, saddr ^ (dev->ifindex << 5), tos);
 
 	/* Check for the most weird martians, which can be not detected
 	   by fib_lookup.
@@ -1445,6 +1449,12 @@ int ip_route_input_slow(struct sk_buff *
 	if (BADCLASS(daddr) || ZERONET(daddr) || LOOPBACK(daddr))
 		goto martian_destination;
 
+	if (lsrc) {
+		if (MULTICAST(lsrc) || BADCLASS(lsrc) ||
+		    ZERONET(lsrc) || LOOPBACK(lsrc))
+			goto e_inval;
+	}
+
 	/*
 	 *	Now we are ready to route packet.
 	 */
@@ -1454,6 +1464,10 @@ int ip_route_input_slow(struct sk_buff *
 		goto no_route;
 	}
 	free_res = 1;
+	if (lsrc && res.type != RTN_UNICAST && res.type != RTN_NAT)
+		goto e_inval;
+	key.iif = dev->ifindex;
+	key.src = saddr;
 
 	rt_cache_stat[smp_processor_id()].in_slow_tot++;
 
@@ -1464,7 +1478,7 @@ int ip_route_input_slow(struct sk_buff *
 
 	if (1) {
 		u32 src_map = saddr;
-		if (res.r)
+		if (res.r && !lsrc)
 			src_map = fib_rules_policy(saddr, &res, &flags);
 
 		if (res.type == RTN_NAT) {
@@ -1503,8 +1517,9 @@ int ip_route_input_slow(struct sk_buff *
 	if (res.type != RTN_UNICAST)
 		goto martian_destination;
 
+	fib_select_default(&key, &res);
 #ifdef CONFIG_IP_ROUTE_MULTIPATH
-	if (res.fi->fib_nhs > 1 && key.oif == 0)
+	if (res.fi->fib_nhs > 1)
 		fib_select_multipath(&key, &res);
 #endif
 	out_dev = in_dev_get(FIB_RES_DEV(res));
@@ -1524,6 +1539,7 @@ int ip_route_input_slow(struct sk_buff *
 		flags |= RTCF_DIRECTSRC;
 
 	if (out_dev == in_dev && err && !(flags & (RTCF_NAT | RTCF_MASQ)) &&
+	    !lsrc &&
 	    (IN_DEV_SHARED_MEDIA(out_dev) ||
 	     inet_addr_onlink(out_dev, saddr, FIB_RES_GW(res))))
 		flags |= RTCF_DOREDIRECT;
@@ -1550,6 +1566,7 @@ int ip_route_input_slow(struct sk_buff *
 #endif
 	rth->key.src	= saddr;
 	rth->rt_src	= saddr;
+	rth->key.lsrc	= lsrc;
 	rth->rt_gateway	= daddr;
 #ifdef CONFIG_IP_ROUTE_NAT
 	rth->rt_src_map	= key.src;
@@ -1562,6 +1579,7 @@ int ip_route_input_slow(struct sk_buff *
 	rth->u.dst.dev	= out_dev->dev;
 	dev_hold(rth->u.dst.dev);
 	rth->key.oif 	= 0;
+	rth->key.gw	= 0;
 	rth->rt_spec_dst= spec_dst;
 
 	rth->u.dst.input = ip_forward;
@@ -1572,7 +1590,8 @@ int ip_route_input_slow(struct sk_buff *
 	rth->rt_flags = flags;
 
 #ifdef CONFIG_NET_FASTROUTE
-	if (netdev_fastroute && !(flags&(RTCF_NAT|RTCF_MASQ|RTCF_DOREDIRECT))) {
+	if (netdev_fastroute && !(flags&(RTCF_NAT|RTCF_MASQ|RTCF_DOREDIRECT)) &&
+	    !lsrc) {
 		struct net_device *odev = rth->u.dst.dev;
 		if (odev != dev &&
 		    dev->accept_fastpath &&
@@ -1595,6 +1614,8 @@ out:	return err;
 brd_input:
 	if (skb->protocol != htons(ETH_P_IP))
 		goto e_inval;
+	if (lsrc)
+		goto e_inval;
 
 	if (ZERONET(saddr))
 		spec_dst = inet_select_addr(dev, 0, RT_SCOPE_LINK);
@@ -1627,6 +1648,7 @@ local_input:
 #endif
 	rth->key.src	= saddr;
 	rth->rt_src	= saddr;
+	rth->key.lsrc	= 0;
 #ifdef CONFIG_IP_ROUTE_NAT
 	rth->rt_dst_map	= key.dst;
 	rth->rt_src_map	= key.src;
@@ -1639,6 +1661,7 @@ local_input:
 	rth->u.dst.dev	= &loopback_dev;
 	dev_hold(rth->u.dst.dev);
 	rth->key.oif 	= 0;
+	rth->key.gw	= 0;
 	rth->rt_gateway	= daddr;
 	rth->rt_spec_dst= spec_dst;
 	rth->u.dst.input= ip_local_deliver;
@@ -1704,8 +1727,9 @@ martian_source:
 	goto e_inval;
 }
 
-int ip_route_input(struct sk_buff *skb, u32 daddr, u32 saddr,
-		   u8 tos, struct net_device *dev)
+static inline int
+ip_route_input_cached(struct sk_buff *skb, u32 daddr, u32 saddr,
+		      u8 tos, struct net_device *dev, u32 lsrc)
 {
 	struct rtable * rth;
 	unsigned	hash;
@@ -1719,6 +1743,7 @@ int ip_route_input(struct sk_buff *skb, 
 		if (rth->key.dst == daddr &&
 		    rth->key.src == saddr &&
 		    rth->key.iif == iif &&
+		    rth->key.lsrc == lsrc &&
 		    rth->key.oif == 0 &&
 #ifdef CONFIG_IP_ROUTE_FWMARK
 		    rth->key.fwmark == skb->nfmark &&
@@ -1766,9 +1791,21 @@ int ip_route_input(struct sk_buff *skb, 
 		read_unlock(&inetdev_lock);
 		return -EINVAL;
 	}
-	return ip_route_input_slow(skb, daddr, saddr, tos, dev);
+	return ip_route_input_slow(skb, daddr, saddr, tos, dev, lsrc);
+}
+
+int ip_route_input(struct sk_buff *skb, u32 daddr, u32 saddr,
+		   u8 tos, struct net_device *dev)
+{
+	return ip_route_input_cached(skb, daddr, saddr, tos, dev, 0);
 }
 
+int ip_route_input_lookup(struct sk_buff *skb, u32 daddr, u32 saddr,
+			  u8 tos, struct net_device *dev, u32 lsrc)
+{
+	return ip_route_input_cached(skb, daddr, saddr, tos, dev, lsrc);
+}
+ 
 /*
  * Major route resolver routine.
  */
@@ -1791,6 +1828,7 @@ int ip_route_output_slow(struct rtable *
 	key.tos		= tos & IPTOS_RT_MASK;
 	key.iif		= loopback_dev.ifindex;
 	key.oif		= oldkey->oif;
+	key.gw		= oldkey->gw;
 #ifdef CONFIG_IP_ROUTE_FWMARK
 	key.fwmark	= oldkey->fwmark;
 #endif
@@ -1880,6 +1918,7 @@ int ip_route_output_slow(struct rtable *
 		dev_out = &loopback_dev;
 		dev_hold(dev_out);
 		key.oif = loopback_dev.ifindex;
+		key.gw = 0;
 		res.type = RTN_LOCAL;
 		flags |= RTCF_LOCAL;
 		goto make_route;
@@ -1887,7 +1926,7 @@ int ip_route_output_slow(struct rtable *
 
 	if (fib_lookup(&key, &res)) {
 		res.fi = NULL;
-		if (oldkey->oif) {
+		if (oldkey->oif && dev_out->flags&IFF_UP) {
 			/* Apparently, routing tables are wrong. Assume,
 			   that the destination is on link.
 
@@ -1930,6 +1969,7 @@ int ip_route_output_slow(struct rtable *
 		dev_out = &loopback_dev;
 		dev_hold(dev_out);
 		key.oif = dev_out->ifindex;
+		key.gw = 0;
 		if (res.fi)
 			fib_info_put(res.fi);
 		res.fi = NULL;
@@ -1937,13 +1977,12 @@ int ip_route_output_slow(struct rtable *
 		goto make_route;
 	}
 
+	if (res.type == RTN_UNICAST)
+		fib_select_default(&key, &res);
 #ifdef CONFIG_IP_ROUTE_MULTIPATH
-	if (res.fi->fib_nhs > 1 && key.oif == 0)
+	if (res.fi->fib_nhs > 1)
 		fib_select_multipath(&key, &res);
-	else
 #endif
-	if (!res.prefixlen && res.type == RTN_UNICAST && !key.oif)
-		fib_select_default(&key, &res);
 
 	if (!key.src)
 		key.src = FIB_RES_PREFSRC(res);
@@ -2001,7 +2040,9 @@ make_route:
 	rth->key.tos	= tos;
 	rth->key.src	= oldkey->src;
 	rth->key.iif	= 0;
+	rth->key.lsrc	= 0;
 	rth->key.oif	= oldkey->oif;
+	rth->key.gw	= oldkey->gw;
 #ifdef CONFIG_IP_ROUTE_FWMARK
 	rth->key.fwmark	= oldkey->fwmark;
 #endif
@@ -2080,6 +2121,7 @@ int ip_route_output_key(struct rtable **
 		    rth->key.src == key->src &&
 		    rth->key.iif == 0 &&
 		    rth->key.oif == key->oif &&
+		    rth->key.gw == key->gw &&
 #ifdef CONFIG_IP_ROUTE_FWMARK
 		    rth->key.fwmark == key->fwmark &&
 #endif
Index: linux-2.4.35.4/net/netsyms.c
===================================================================
--- linux-2.4.35.4.orig/net/netsyms.c
+++ linux-2.4.35.4/net/netsyms.c
@@ -260,6 +260,7 @@ EXPORT_SYMBOL(inet_register_protosw);
 EXPORT_SYMBOL(inet_unregister_protosw);
 EXPORT_SYMBOL(ip_route_output_key);
 EXPORT_SYMBOL(ip_route_input);
+EXPORT_SYMBOL(ip_route_input_lookup);
 EXPORT_SYMBOL(icmp_send);
 EXPORT_SYMBOL(icmp_statistics);
 EXPORT_SYMBOL(icmp_err_convert);
