--- a/drivers/net/sl351x_gmac.c
+++ b/drivers/net/sl351x_gmac.c
@@ -68,9 +68,11 @@
 #include <linux/ip.h>
 #endif
 
+/* Enables NAPI unconditionally */
+#define CONFIG_SL_NAPI					1
+
 // #define SL351x_TEST_WORKAROUND
 #ifdef CONFIG_SL351x_NAT
-#define CONFIG_SL_NAPI					1
 #endif
 #define GMAX_TX_INTR_DISABLED			1
 #define DO_HW_CHKSUM					1
@@ -124,12 +126,17 @@ static	char _debug_prefetch_buf[_DEBUG_P
  *************************************************************/
 static int	gmac_initialized = 0;
 TOE_INFO_T toe_private_data;
-//static int		do_again = 0;
+static int		do_again = 0;
 spinlock_t gmac_fq_lock;
 unsigned int FLAG_SWITCH;
 
 static unsigned int     	next_tick = 3 * HZ;
-static unsigned char    	eth_mac[CONFIG_MAC_NUM][6]= {{0x00,0x11,0x11,0x87,0x87,0x87}, {0x00,0x22,0x22,0xab,0xab,0xab}};
+static unsigned char    	eth_mac[CONFIG_MAC_NUM][6]= {
+		{0x00,0x11,0x11,0x87,0x87,0x87},
+#if GMAC_NUM != 1
+		{0x00,0x22,0x22,0xab,0xab,0xab}
+#endif
+};
 
 #undef CONFIG_SL351x_RXTOE
 extern NAT_CFG_T nat_cfg;
@@ -2443,7 +2450,8 @@ static irqreturn_t toe_gmac_interrupt (i
 	toe = (TOE_INFO_T *)&toe_private_data;
 //	handle NAPI
 #ifdef CONFIG_SL_NAPI
-if (storlink_ctl.pauseoff == 1)
+	/* XXX: check this, changed from 'storlink_ctl.pauseoff == 1' to if (1) */
+if (1)
 {
 /* disable GMAC interrupt */
     //toe_gmac_disable_interrupt(tp->irq);
@@ -2530,7 +2538,7 @@ if (storlink_ctl.pauseoff == 1)
 				{
 					if (likely(netif_rx_schedule_prep(dev)))
         			{
-        				unsigned int data32;
+        				// unsigned int data32;
         				// disable GMAC-0 rx interrupt
         				// class-Q & TOE-Q are implemented in future
         				//data32 = readl(TOE_GLOBAL_BASE + GLOBAL_INTERRUPT_ENABLE_1_REG);
@@ -2563,7 +2571,7 @@ if (storlink_ctl.pauseoff == 1)
 			{
 				if (likely(netif_rx_schedule_prep(dev)))
         		{
-        			unsigned int data32;
+        			// unsigned int data32;
          			// disable GMAC-0 rx interrupt
         			// class-Q & TOE-Q are implemented in future
         			//data32 = readl(TOE_GLOBAL_BASE + GLOBAL_INTERRUPT_ENABLE_1_REG);
@@ -4217,7 +4225,7 @@ static int gmac_rx_poll(struct net_devic
 	GMAC_INFO_T			*tp = (GMAC_INFO_T *)dev->priv;
 	unsigned int		status4;
 	volatile DMA_RWPTR_T	fq_rwptr;
-	int					max_cnt = TOE_SW_FREEQ_DESC_NUM;//TOE_SW_FREEQ_DESC_NUM = 64
+	// int					max_cnt = TOE_SW_FREEQ_DESC_NUM;//TOE_SW_FREEQ_DESC_NUM = 64
 	//unsigned long		rx_old_bytes;
 	struct net_device_stats *isPtr = (struct net_device_stats *)&tp->ifStatics;
 	//unsigned long long	rx_time;
@@ -4479,7 +4487,7 @@ static int gmac_rx_poll(struct net_devic
 
 	if (rwptr.bits.rptr == rwptr.bits.wptr)
 	{
-		unsigned int data32;
+		// unsigned int data32;
 			//printk("%s:---[rwptr.bits.rptr == rwptr.bits.wptr]   rx_pkts_num=%d------rwptr.bits.rptr=0x%x------->Default_Q [rwptr.bits.rptr(SW)=0x%x,   rwptr.bits.wptr(HW) = 0x%x ]---->Free_Q(SW_HW) = 0x%8x \n",__func__,rx_pkts_num,rwptr.bits.rptr,rwptr.bits.rptr,rwptr.bits.wptr,fq_rwptr.bits32 );
 
 	    /* Receive descriptor is empty now */
