From 1a3175837f88ce0d121bcaa4c8947872eb201a22 Mon Sep 17 00:00:00 2001
From: Daniel Machon <daniel.machon@microchip.com>
Date: Fri, 1 Nov 2024 08:09:11 +0100
Subject: [PATCH 62/82] net: lan969x: add autogenerated VCAP information
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Platform VCAP data for each VCAP instance is auto-generated using an
internal Microchip tool. The generated VCAP data contains information
about keyfields, keyfield sets, actionfields, actionfield sets and
typegroups, which in combination are used to encode and decode rules in
the VCAP.

Add the auto-generated VCAP file lan969x_vcap_ag_api.c and assign the
two structs: lan969x_vcaps and lan969x_vcap_stats to the match data.

Reviewed-by: Steen Hegelund <Steen.Hegelund@microchip.com>
Reviewed-by: Jens Emil Schulz Østergaard <jensemil.schulzostergaard@microchip.com>
Signed-off-by: Daniel Machon <daniel.machon@microchip.com>
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 .../net/ethernet/microchip/lan969x/Makefile   |    3 +-
 .../net/ethernet/microchip/lan969x/lan969x.c  |    2 +
 .../net/ethernet/microchip/lan969x/lan969x.h  |    5 +
 .../microchip/lan969x/lan969x_vcap_ag_api.c   | 3843 +++++++++++++++++
 4 files changed, 3852 insertions(+), 1 deletion(-)
 create mode 100644 drivers/net/ethernet/microchip/lan969x/lan969x_vcap_ag_api.c

--- a/drivers/net/ethernet/microchip/lan969x/Makefile
+++ b/drivers/net/ethernet/microchip/lan969x/Makefile
@@ -5,7 +5,8 @@
 
 obj-$(CONFIG_LAN969X_SWITCH) += lan969x-switch.o
 
-lan969x-switch-y := lan969x_regs.o lan969x.o lan969x_calendar.o
+lan969x-switch-y := lan969x_regs.o lan969x.o lan969x_calendar.o \
+ lan969x_vcap_ag_api.o
 
 # Provide include files
 ccflags-y += -I$(srctree)/drivers/net/ethernet/microchip/fdma
--- a/drivers/net/ethernet/microchip/lan969x/lan969x.c
+++ b/drivers/net/ethernet/microchip/lan969x/lan969x.c
@@ -319,6 +319,8 @@ static const struct sparx5_consts lan969
 	.qres_max_prio_idx   = 315,
 	.qres_max_colour_idx = 323,
 	.tod_pin             = 4,
+	.vcaps               = lan969x_vcaps,
+	.vcap_stats          = &lan969x_vcap_stats,
 };
 
 static const struct sparx5_ops lan969x_ops = {
--- a/drivers/net/ethernet/microchip/lan969x/lan969x.h
+++ b/drivers/net/ethernet/microchip/lan969x/lan969x.h
@@ -9,10 +9,15 @@
 
 #include "../sparx5/sparx5_main.h"
 #include "../sparx5/sparx5_regs.h"
+#include "../sparx5/sparx5_vcap_impl.h"
 
 /* lan969x.c */
 extern const struct sparx5_match_data lan969x_desc;
 
+/* lan969x_vcap_ag_api.c */
+extern const struct vcap_statistics lan969x_vcap_stats;
+extern const struct vcap_info lan969x_vcaps[];
+
 /* lan969x_regs.c */
 extern const unsigned int lan969x_tsize[TSIZE_LAST];
 extern const unsigned int lan969x_raddr[RADDR_LAST];
--- /dev/null
+++ b/drivers/net/ethernet/microchip/lan969x/lan969x_vcap_ag_api.c
@@ -0,0 +1,3843 @@
+// SPDX-License-Identifier: BSD-3-Clause
+/* Copyright (C) 2024 Microchip Technology Inc. and its subsidiaries.
+ * Microchip VCAP API
+ */
+
+/* This file is autogenerated by cml-utils 2024-10-07 11:10:56 +0200.
+ * Commit ID: b5ddc8e244eb2481a9524f1ddc630a8b41e7c391
+ */
+
+#include <linux/types.h>
+#include <linux/kernel.h>
+
+#include "lan969x.h"
+
+/* keyfields */
+static const struct vcap_field is0_normal_7tuple_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 0,
+		.width = 1,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 1,
+		.width = 1,
+	},
+	[VCAP_KF_LOOKUP_GEN_IDX_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 2,
+		.width = 2,
+	},
+	[VCAP_KF_LOOKUP_GEN_IDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 4,
+		.width = 10,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 14,
+		.width = 2,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U72,
+		.offset = 16,
+		.width = 65,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 81,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 82,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 83,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_TPID0] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 86,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_PCP0] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 89,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 92,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID0] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 93,
+		.width = 12,
+	},
+	[VCAP_KF_8021Q_TPID1] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 105,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_PCP1] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 108,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI1] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 111,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID1] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 112,
+		.width = 12,
+	},
+	[VCAP_KF_8021Q_TPID2] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 124,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_PCP2] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 127,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI2] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 130,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID2] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 131,
+		.width = 12,
+	},
+	[VCAP_KF_L2_DMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 144,
+		.width = 48,
+	},
+	[VCAP_KF_L2_SMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 192,
+		.width = 48,
+	},
+	[VCAP_KF_IP_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 240,
+		.width = 1,
+	},
+	[VCAP_KF_ETYPE_LEN_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 241,
+		.width = 1,
+	},
+	[VCAP_KF_ETYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 242,
+		.width = 16,
+	},
+	[VCAP_KF_IP_SNAP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 258,
+		.width = 1,
+	},
+	[VCAP_KF_IP4_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 259,
+		.width = 1,
+	},
+	[VCAP_KF_L3_FRAGMENT_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 260,
+		.width = 2,
+	},
+	[VCAP_KF_L3_FRAG_INVLD_L4_LEN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 262,
+		.width = 1,
+	},
+	[VCAP_KF_L3_OPTIONS_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 263,
+		.width = 1,
+	},
+	[VCAP_KF_L3_DSCP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 264,
+		.width = 6,
+	},
+	[VCAP_KF_L3_IP6_DIP] = {
+		.type = VCAP_FIELD_U128,
+		.offset = 270,
+		.width = 128,
+	},
+	[VCAP_KF_L3_IP6_SIP] = {
+		.type = VCAP_FIELD_U128,
+		.offset = 398,
+		.width = 128,
+	},
+	[VCAP_KF_TCP_UDP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 526,
+		.width = 1,
+	},
+	[VCAP_KF_TCP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 527,
+		.width = 1,
+	},
+	[VCAP_KF_L4_SPORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 528,
+		.width = 16,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 544,
+		.width = 8,
+	},
+};
+
+static const struct vcap_field is0_normal_5tuple_ip4_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 2,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 2,
+		.width = 1,
+	},
+	[VCAP_KF_LOOKUP_GEN_IDX_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 3,
+		.width = 2,
+	},
+	[VCAP_KF_LOOKUP_GEN_IDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 5,
+		.width = 10,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 15,
+		.width = 2,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U72,
+		.offset = 17,
+		.width = 65,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 82,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 83,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 84,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_TPID0] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 87,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_PCP0] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 90,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 93,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID0] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 94,
+		.width = 12,
+	},
+	[VCAP_KF_8021Q_TPID1] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 106,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_PCP1] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 109,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI1] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 112,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID1] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 113,
+		.width = 12,
+	},
+	[VCAP_KF_8021Q_TPID2] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 125,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_PCP2] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 128,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI2] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 131,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID2] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 132,
+		.width = 12,
+	},
+	[VCAP_KF_IP_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 145,
+		.width = 1,
+	},
+	[VCAP_KF_IP4_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 146,
+		.width = 1,
+	},
+	[VCAP_KF_L3_FRAGMENT_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 147,
+		.width = 2,
+	},
+	[VCAP_KF_L3_FRAG_INVLD_L4_LEN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 149,
+		.width = 1,
+	},
+	[VCAP_KF_L3_OPTIONS_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 150,
+		.width = 1,
+	},
+	[VCAP_KF_L3_DSCP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 151,
+		.width = 6,
+	},
+	[VCAP_KF_L3_IP4_DIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 157,
+		.width = 32,
+	},
+	[VCAP_KF_L3_IP4_SIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 189,
+		.width = 32,
+	},
+	[VCAP_KF_L3_IP_PROTO] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 221,
+		.width = 8,
+	},
+	[VCAP_KF_TCP_UDP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 229,
+		.width = 1,
+	},
+	[VCAP_KF_TCP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 230,
+		.width = 1,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 231,
+		.width = 8,
+	},
+	[VCAP_KF_IP_PAYLOAD_5TUPLE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 239,
+		.width = 32,
+	},
+};
+
+static const struct vcap_field is2_mac_etype_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 4,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 4,
+		.width = 1,
+	},
+	[VCAP_KF_LOOKUP_PAG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 5,
+		.width = 8,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_L3] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 14,
+		.width = 4,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 18,
+		.width = 2,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 20,
+		.width = 32,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 52,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 53,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 54,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 56,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 57,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 67,
+		.width = 13,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 80,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 81,
+		.width = 3,
+	},
+	[VCAP_KF_L2_FWD_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 84,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_L3_DST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 88,
+		.width = 1,
+	},
+	[VCAP_KF_L2_DMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 89,
+		.width = 48,
+	},
+	[VCAP_KF_L2_SMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 137,
+		.width = 48,
+	},
+	[VCAP_KF_ETYPE_LEN_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 185,
+		.width = 1,
+	},
+	[VCAP_KF_ETYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 186,
+		.width = 16,
+	},
+	[VCAP_KF_L2_PAYLOAD_ETYPE] = {
+		.type = VCAP_FIELD_U64,
+		.offset = 202,
+		.width = 64,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 266,
+		.width = 16,
+	},
+	[VCAP_KF_OAM_CCM_CNTS_EQ0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 282,
+		.width = 1,
+	},
+	[VCAP_KF_OAM_Y1731_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 283,
+		.width = 1,
+	},
+};
+
+static const struct vcap_field is2_arp_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 4,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 4,
+		.width = 1,
+	},
+	[VCAP_KF_LOOKUP_PAG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 5,
+		.width = 8,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_L3] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 14,
+		.width = 4,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 18,
+		.width = 2,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 20,
+		.width = 32,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 52,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 53,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 54,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 56,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 57,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 67,
+		.width = 13,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 80,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 81,
+		.width = 3,
+	},
+	[VCAP_KF_L2_FWD_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 84,
+		.width = 1,
+	},
+	[VCAP_KF_L2_SMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 85,
+		.width = 48,
+	},
+	[VCAP_KF_ARP_ADDR_SPACE_OK_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 133,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_PROTO_SPACE_OK_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 134,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_LEN_OK_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 135,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_TGT_MATCH_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 136,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_SENDER_MATCH_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 137,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_OPCODE_UNKNOWN_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 138,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_OPCODE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 139,
+		.width = 2,
+	},
+	[VCAP_KF_L3_IP4_DIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 141,
+		.width = 32,
+	},
+	[VCAP_KF_L3_IP4_SIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 173,
+		.width = 32,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 205,
+		.width = 1,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 206,
+		.width = 16,
+	},
+};
+
+static const struct vcap_field is2_ip4_tcp_udp_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 4,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 4,
+		.width = 1,
+	},
+	[VCAP_KF_LOOKUP_PAG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 5,
+		.width = 8,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_L3] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 14,
+		.width = 4,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 18,
+		.width = 2,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 20,
+		.width = 32,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 52,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 53,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 54,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 56,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 57,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 67,
+		.width = 13,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 80,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 81,
+		.width = 3,
+	},
+	[VCAP_KF_L2_FWD_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 84,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_L3_DST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 88,
+		.width = 1,
+	},
+	[VCAP_KF_IP4_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 89,
+		.width = 1,
+	},
+	[VCAP_KF_L3_FRAGMENT_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 90,
+		.width = 2,
+	},
+	[VCAP_KF_L3_FRAG_INVLD_L4_LEN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 92,
+		.width = 1,
+	},
+	[VCAP_KF_L3_OPTIONS_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 93,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TTL_GT0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 94,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TOS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 95,
+		.width = 8,
+	},
+	[VCAP_KF_L3_IP4_DIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 103,
+		.width = 32,
+	},
+	[VCAP_KF_L3_IP4_SIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 135,
+		.width = 32,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 167,
+		.width = 1,
+	},
+	[VCAP_KF_TCP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 168,
+		.width = 1,
+	},
+	[VCAP_KF_L4_DPORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 169,
+		.width = 16,
+	},
+	[VCAP_KF_L4_SPORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 185,
+		.width = 16,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 201,
+		.width = 16,
+	},
+	[VCAP_KF_L4_SPORT_EQ_DPORT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 217,
+		.width = 1,
+	},
+	[VCAP_KF_L4_SEQUENCE_EQ0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 218,
+		.width = 1,
+	},
+	[VCAP_KF_L4_FIN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 219,
+		.width = 1,
+	},
+	[VCAP_KF_L4_SYN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 220,
+		.width = 1,
+	},
+	[VCAP_KF_L4_RST] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 221,
+		.width = 1,
+	},
+	[VCAP_KF_L4_PSH] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 222,
+		.width = 1,
+	},
+	[VCAP_KF_L4_ACK] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 223,
+		.width = 1,
+	},
+	[VCAP_KF_L4_URG] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 224,
+		.width = 1,
+	},
+	[VCAP_KF_L4_PAYLOAD] = {
+		.type = VCAP_FIELD_U64,
+		.offset = 225,
+		.width = 64,
+	},
+};
+
+static const struct vcap_field is2_ip4_other_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 4,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 4,
+		.width = 1,
+	},
+	[VCAP_KF_LOOKUP_PAG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 5,
+		.width = 8,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_L3] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 14,
+		.width = 4,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 18,
+		.width = 2,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 20,
+		.width = 32,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 52,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 53,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 54,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 56,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 57,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 67,
+		.width = 13,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 80,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 81,
+		.width = 3,
+	},
+	[VCAP_KF_L2_FWD_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 84,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_L3_DST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 88,
+		.width = 1,
+	},
+	[VCAP_KF_IP4_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 89,
+		.width = 1,
+	},
+	[VCAP_KF_L3_FRAGMENT_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 90,
+		.width = 2,
+	},
+	[VCAP_KF_L3_FRAG_INVLD_L4_LEN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 92,
+		.width = 1,
+	},
+	[VCAP_KF_L3_OPTIONS_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 93,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TTL_GT0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 94,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TOS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 95,
+		.width = 8,
+	},
+	[VCAP_KF_L3_IP4_DIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 103,
+		.width = 32,
+	},
+	[VCAP_KF_L3_IP4_SIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 135,
+		.width = 32,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 167,
+		.width = 1,
+	},
+	[VCAP_KF_L3_IP_PROTO] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 168,
+		.width = 8,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 176,
+		.width = 16,
+	},
+	[VCAP_KF_L3_PAYLOAD] = {
+		.type = VCAP_FIELD_U112,
+		.offset = 192,
+		.width = 96,
+	},
+};
+
+static const struct vcap_field is2_ip6_std_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 4,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 4,
+		.width = 1,
+	},
+	[VCAP_KF_LOOKUP_PAG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 5,
+		.width = 8,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_L3] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 14,
+		.width = 4,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 18,
+		.width = 2,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 20,
+		.width = 32,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 52,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 53,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 54,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 56,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 57,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 67,
+		.width = 13,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 80,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 81,
+		.width = 3,
+	},
+	[VCAP_KF_L2_FWD_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 84,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TTL_GT0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 89,
+		.width = 1,
+	},
+	[VCAP_KF_L3_IP6_SIP] = {
+		.type = VCAP_FIELD_U128,
+		.offset = 90,
+		.width = 128,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 218,
+		.width = 1,
+	},
+	[VCAP_KF_L3_IP_PROTO] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 219,
+		.width = 8,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 227,
+		.width = 16,
+	},
+	[VCAP_KF_L3_PAYLOAD] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 243,
+		.width = 40,
+	},
+};
+
+static const struct vcap_field is2_ip_7tuple_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 2,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 2,
+		.width = 1,
+	},
+	[VCAP_KF_LOOKUP_PAG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 3,
+		.width = 8,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_L3] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 11,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 12,
+		.width = 4,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 16,
+		.width = 2,
+	},
+	[VCAP_KF_IF_IGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U72,
+		.offset = 18,
+		.width = 65,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 83,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 84,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 85,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 88,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 98,
+		.width = 13,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 111,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 112,
+		.width = 3,
+	},
+	[VCAP_KF_L2_FWD_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 115,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 118,
+		.width = 1,
+	},
+	[VCAP_KF_L3_DST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 119,
+		.width = 1,
+	},
+	[VCAP_KF_L2_DMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 120,
+		.width = 48,
+	},
+	[VCAP_KF_L2_SMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 168,
+		.width = 48,
+	},
+	[VCAP_KF_IP4_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 218,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TTL_GT0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 219,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TOS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 220,
+		.width = 8,
+	},
+	[VCAP_KF_L3_IP6_DIP] = {
+		.type = VCAP_FIELD_U128,
+		.offset = 228,
+		.width = 128,
+	},
+	[VCAP_KF_L3_IP6_SIP] = {
+		.type = VCAP_FIELD_U128,
+		.offset = 356,
+		.width = 128,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 484,
+		.width = 1,
+	},
+	[VCAP_KF_TCP_UDP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 485,
+		.width = 1,
+	},
+	[VCAP_KF_TCP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 486,
+		.width = 1,
+	},
+	[VCAP_KF_L4_DPORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 487,
+		.width = 16,
+	},
+	[VCAP_KF_L4_SPORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 503,
+		.width = 16,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 519,
+		.width = 16,
+	},
+	[VCAP_KF_L4_SPORT_EQ_DPORT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 535,
+		.width = 1,
+	},
+	[VCAP_KF_L4_SEQUENCE_EQ0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 536,
+		.width = 1,
+	},
+	[VCAP_KF_L4_FIN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 537,
+		.width = 1,
+	},
+	[VCAP_KF_L4_SYN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 538,
+		.width = 1,
+	},
+	[VCAP_KF_L4_RST] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 539,
+		.width = 1,
+	},
+	[VCAP_KF_L4_PSH] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 540,
+		.width = 1,
+	},
+	[VCAP_KF_L4_ACK] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 541,
+		.width = 1,
+	},
+	[VCAP_KF_L4_URG] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 542,
+		.width = 1,
+	},
+	[VCAP_KF_L4_PAYLOAD] = {
+		.type = VCAP_FIELD_U64,
+		.offset = 543,
+		.width = 64,
+	},
+};
+
+static const struct vcap_field es0_isdx_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 0,
+		.width = 1,
+	},
+	[VCAP_KF_IF_EGR_PORT_NO] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 1,
+		.width = 6,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 7,
+		.width = 13,
+	},
+	[VCAP_KF_COSID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 20,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_TPID] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 23,
+		.width = 3,
+	},
+	[VCAP_KF_L3_DPL_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 26,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 27,
+		.width = 1,
+	},
+	[VCAP_KF_PROT_ACTIVE] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 28,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 38,
+		.width = 10,
+	},
+};
+
+static const struct vcap_field es2_mac_etype_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 3,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 3,
+		.width = 1,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 14,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 15,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 16,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 26,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 28,
+		.width = 13,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 41,
+		.width = 3,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 44,
+		.width = 32,
+	},
+	[VCAP_KF_IF_IGR_PORT_SEL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 76,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 77,
+		.width = 7,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 84,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_COSID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 88,
+		.width = 3,
+	},
+	[VCAP_KF_L3_DPL_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 91,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 92,
+		.width = 1,
+	},
+	[VCAP_KF_L2_DMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 96,
+		.width = 48,
+	},
+	[VCAP_KF_L2_SMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 144,
+		.width = 48,
+	},
+	[VCAP_KF_ETYPE_LEN_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 192,
+		.width = 1,
+	},
+	[VCAP_KF_ETYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 193,
+		.width = 16,
+	},
+	[VCAP_KF_L2_PAYLOAD_ETYPE] = {
+		.type = VCAP_FIELD_U64,
+		.offset = 209,
+		.width = 64,
+	},
+	[VCAP_KF_OAM_CCM_CNTS_EQ0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 273,
+		.width = 1,
+	},
+	[VCAP_KF_OAM_Y1731_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 274,
+		.width = 1,
+	},
+};
+
+static const struct vcap_field es2_arp_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 3,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 3,
+		.width = 1,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 14,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 15,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 16,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 26,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 28,
+		.width = 13,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 41,
+		.width = 3,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 44,
+		.width = 32,
+	},
+	[VCAP_KF_IF_IGR_PORT_SEL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 76,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 77,
+		.width = 7,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 84,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_COSID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 88,
+		.width = 3,
+	},
+	[VCAP_KF_L3_DPL_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 91,
+		.width = 1,
+	},
+	[VCAP_KF_L2_SMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 95,
+		.width = 48,
+	},
+	[VCAP_KF_ARP_ADDR_SPACE_OK_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 143,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_PROTO_SPACE_OK_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 144,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_LEN_OK_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 145,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_TGT_MATCH_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 146,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_SENDER_MATCH_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 147,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_OPCODE_UNKNOWN_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 148,
+		.width = 1,
+	},
+	[VCAP_KF_ARP_OPCODE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 149,
+		.width = 2,
+	},
+	[VCAP_KF_L3_IP4_DIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 151,
+		.width = 32,
+	},
+	[VCAP_KF_L3_IP4_SIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 183,
+		.width = 32,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 215,
+		.width = 1,
+	},
+};
+
+static const struct vcap_field es2_ip4_tcp_udp_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 3,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 3,
+		.width = 1,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 14,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 15,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 16,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 26,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 28,
+		.width = 13,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 41,
+		.width = 3,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 44,
+		.width = 32,
+	},
+	[VCAP_KF_IF_IGR_PORT_SEL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 76,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 77,
+		.width = 7,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 84,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_COSID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 88,
+		.width = 3,
+	},
+	[VCAP_KF_L3_DPL_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 91,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 92,
+		.width = 1,
+	},
+	[VCAP_KF_IP4_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 96,
+		.width = 1,
+	},
+	[VCAP_KF_L3_FRAGMENT_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 97,
+		.width = 2,
+	},
+	[VCAP_KF_L3_OPTIONS_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 99,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TTL_GT0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 100,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TOS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 101,
+		.width = 8,
+	},
+	[VCAP_KF_L3_IP4_DIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 109,
+		.width = 32,
+	},
+	[VCAP_KF_L3_IP4_SIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 141,
+		.width = 32,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 173,
+		.width = 1,
+	},
+	[VCAP_KF_TCP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 174,
+		.width = 1,
+	},
+	[VCAP_KF_L4_DPORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 175,
+		.width = 16,
+	},
+	[VCAP_KF_L4_SPORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 191,
+		.width = 16,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 207,
+		.width = 16,
+	},
+	[VCAP_KF_L4_SPORT_EQ_DPORT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 223,
+		.width = 1,
+	},
+	[VCAP_KF_L4_SEQUENCE_EQ0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 224,
+		.width = 1,
+	},
+	[VCAP_KF_L4_FIN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 225,
+		.width = 1,
+	},
+	[VCAP_KF_L4_SYN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 226,
+		.width = 1,
+	},
+	[VCAP_KF_L4_RST] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 227,
+		.width = 1,
+	},
+	[VCAP_KF_L4_PSH] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 228,
+		.width = 1,
+	},
+	[VCAP_KF_L4_ACK] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 229,
+		.width = 1,
+	},
+	[VCAP_KF_L4_URG] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 230,
+		.width = 1,
+	},
+	[VCAP_KF_L4_PAYLOAD] = {
+		.type = VCAP_FIELD_U64,
+		.offset = 231,
+		.width = 64,
+	},
+};
+
+static const struct vcap_field es2_ip4_other_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 3,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 3,
+		.width = 1,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 14,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 15,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 16,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 26,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 28,
+		.width = 13,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 41,
+		.width = 3,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 44,
+		.width = 32,
+	},
+	[VCAP_KF_IF_IGR_PORT_SEL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 76,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 77,
+		.width = 7,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 84,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_COSID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 88,
+		.width = 3,
+	},
+	[VCAP_KF_L3_DPL_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 91,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 92,
+		.width = 1,
+	},
+	[VCAP_KF_IP4_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 96,
+		.width = 1,
+	},
+	[VCAP_KF_L3_FRAGMENT_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 97,
+		.width = 2,
+	},
+	[VCAP_KF_L3_OPTIONS_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 99,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TTL_GT0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 100,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TOS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 101,
+		.width = 8,
+	},
+	[VCAP_KF_L3_IP4_DIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 109,
+		.width = 32,
+	},
+	[VCAP_KF_L3_IP4_SIP] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 141,
+		.width = 32,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 173,
+		.width = 1,
+	},
+	[VCAP_KF_L3_IP_PROTO] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 174,
+		.width = 8,
+	},
+	[VCAP_KF_L3_PAYLOAD] = {
+		.type = VCAP_FIELD_U112,
+		.offset = 182,
+		.width = 96,
+	},
+};
+
+static const struct vcap_field es2_ip_7tuple_keyfield[] = {
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 0,
+		.width = 1,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 10,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 11,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 12,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 13,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 23,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 25,
+		.width = 13,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 38,
+		.width = 3,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 41,
+		.width = 32,
+	},
+	[VCAP_KF_IF_IGR_PORT_SEL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 73,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 74,
+		.width = 7,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 81,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 84,
+		.width = 1,
+	},
+	[VCAP_KF_COSID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 85,
+		.width = 3,
+	},
+	[VCAP_KF_L3_DPL_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 88,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 89,
+		.width = 1,
+	},
+	[VCAP_KF_L2_DMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 93,
+		.width = 48,
+	},
+	[VCAP_KF_L2_SMAC] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 141,
+		.width = 48,
+	},
+	[VCAP_KF_IP4_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 191,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TTL_GT0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 192,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TOS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 193,
+		.width = 8,
+	},
+	[VCAP_KF_L3_IP6_DIP] = {
+		.type = VCAP_FIELD_U128,
+		.offset = 201,
+		.width = 128,
+	},
+	[VCAP_KF_L3_IP6_SIP] = {
+		.type = VCAP_FIELD_U128,
+		.offset = 329,
+		.width = 128,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 457,
+		.width = 1,
+	},
+	[VCAP_KF_TCP_UDP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 458,
+		.width = 1,
+	},
+	[VCAP_KF_TCP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 459,
+		.width = 1,
+	},
+	[VCAP_KF_L4_DPORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 460,
+		.width = 16,
+	},
+	[VCAP_KF_L4_SPORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 476,
+		.width = 16,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 492,
+		.width = 16,
+	},
+	[VCAP_KF_L4_SPORT_EQ_DPORT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 508,
+		.width = 1,
+	},
+	[VCAP_KF_L4_SEQUENCE_EQ0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 509,
+		.width = 1,
+	},
+	[VCAP_KF_L4_FIN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 510,
+		.width = 1,
+	},
+	[VCAP_KF_L4_SYN] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 511,
+		.width = 1,
+	},
+	[VCAP_KF_L4_RST] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 512,
+		.width = 1,
+	},
+	[VCAP_KF_L4_PSH] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 513,
+		.width = 1,
+	},
+	[VCAP_KF_L4_ACK] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 514,
+		.width = 1,
+	},
+	[VCAP_KF_L4_URG] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 515,
+		.width = 1,
+	},
+	[VCAP_KF_L4_PAYLOAD] = {
+		.type = VCAP_FIELD_U64,
+		.offset = 516,
+		.width = 64,
+	},
+};
+
+static const struct vcap_field es2_ip6_std_keyfield[] = {
+	[VCAP_KF_TYPE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 3,
+	},
+	[VCAP_KF_LOOKUP_FIRST_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 3,
+		.width = 1,
+	},
+	[VCAP_KF_L2_MC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 13,
+		.width = 1,
+	},
+	[VCAP_KF_L2_BC_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 14,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_GT0_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 15,
+		.width = 1,
+	},
+	[VCAP_KF_ISDX_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 16,
+		.width = 10,
+	},
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 26,
+		.width = 1,
+	},
+	[VCAP_KF_8021Q_VID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 28,
+		.width = 13,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 41,
+		.width = 3,
+	},
+	[VCAP_KF_IF_EGR_PORT_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 44,
+		.width = 32,
+	},
+	[VCAP_KF_IF_IGR_PORT_SEL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 76,
+		.width = 1,
+	},
+	[VCAP_KF_IF_IGR_PORT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 77,
+		.width = 7,
+	},
+	[VCAP_KF_8021Q_PCP_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 84,
+		.width = 3,
+	},
+	[VCAP_KF_8021Q_DEI_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 87,
+		.width = 1,
+	},
+	[VCAP_KF_COSID_CLS] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 88,
+		.width = 3,
+	},
+	[VCAP_KF_L3_DPL_CLS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 91,
+		.width = 1,
+	},
+	[VCAP_KF_L3_RT_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 92,
+		.width = 1,
+	},
+	[VCAP_KF_L3_TTL_GT0] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 96,
+		.width = 1,
+	},
+	[VCAP_KF_L3_IP6_SIP] = {
+		.type = VCAP_FIELD_U128,
+		.offset = 97,
+		.width = 128,
+	},
+	[VCAP_KF_L3_DIP_EQ_SIP_IS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 225,
+		.width = 1,
+	},
+	[VCAP_KF_L3_IP_PROTO] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 226,
+		.width = 8,
+	},
+	[VCAP_KF_L4_RNG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 234,
+		.width = 16,
+	},
+	[VCAP_KF_L3_PAYLOAD] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 250,
+		.width = 40,
+	},
+};
+
+/* keyfield_set */
+static const struct vcap_set is0_keyfield_set[] = {
+	[VCAP_KFS_NORMAL_7TUPLE] = {
+		.type_id = 0,
+		.sw_per_item = 12,
+		.sw_cnt = 1,
+	},
+	[VCAP_KFS_NORMAL_5TUPLE_IP4] = {
+		.type_id = 2,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+};
+
+static const struct vcap_set is2_keyfield_set[] = {
+	[VCAP_KFS_MAC_ETYPE] = {
+		.type_id = 0,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+	[VCAP_KFS_ARP] = {
+		.type_id = 3,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+	[VCAP_KFS_IP4_TCP_UDP] = {
+		.type_id = 4,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+	[VCAP_KFS_IP4_OTHER] = {
+		.type_id = 5,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+	[VCAP_KFS_IP6_STD] = {
+		.type_id = 6,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+	[VCAP_KFS_IP_7TUPLE] = {
+		.type_id = 1,
+		.sw_per_item = 12,
+		.sw_cnt = 1,
+	},
+};
+
+static const struct vcap_set es0_keyfield_set[] = {
+	[VCAP_KFS_ISDX] = {
+		.type_id = 0,
+		.sw_per_item = 1,
+		.sw_cnt = 1,
+	},
+};
+
+static const struct vcap_set es2_keyfield_set[] = {
+	[VCAP_KFS_MAC_ETYPE] = {
+		.type_id = 0,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+	[VCAP_KFS_ARP] = {
+		.type_id = 1,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+	[VCAP_KFS_IP4_TCP_UDP] = {
+		.type_id = 2,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+	[VCAP_KFS_IP4_OTHER] = {
+		.type_id = 3,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+	[VCAP_KFS_IP_7TUPLE] = {
+		.type_id = -1,
+		.sw_per_item = 12,
+		.sw_cnt = 1,
+	},
+	[VCAP_KFS_IP6_STD] = {
+		.type_id = 4,
+		.sw_per_item = 6,
+		.sw_cnt = 2,
+	},
+};
+
+/* keyfield_set map */
+static const struct vcap_field *is0_keyfield_set_map[] = {
+	[VCAP_KFS_NORMAL_7TUPLE] = is0_normal_7tuple_keyfield,
+	[VCAP_KFS_NORMAL_5TUPLE_IP4] = is0_normal_5tuple_ip4_keyfield,
+};
+
+static const struct vcap_field *is2_keyfield_set_map[] = {
+	[VCAP_KFS_MAC_ETYPE] = is2_mac_etype_keyfield,
+	[VCAP_KFS_ARP] = is2_arp_keyfield,
+	[VCAP_KFS_IP4_TCP_UDP] = is2_ip4_tcp_udp_keyfield,
+	[VCAP_KFS_IP4_OTHER] = is2_ip4_other_keyfield,
+	[VCAP_KFS_IP6_STD] = is2_ip6_std_keyfield,
+	[VCAP_KFS_IP_7TUPLE] = is2_ip_7tuple_keyfield,
+};
+
+static const struct vcap_field *es0_keyfield_set_map[] = {
+	[VCAP_KFS_ISDX] = es0_isdx_keyfield,
+};
+
+static const struct vcap_field *es2_keyfield_set_map[] = {
+	[VCAP_KFS_MAC_ETYPE] = es2_mac_etype_keyfield,
+	[VCAP_KFS_ARP] = es2_arp_keyfield,
+	[VCAP_KFS_IP4_TCP_UDP] = es2_ip4_tcp_udp_keyfield,
+	[VCAP_KFS_IP4_OTHER] = es2_ip4_other_keyfield,
+	[VCAP_KFS_IP_7TUPLE] = es2_ip_7tuple_keyfield,
+	[VCAP_KFS_IP6_STD] = es2_ip6_std_keyfield,
+};
+
+/* keyfield_set map sizes */
+static int is0_keyfield_set_map_size[] = {
+	[VCAP_KFS_NORMAL_7TUPLE] = ARRAY_SIZE(is0_normal_7tuple_keyfield),
+	[VCAP_KFS_NORMAL_5TUPLE_IP4] = ARRAY_SIZE(is0_normal_5tuple_ip4_keyfield),
+};
+
+static int is2_keyfield_set_map_size[] = {
+	[VCAP_KFS_MAC_ETYPE] = ARRAY_SIZE(is2_mac_etype_keyfield),
+	[VCAP_KFS_ARP] = ARRAY_SIZE(is2_arp_keyfield),
+	[VCAP_KFS_IP4_TCP_UDP] = ARRAY_SIZE(is2_ip4_tcp_udp_keyfield),
+	[VCAP_KFS_IP4_OTHER] = ARRAY_SIZE(is2_ip4_other_keyfield),
+	[VCAP_KFS_IP6_STD] = ARRAY_SIZE(is2_ip6_std_keyfield),
+	[VCAP_KFS_IP_7TUPLE] = ARRAY_SIZE(is2_ip_7tuple_keyfield),
+};
+
+static int es0_keyfield_set_map_size[] = {
+	[VCAP_KFS_ISDX] = ARRAY_SIZE(es0_isdx_keyfield),
+};
+
+static int es2_keyfield_set_map_size[] = {
+	[VCAP_KFS_MAC_ETYPE] = ARRAY_SIZE(es2_mac_etype_keyfield),
+	[VCAP_KFS_ARP] = ARRAY_SIZE(es2_arp_keyfield),
+	[VCAP_KFS_IP4_TCP_UDP] = ARRAY_SIZE(es2_ip4_tcp_udp_keyfield),
+	[VCAP_KFS_IP4_OTHER] = ARRAY_SIZE(es2_ip4_other_keyfield),
+	[VCAP_KFS_IP_7TUPLE] = ARRAY_SIZE(es2_ip_7tuple_keyfield),
+	[VCAP_KFS_IP6_STD] = ARRAY_SIZE(es2_ip6_std_keyfield),
+};
+
+/* actionfields */
+static const struct vcap_field is0_classification_actionfield[] = {
+	[VCAP_AF_TYPE] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 0,
+		.width = 1,
+	},
+	[VCAP_AF_DSCP_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 1,
+		.width = 1,
+	},
+	[VCAP_AF_DSCP_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 2,
+		.width = 6,
+	},
+	[VCAP_AF_QOS_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 12,
+		.width = 1,
+	},
+	[VCAP_AF_QOS_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 13,
+		.width = 3,
+	},
+	[VCAP_AF_DP_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 16,
+		.width = 1,
+	},
+	[VCAP_AF_DP_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 17,
+		.width = 2,
+	},
+	[VCAP_AF_DEI_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 19,
+		.width = 1,
+	},
+	[VCAP_AF_DEI_VAL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 20,
+		.width = 1,
+	},
+	[VCAP_AF_PCP_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 21,
+		.width = 1,
+	},
+	[VCAP_AF_PCP_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 22,
+		.width = 3,
+	},
+	[VCAP_AF_MAP_LOOKUP_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 25,
+		.width = 2,
+	},
+	[VCAP_AF_MAP_KEY] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 27,
+		.width = 3,
+	},
+	[VCAP_AF_MAP_IDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 30,
+		.width = 7,
+	},
+	[VCAP_AF_CLS_VID_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 37,
+		.width = 3,
+	},
+	[VCAP_AF_VID_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 43,
+		.width = 13,
+	},
+	[VCAP_AF_ISDX_ADD_REPLACE_SEL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 66,
+		.width = 1,
+	},
+	[VCAP_AF_ISDX_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 67,
+		.width = 10,
+	},
+	[VCAP_AF_PAG_OVERRIDE_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 107,
+		.width = 8,
+	},
+	[VCAP_AF_PAG_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 115,
+		.width = 8,
+	},
+	[VCAP_AF_NXT_IDX_CTRL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 167,
+		.width = 3,
+	},
+	[VCAP_AF_NXT_IDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 170,
+		.width = 10,
+	},
+};
+
+static const struct vcap_field is0_full_actionfield[] = {
+	[VCAP_AF_DSCP_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 0,
+		.width = 1,
+	},
+	[VCAP_AF_DSCP_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 1,
+		.width = 6,
+	},
+	[VCAP_AF_QOS_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 11,
+		.width = 1,
+	},
+	[VCAP_AF_QOS_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 12,
+		.width = 3,
+	},
+	[VCAP_AF_DP_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 15,
+		.width = 1,
+	},
+	[VCAP_AF_DP_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 16,
+		.width = 2,
+	},
+	[VCAP_AF_DEI_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 18,
+		.width = 1,
+	},
+	[VCAP_AF_DEI_VAL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 19,
+		.width = 1,
+	},
+	[VCAP_AF_PCP_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 20,
+		.width = 1,
+	},
+	[VCAP_AF_PCP_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 21,
+		.width = 3,
+	},
+	[VCAP_AF_MAP_LOOKUP_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 24,
+		.width = 2,
+	},
+	[VCAP_AF_MAP_KEY] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 26,
+		.width = 3,
+	},
+	[VCAP_AF_MAP_IDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 29,
+		.width = 7,
+	},
+	[VCAP_AF_CLS_VID_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 36,
+		.width = 3,
+	},
+	[VCAP_AF_VID_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 42,
+		.width = 13,
+	},
+	[VCAP_AF_ISDX_ADD_REPLACE_SEL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 65,
+		.width = 1,
+	},
+	[VCAP_AF_ISDX_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 66,
+		.width = 10,
+	},
+	[VCAP_AF_MASK_MODE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 76,
+		.width = 3,
+	},
+	[VCAP_AF_PORT_MASK] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 79,
+		.width = 37,
+	},
+	[VCAP_AF_PAG_OVERRIDE_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 174,
+		.width = 8,
+	},
+	[VCAP_AF_PAG_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 182,
+		.width = 8,
+	},
+	[VCAP_AF_NXT_IDX_CTRL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 266,
+		.width = 3,
+	},
+	[VCAP_AF_NXT_IDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 269,
+		.width = 10,
+	},
+};
+
+static const struct vcap_field is0_class_reduced_actionfield[] = {
+	[VCAP_AF_TYPE] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 0,
+		.width = 1,
+	},
+	[VCAP_AF_QOS_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 5,
+		.width = 1,
+	},
+	[VCAP_AF_QOS_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 6,
+		.width = 3,
+	},
+	[VCAP_AF_DP_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 9,
+		.width = 1,
+	},
+	[VCAP_AF_DP_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 10,
+		.width = 2,
+	},
+	[VCAP_AF_MAP_LOOKUP_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 12,
+		.width = 2,
+	},
+	[VCAP_AF_MAP_KEY] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 14,
+		.width = 3,
+	},
+	[VCAP_AF_CLS_VID_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 17,
+		.width = 3,
+	},
+	[VCAP_AF_VID_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 23,
+		.width = 13,
+	},
+	[VCAP_AF_ISDX_ADD_REPLACE_SEL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 46,
+		.width = 1,
+	},
+	[VCAP_AF_ISDX_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 47,
+		.width = 10,
+	},
+	[VCAP_AF_NXT_IDX_CTRL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 89,
+		.width = 3,
+	},
+	[VCAP_AF_NXT_IDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 92,
+		.width = 10,
+	},
+};
+
+static const struct vcap_field is2_base_type_actionfield[] = {
+	[VCAP_AF_PIPELINE_FORCE_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 1,
+		.width = 1,
+	},
+	[VCAP_AF_PIPELINE_PT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 2,
+		.width = 5,
+	},
+	[VCAP_AF_HIT_ME_ONCE] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 7,
+		.width = 1,
+	},
+	[VCAP_AF_INTR_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 8,
+		.width = 1,
+	},
+	[VCAP_AF_CPU_COPY_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 9,
+		.width = 1,
+	},
+	[VCAP_AF_CPU_QUEUE_NUM] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 10,
+		.width = 3,
+	},
+	[VCAP_AF_LRN_DIS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 15,
+		.width = 1,
+	},
+	[VCAP_AF_RT_DIS] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 16,
+		.width = 1,
+	},
+	[VCAP_AF_POLICE_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 17,
+		.width = 1,
+	},
+	[VCAP_AF_POLICE_IDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 18,
+		.width = 5,
+	},
+	[VCAP_AF_IGNORE_PIPELINE_CTRL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 23,
+		.width = 1,
+	},
+	[VCAP_AF_MASK_MODE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 27,
+		.width = 3,
+	},
+	[VCAP_AF_PORT_MASK] = {
+		.type = VCAP_FIELD_U48,
+		.offset = 30,
+		.width = 37,
+	},
+	[VCAP_AF_MIRROR_PROBE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 78,
+		.width = 2,
+	},
+	[VCAP_AF_MATCH_ID] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 131,
+		.width = 16,
+	},
+	[VCAP_AF_MATCH_ID_MASK] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 147,
+		.width = 16,
+	},
+	[VCAP_AF_CNT_ID] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 163,
+		.width = 10,
+	},
+};
+
+static const struct vcap_field es0_es0_actionfield[] = {
+	[VCAP_AF_PUSH_OUTER_TAG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 0,
+		.width = 2,
+	},
+	[VCAP_AF_PUSH_INNER_TAG] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 2,
+		.width = 1,
+	},
+	[VCAP_AF_TAG_A_TPID_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 3,
+		.width = 3,
+	},
+	[VCAP_AF_TAG_A_VID_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 6,
+		.width = 2,
+	},
+	[VCAP_AF_TAG_A_PCP_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 8,
+		.width = 3,
+	},
+	[VCAP_AF_TAG_A_DEI_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 11,
+		.width = 3,
+	},
+	[VCAP_AF_TAG_B_TPID_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 14,
+		.width = 3,
+	},
+	[VCAP_AF_TAG_B_VID_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 17,
+		.width = 2,
+	},
+	[VCAP_AF_TAG_B_PCP_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 19,
+		.width = 3,
+	},
+	[VCAP_AF_TAG_B_DEI_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 22,
+		.width = 3,
+	},
+	[VCAP_AF_TAG_C_TPID_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 25,
+		.width = 3,
+	},
+	[VCAP_AF_TAG_C_PCP_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 28,
+		.width = 3,
+	},
+	[VCAP_AF_TAG_C_DEI_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 31,
+		.width = 3,
+	},
+	[VCAP_AF_VID_A_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 34,
+		.width = 12,
+	},
+	[VCAP_AF_PCP_A_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 46,
+		.width = 3,
+	},
+	[VCAP_AF_DEI_A_VAL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 49,
+		.width = 1,
+	},
+	[VCAP_AF_VID_B_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 50,
+		.width = 12,
+	},
+	[VCAP_AF_PCP_B_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 62,
+		.width = 3,
+	},
+	[VCAP_AF_DEI_B_VAL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 65,
+		.width = 1,
+	},
+	[VCAP_AF_VID_C_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 66,
+		.width = 12,
+	},
+	[VCAP_AF_PCP_C_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 78,
+		.width = 3,
+	},
+	[VCAP_AF_DEI_C_VAL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 81,
+		.width = 1,
+	},
+	[VCAP_AF_POP_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 82,
+		.width = 2,
+	},
+	[VCAP_AF_UNTAG_VID_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 84,
+		.width = 1,
+	},
+	[VCAP_AF_PUSH_CUSTOMER_TAG] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 85,
+		.width = 2,
+	},
+	[VCAP_AF_TAG_C_VID_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 87,
+		.width = 2,
+	},
+	[VCAP_AF_DSCP_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 127,
+		.width = 3,
+	},
+	[VCAP_AF_DSCP_VAL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 130,
+		.width = 6,
+	},
+	[VCAP_AF_ESDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 319,
+		.width = 10,
+	},
+	[VCAP_AF_FWD_SEL] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 438,
+		.width = 2,
+	},
+	[VCAP_AF_CPU_QU] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 440,
+		.width = 3,
+	},
+	[VCAP_AF_PIPELINE_PT] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 443,
+		.width = 2,
+	},
+	[VCAP_AF_PIPELINE_ACT] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 445,
+		.width = 1,
+	},
+	[VCAP_AF_SWAP_MACS_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 454,
+		.width = 1,
+	},
+	[VCAP_AF_LOOP_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 455,
+		.width = 1,
+	},
+};
+
+static const struct vcap_field es2_base_type_actionfield[] = {
+	[VCAP_AF_HIT_ME_ONCE] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 0,
+		.width = 1,
+	},
+	[VCAP_AF_INTR_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 1,
+		.width = 1,
+	},
+	[VCAP_AF_FWD_MODE] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 2,
+		.width = 2,
+	},
+	[VCAP_AF_COPY_QUEUE_NUM] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 4,
+		.width = 14,
+	},
+	[VCAP_AF_COPY_PORT_NUM] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 18,
+		.width = 6,
+	},
+	[VCAP_AF_MIRROR_PROBE_ID] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 24,
+		.width = 2,
+	},
+	[VCAP_AF_CPU_COPY_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 26,
+		.width = 1,
+	},
+	[VCAP_AF_CPU_QUEUE_NUM] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 27,
+		.width = 3,
+	},
+	[VCAP_AF_POLICE_ENA] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 30,
+		.width = 1,
+	},
+	[VCAP_AF_POLICE_REMARK] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 31,
+		.width = 1,
+	},
+	[VCAP_AF_POLICE_IDX] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 32,
+		.width = 5,
+	},
+	[VCAP_AF_ES2_REW_CMD] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 37,
+		.width = 3,
+	},
+	[VCAP_AF_CNT_ID] = {
+		.type = VCAP_FIELD_U32,
+		.offset = 40,
+		.width = 9,
+	},
+	[VCAP_AF_IGNORE_PIPELINE_CTRL] = {
+		.type = VCAP_FIELD_BIT,
+		.offset = 49,
+		.width = 1,
+	},
+};
+
+/* actionfield_set */
+static const struct vcap_set is0_actionfield_set[] = {
+	[VCAP_AFS_CLASSIFICATION] = {
+		.type_id = 1,
+		.sw_per_item = 2,
+		.sw_cnt = 6,
+	},
+	[VCAP_AFS_FULL] = {
+		.type_id = -1,
+		.sw_per_item = 3,
+		.sw_cnt = 4,
+	},
+	[VCAP_AFS_CLASS_REDUCED] = {
+		.type_id = 1,
+		.sw_per_item = 1,
+		.sw_cnt = 12,
+	},
+};
+
+static const struct vcap_set is2_actionfield_set[] = {
+	[VCAP_AFS_BASE_TYPE] = {
+		.type_id = -1,
+		.sw_per_item = 3,
+		.sw_cnt = 4,
+	},
+};
+
+static const struct vcap_set es0_actionfield_set[] = {
+	[VCAP_AFS_ES0] = {
+		.type_id = -1,
+		.sw_per_item = 1,
+		.sw_cnt = 1,
+	},
+};
+
+static const struct vcap_set es2_actionfield_set[] = {
+	[VCAP_AFS_BASE_TYPE] = {
+		.type_id = -1,
+		.sw_per_item = 3,
+		.sw_cnt = 4,
+	},
+};
+
+/* actionfield_set map */
+static const struct vcap_field *is0_actionfield_set_map[] = {
+	[VCAP_AFS_CLASSIFICATION] = is0_classification_actionfield,
+	[VCAP_AFS_FULL] = is0_full_actionfield,
+	[VCAP_AFS_CLASS_REDUCED] = is0_class_reduced_actionfield,
+};
+
+static const struct vcap_field *is2_actionfield_set_map[] = {
+	[VCAP_AFS_BASE_TYPE] = is2_base_type_actionfield,
+};
+
+static const struct vcap_field *es0_actionfield_set_map[] = {
+	[VCAP_AFS_ES0] = es0_es0_actionfield,
+};
+
+static const struct vcap_field *es2_actionfield_set_map[] = {
+	[VCAP_AFS_BASE_TYPE] = es2_base_type_actionfield,
+};
+
+/* actionfield_set map size */
+static int is0_actionfield_set_map_size[] = {
+	[VCAP_AFS_CLASSIFICATION] = ARRAY_SIZE(is0_classification_actionfield),
+	[VCAP_AFS_FULL] = ARRAY_SIZE(is0_full_actionfield),
+	[VCAP_AFS_CLASS_REDUCED] = ARRAY_SIZE(is0_class_reduced_actionfield),
+};
+
+static int is2_actionfield_set_map_size[] = {
+	[VCAP_AFS_BASE_TYPE] = ARRAY_SIZE(is2_base_type_actionfield),
+};
+
+static int es0_actionfield_set_map_size[] = {
+	[VCAP_AFS_ES0] = ARRAY_SIZE(es0_es0_actionfield),
+};
+
+static int es2_actionfield_set_map_size[] = {
+	[VCAP_AFS_BASE_TYPE] = ARRAY_SIZE(es2_base_type_actionfield),
+};
+
+/* Type Groups */
+static const struct vcap_typegroup is0_x12_keyfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 5,
+		.value = 16,
+	},
+	{
+		.offset = 52,
+		.width = 1,
+		.value = 0,
+	},
+	{
+		.offset = 104,
+		.width = 2,
+		.value = 0,
+	},
+	{
+		.offset = 156,
+		.width = 3,
+		.value = 0,
+	},
+	{
+		.offset = 208,
+		.width = 2,
+		.value = 0,
+	},
+	{
+		.offset = 260,
+		.width = 1,
+		.value = 0,
+	},
+	{
+		.offset = 312,
+		.width = 4,
+		.value = 0,
+	},
+	{
+		.offset = 364,
+		.width = 1,
+		.value = 0,
+	},
+	{
+		.offset = 416,
+		.width = 2,
+		.value = 0,
+	},
+	{
+		.offset = 468,
+		.width = 3,
+		.value = 0,
+	},
+	{
+		.offset = 520,
+		.width = 2,
+		.value = 0,
+	},
+	{
+		.offset = 572,
+		.width = 1,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup is0_x6_keyfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 4,
+		.value = 8,
+	},
+	{
+		.offset = 52,
+		.width = 1,
+		.value = 0,
+	},
+	{
+		.offset = 104,
+		.width = 2,
+		.value = 0,
+	},
+	{
+		.offset = 156,
+		.width = 3,
+		.value = 0,
+	},
+	{
+		.offset = 208,
+		.width = 2,
+		.value = 0,
+	},
+	{
+		.offset = 260,
+		.width = 1,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup is0_x3_keyfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup is0_x2_keyfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup is0_x1_keyfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup is2_x12_keyfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 3,
+		.value = 4,
+	},
+	{
+		.offset = 156,
+		.width = 1,
+		.value = 0,
+	},
+	{
+		.offset = 312,
+		.width = 2,
+		.value = 0,
+	},
+	{
+		.offset = 468,
+		.width = 1,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup is2_x6_keyfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 2,
+		.value = 2,
+	},
+	{
+		.offset = 156,
+		.width = 1,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup is2_x3_keyfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup is2_x1_keyfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup es0_x1_keyfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup es2_x12_keyfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 3,
+		.value = 4,
+	},
+	{
+		.offset = 156,
+		.width = 1,
+		.value = 0,
+	},
+	{
+		.offset = 312,
+		.width = 2,
+		.value = 0,
+	},
+	{
+		.offset = 468,
+		.width = 1,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup es2_x6_keyfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 2,
+		.value = 2,
+	},
+	{
+		.offset = 156,
+		.width = 1,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup es2_x3_keyfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup es2_x1_keyfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup *is0_keyfield_set_typegroups[] = {
+	[12] = is0_x12_keyfield_set_typegroups,
+	[6] = is0_x6_keyfield_set_typegroups,
+	[3] = is0_x3_keyfield_set_typegroups,
+	[2] = is0_x2_keyfield_set_typegroups,
+	[1] = is0_x1_keyfield_set_typegroups,
+	[13] = NULL,
+};
+
+static const struct vcap_typegroup *is2_keyfield_set_typegroups[] = {
+	[12] = is2_x12_keyfield_set_typegroups,
+	[6] = is2_x6_keyfield_set_typegroups,
+	[3] = is2_x3_keyfield_set_typegroups,
+	[1] = is2_x1_keyfield_set_typegroups,
+	[13] = NULL,
+};
+
+static const struct vcap_typegroup *es0_keyfield_set_typegroups[] = {
+	[1] = es0_x1_keyfield_set_typegroups,
+	[2] = NULL,
+};
+
+static const struct vcap_typegroup *es2_keyfield_set_typegroups[] = {
+	[12] = es2_x12_keyfield_set_typegroups,
+	[6] = es2_x6_keyfield_set_typegroups,
+	[3] = es2_x3_keyfield_set_typegroups,
+	[1] = es2_x1_keyfield_set_typegroups,
+	[13] = NULL,
+};
+
+static const struct vcap_typegroup is0_x3_actionfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 3,
+		.value = 4,
+	},
+	{
+		.offset = 103,
+		.width = 2,
+		.value = 0,
+	},
+	{
+		.offset = 206,
+		.width = 2,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup is0_x2_actionfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 2,
+		.value = 2,
+	},
+	{
+		.offset = 103,
+		.width = 1,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup is0_x1_actionfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 1,
+		.value = 1,
+	},
+	{}
+};
+
+static const struct vcap_typegroup is2_x3_actionfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 2,
+		.value = 2,
+	},
+	{
+		.offset = 95,
+		.width = 1,
+		.value = 0,
+	},
+	{
+		.offset = 190,
+		.width = 1,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup is2_x1_actionfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup es0_x1_actionfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup es2_x3_actionfield_set_typegroups[] = {
+	{
+		.offset = 0,
+		.width = 2,
+		.value = 2,
+	},
+	{
+		.offset = 19,
+		.width = 1,
+		.value = 0,
+	},
+	{
+		.offset = 38,
+		.width = 1,
+		.value = 0,
+	},
+	{}
+};
+
+static const struct vcap_typegroup es2_x1_actionfield_set_typegroups[] = {
+	{}
+};
+
+static const struct vcap_typegroup *is0_actionfield_set_typegroups[] = {
+	[3] = is0_x3_actionfield_set_typegroups,
+	[2] = is0_x2_actionfield_set_typegroups,
+	[1] = is0_x1_actionfield_set_typegroups,
+	[13] = NULL,
+};
+
+static const struct vcap_typegroup *is2_actionfield_set_typegroups[] = {
+	[3] = is2_x3_actionfield_set_typegroups,
+	[1] = is2_x1_actionfield_set_typegroups,
+	[13] = NULL,
+};
+
+static const struct vcap_typegroup *es0_actionfield_set_typegroups[] = {
+	[1] = es0_x1_actionfield_set_typegroups,
+	[2] = NULL,
+};
+
+static const struct vcap_typegroup *es2_actionfield_set_typegroups[] = {
+	[3] = es2_x3_actionfield_set_typegroups,
+	[1] = es2_x1_actionfield_set_typegroups,
+	[13] = NULL,
+};
+
+/* Keyfieldset names */
+static const char * const vcap_keyfield_set_names[] = {
+	[VCAP_KFS_NO_VALUE]                      =  "(None)",
+	[VCAP_KFS_ARP]                           =  "VCAP_KFS_ARP",
+	[VCAP_KFS_ETAG]                          =  "VCAP_KFS_ETAG",
+	[VCAP_KFS_IP4_OTHER]                     =  "VCAP_KFS_IP4_OTHER",
+	[VCAP_KFS_IP4_TCP_UDP]                   =  "VCAP_KFS_IP4_TCP_UDP",
+	[VCAP_KFS_IP4_VID]                       =  "VCAP_KFS_IP4_VID",
+	[VCAP_KFS_IP6_OTHER]                     =  "VCAP_KFS_IP6_OTHER",
+	[VCAP_KFS_IP6_STD]                       =  "VCAP_KFS_IP6_STD",
+	[VCAP_KFS_IP6_TCP_UDP]                   =  "VCAP_KFS_IP6_TCP_UDP",
+	[VCAP_KFS_IP6_VID]                       =  "VCAP_KFS_IP6_VID",
+	[VCAP_KFS_IP_7TUPLE]                     =  "VCAP_KFS_IP_7TUPLE",
+	[VCAP_KFS_ISDX]                          =  "VCAP_KFS_ISDX",
+	[VCAP_KFS_LL_FULL]                       =  "VCAP_KFS_LL_FULL",
+	[VCAP_KFS_MAC_ETYPE]                     =  "VCAP_KFS_MAC_ETYPE",
+	[VCAP_KFS_MAC_LLC]                       =  "VCAP_KFS_MAC_LLC",
+	[VCAP_KFS_MAC_SNAP]                      =  "VCAP_KFS_MAC_SNAP",
+	[VCAP_KFS_NORMAL_5TUPLE_IP4]             =  "VCAP_KFS_NORMAL_5TUPLE_IP4",
+	[VCAP_KFS_NORMAL_7TUPLE]                 =  "VCAP_KFS_NORMAL_7TUPLE",
+	[VCAP_KFS_OAM]                           =  "VCAP_KFS_OAM",
+	[VCAP_KFS_PURE_5TUPLE_IP4]               =  "VCAP_KFS_PURE_5TUPLE_IP4",
+	[VCAP_KFS_SMAC_SIP4]                     =  "VCAP_KFS_SMAC_SIP4",
+	[VCAP_KFS_SMAC_SIP6]                     =  "VCAP_KFS_SMAC_SIP6",
+};
+
+/* Actionfieldset names */
+static const char * const vcap_actionfield_set_names[] = {
+	[VCAP_AFS_NO_VALUE]                      =  "(None)",
+	[VCAP_AFS_BASE_TYPE]                     =  "VCAP_AFS_BASE_TYPE",
+	[VCAP_AFS_CLASSIFICATION]                =  "VCAP_AFS_CLASSIFICATION",
+	[VCAP_AFS_CLASS_REDUCED]                 =  "VCAP_AFS_CLASS_REDUCED",
+	[VCAP_AFS_ES0]                           =  "VCAP_AFS_ES0",
+	[VCAP_AFS_FULL]                          =  "VCAP_AFS_FULL",
+	[VCAP_AFS_SMAC_SIP]                      =  "VCAP_AFS_SMAC_SIP",
+};
+
+/* Keyfield names */
+static const char * const vcap_keyfield_names[] = {
+	[VCAP_KF_NO_VALUE]                       =  "(None)",
+	[VCAP_KF_8021BR_ECID_BASE]               =  "8021BR_ECID_BASE",
+	[VCAP_KF_8021BR_ECID_EXT]                =  "8021BR_ECID_EXT",
+	[VCAP_KF_8021BR_E_TAGGED]                =  "8021BR_E_TAGGED",
+	[VCAP_KF_8021BR_GRP]                     =  "8021BR_GRP",
+	[VCAP_KF_8021BR_IGR_ECID_BASE]           =  "8021BR_IGR_ECID_BASE",
+	[VCAP_KF_8021BR_IGR_ECID_EXT]            =  "8021BR_IGR_ECID_EXT",
+	[VCAP_KF_8021Q_DEI0]                     =  "8021Q_DEI0",
+	[VCAP_KF_8021Q_DEI1]                     =  "8021Q_DEI1",
+	[VCAP_KF_8021Q_DEI2]                     =  "8021Q_DEI2",
+	[VCAP_KF_8021Q_DEI_CLS]                  =  "8021Q_DEI_CLS",
+	[VCAP_KF_8021Q_PCP0]                     =  "8021Q_PCP0",
+	[VCAP_KF_8021Q_PCP1]                     =  "8021Q_PCP1",
+	[VCAP_KF_8021Q_PCP2]                     =  "8021Q_PCP2",
+	[VCAP_KF_8021Q_PCP_CLS]                  =  "8021Q_PCP_CLS",
+	[VCAP_KF_8021Q_TPID]                     =  "8021Q_TPID",
+	[VCAP_KF_8021Q_TPID0]                    =  "8021Q_TPID0",
+	[VCAP_KF_8021Q_TPID1]                    =  "8021Q_TPID1",
+	[VCAP_KF_8021Q_TPID2]                    =  "8021Q_TPID2",
+	[VCAP_KF_8021Q_VID0]                     =  "8021Q_VID0",
+	[VCAP_KF_8021Q_VID1]                     =  "8021Q_VID1",
+	[VCAP_KF_8021Q_VID2]                     =  "8021Q_VID2",
+	[VCAP_KF_8021Q_VID_CLS]                  =  "8021Q_VID_CLS",
+	[VCAP_KF_8021Q_VLAN_TAGGED_IS]           =  "8021Q_VLAN_TAGGED_IS",
+	[VCAP_KF_8021Q_VLAN_TAGS]                =  "8021Q_VLAN_TAGS",
+	[VCAP_KF_ACL_GRP_ID]                     =  "ACL_GRP_ID",
+	[VCAP_KF_ARP_ADDR_SPACE_OK_IS]           =  "ARP_ADDR_SPACE_OK_IS",
+	[VCAP_KF_ARP_LEN_OK_IS]                  =  "ARP_LEN_OK_IS",
+	[VCAP_KF_ARP_OPCODE]                     =  "ARP_OPCODE",
+	[VCAP_KF_ARP_OPCODE_UNKNOWN_IS]          =  "ARP_OPCODE_UNKNOWN_IS",
+	[VCAP_KF_ARP_PROTO_SPACE_OK_IS]          =  "ARP_PROTO_SPACE_OK_IS",
+	[VCAP_KF_ARP_SENDER_MATCH_IS]            =  "ARP_SENDER_MATCH_IS",
+	[VCAP_KF_ARP_TGT_MATCH_IS]               =  "ARP_TGT_MATCH_IS",
+	[VCAP_KF_COSID_CLS]                      =  "COSID_CLS",
+	[VCAP_KF_ES0_ISDX_KEY_ENA]               =  "ES0_ISDX_KEY_ENA",
+	[VCAP_KF_ETYPE]                          =  "ETYPE",
+	[VCAP_KF_ETYPE_LEN_IS]                   =  "ETYPE_LEN_IS",
+	[VCAP_KF_HOST_MATCH]                     =  "HOST_MATCH",
+	[VCAP_KF_IF_EGR_PORT_MASK]               =  "IF_EGR_PORT_MASK",
+	[VCAP_KF_IF_EGR_PORT_MASK_RNG]           =  "IF_EGR_PORT_MASK_RNG",
+	[VCAP_KF_IF_EGR_PORT_NO]                 =  "IF_EGR_PORT_NO",
+	[VCAP_KF_IF_IGR_PORT]                    =  "IF_IGR_PORT",
+	[VCAP_KF_IF_IGR_PORT_MASK]               =  "IF_IGR_PORT_MASK",
+	[VCAP_KF_IF_IGR_PORT_MASK_L3]            =  "IF_IGR_PORT_MASK_L3",
+	[VCAP_KF_IF_IGR_PORT_MASK_RNG]           =  "IF_IGR_PORT_MASK_RNG",
+	[VCAP_KF_IF_IGR_PORT_MASK_SEL]           =  "IF_IGR_PORT_MASK_SEL",
+	[VCAP_KF_IF_IGR_PORT_SEL]                =  "IF_IGR_PORT_SEL",
+	[VCAP_KF_IP4_IS]                         =  "IP4_IS",
+	[VCAP_KF_IP_MC_IS]                       =  "IP_MC_IS",
+	[VCAP_KF_IP_PAYLOAD_5TUPLE]              =  "IP_PAYLOAD_5TUPLE",
+	[VCAP_KF_IP_SNAP_IS]                     =  "IP_SNAP_IS",
+	[VCAP_KF_ISDX_CLS]                       =  "ISDX_CLS",
+	[VCAP_KF_ISDX_GT0_IS]                    =  "ISDX_GT0_IS",
+	[VCAP_KF_L2_BC_IS]                       =  "L2_BC_IS",
+	[VCAP_KF_L2_DMAC]                        =  "L2_DMAC",
+	[VCAP_KF_L2_FRM_TYPE]                    =  "L2_FRM_TYPE",
+	[VCAP_KF_L2_FWD_IS]                      =  "L2_FWD_IS",
+	[VCAP_KF_L2_LLC]                         =  "L2_LLC",
+	[VCAP_KF_L2_MC_IS]                       =  "L2_MC_IS",
+	[VCAP_KF_L2_PAYLOAD0]                    =  "L2_PAYLOAD0",
+	[VCAP_KF_L2_PAYLOAD1]                    =  "L2_PAYLOAD1",
+	[VCAP_KF_L2_PAYLOAD2]                    =  "L2_PAYLOAD2",
+	[VCAP_KF_L2_PAYLOAD_ETYPE]               =  "L2_PAYLOAD_ETYPE",
+	[VCAP_KF_L2_SMAC]                        =  "L2_SMAC",
+	[VCAP_KF_L2_SNAP]                        =  "L2_SNAP",
+	[VCAP_KF_L3_DIP_EQ_SIP_IS]               =  "L3_DIP_EQ_SIP_IS",
+	[VCAP_KF_L3_DPL_CLS]                     =  "L3_DPL_CLS",
+	[VCAP_KF_L3_DSCP]                        =  "L3_DSCP",
+	[VCAP_KF_L3_DST_IS]                      =  "L3_DST_IS",
+	[VCAP_KF_L3_FRAGMENT]                    =  "L3_FRAGMENT",
+	[VCAP_KF_L3_FRAGMENT_TYPE]               =  "L3_FRAGMENT_TYPE",
+	[VCAP_KF_L3_FRAG_INVLD_L4_LEN]           =  "L3_FRAG_INVLD_L4_LEN",
+	[VCAP_KF_L3_FRAG_OFS_GT0]                =  "L3_FRAG_OFS_GT0",
+	[VCAP_KF_L3_IP4_DIP]                     =  "L3_IP4_DIP",
+	[VCAP_KF_L3_IP4_SIP]                     =  "L3_IP4_SIP",
+	[VCAP_KF_L3_IP6_DIP]                     =  "L3_IP6_DIP",
+	[VCAP_KF_L3_IP6_SIP]                     =  "L3_IP6_SIP",
+	[VCAP_KF_L3_IP_PROTO]                    =  "L3_IP_PROTO",
+	[VCAP_KF_L3_OPTIONS_IS]                  =  "L3_OPTIONS_IS",
+	[VCAP_KF_L3_PAYLOAD]                     =  "L3_PAYLOAD",
+	[VCAP_KF_L3_RT_IS]                       =  "L3_RT_IS",
+	[VCAP_KF_L3_TOS]                         =  "L3_TOS",
+	[VCAP_KF_L3_TTL_GT0]                     =  "L3_TTL_GT0",
+	[VCAP_KF_L4_1588_DOM]                    =  "L4_1588_DOM",
+	[VCAP_KF_L4_1588_VER]                    =  "L4_1588_VER",
+	[VCAP_KF_L4_ACK]                         =  "L4_ACK",
+	[VCAP_KF_L4_DPORT]                       =  "L4_DPORT",
+	[VCAP_KF_L4_FIN]                         =  "L4_FIN",
+	[VCAP_KF_L4_PAYLOAD]                     =  "L4_PAYLOAD",
+	[VCAP_KF_L4_PSH]                         =  "L4_PSH",
+	[VCAP_KF_L4_RNG]                         =  "L4_RNG",
+	[VCAP_KF_L4_RST]                         =  "L4_RST",
+	[VCAP_KF_L4_SEQUENCE_EQ0_IS]             =  "L4_SEQUENCE_EQ0_IS",
+	[VCAP_KF_L4_SPORT]                       =  "L4_SPORT",
+	[VCAP_KF_L4_SPORT_EQ_DPORT_IS]           =  "L4_SPORT_EQ_DPORT_IS",
+	[VCAP_KF_L4_SYN]                         =  "L4_SYN",
+	[VCAP_KF_L4_URG]                         =  "L4_URG",
+	[VCAP_KF_LOOKUP_FIRST_IS]                =  "LOOKUP_FIRST_IS",
+	[VCAP_KF_LOOKUP_GEN_IDX]                 =  "LOOKUP_GEN_IDX",
+	[VCAP_KF_LOOKUP_GEN_IDX_SEL]             =  "LOOKUP_GEN_IDX_SEL",
+	[VCAP_KF_LOOKUP_PAG]                     =  "LOOKUP_PAG",
+	[VCAP_KF_MIRROR_PROBE]                   =  "MIRROR_PROBE",
+	[VCAP_KF_OAM_CCM_CNTS_EQ0]               =  "OAM_CCM_CNTS_EQ0",
+	[VCAP_KF_OAM_DETECTED]                   =  "OAM_DETECTED",
+	[VCAP_KF_OAM_FLAGS]                      =  "OAM_FLAGS",
+	[VCAP_KF_OAM_MEL_FLAGS]                  =  "OAM_MEL_FLAGS",
+	[VCAP_KF_OAM_MEPID]                      =  "OAM_MEPID",
+	[VCAP_KF_OAM_OPCODE]                     =  "OAM_OPCODE",
+	[VCAP_KF_OAM_VER]                        =  "OAM_VER",
+	[VCAP_KF_OAM_Y1731_IS]                   =  "OAM_Y1731_IS",
+	[VCAP_KF_PROT_ACTIVE]                    =  "PROT_ACTIVE",
+	[VCAP_KF_TCP_IS]                         =  "TCP_IS",
+	[VCAP_KF_TCP_UDP_IS]                     =  "TCP_UDP_IS",
+	[VCAP_KF_TYPE]                           =  "TYPE",
+};
+
+/* Actionfield names */
+static const char * const vcap_actionfield_names[] = {
+	[VCAP_AF_NO_VALUE]                       =  "(None)",
+	[VCAP_AF_ACL_ID]                         =  "ACL_ID",
+	[VCAP_AF_CLS_VID_SEL]                    =  "CLS_VID_SEL",
+	[VCAP_AF_CNT_ID]                         =  "CNT_ID",
+	[VCAP_AF_COPY_PORT_NUM]                  =  "COPY_PORT_NUM",
+	[VCAP_AF_COPY_QUEUE_NUM]                 =  "COPY_QUEUE_NUM",
+	[VCAP_AF_CPU_COPY_ENA]                   =  "CPU_COPY_ENA",
+	[VCAP_AF_CPU_QU]                         =  "CPU_QU",
+	[VCAP_AF_CPU_QUEUE_NUM]                  =  "CPU_QUEUE_NUM",
+	[VCAP_AF_DEI_A_VAL]                      =  "DEI_A_VAL",
+	[VCAP_AF_DEI_B_VAL]                      =  "DEI_B_VAL",
+	[VCAP_AF_DEI_C_VAL]                      =  "DEI_C_VAL",
+	[VCAP_AF_DEI_ENA]                        =  "DEI_ENA",
+	[VCAP_AF_DEI_VAL]                        =  "DEI_VAL",
+	[VCAP_AF_DP_ENA]                         =  "DP_ENA",
+	[VCAP_AF_DP_VAL]                         =  "DP_VAL",
+	[VCAP_AF_DSCP_ENA]                       =  "DSCP_ENA",
+	[VCAP_AF_DSCP_SEL]                       =  "DSCP_SEL",
+	[VCAP_AF_DSCP_VAL]                       =  "DSCP_VAL",
+	[VCAP_AF_ES2_REW_CMD]                    =  "ES2_REW_CMD",
+	[VCAP_AF_ESDX]                           =  "ESDX",
+	[VCAP_AF_FWD_KILL_ENA]                   =  "FWD_KILL_ENA",
+	[VCAP_AF_FWD_MODE]                       =  "FWD_MODE",
+	[VCAP_AF_FWD_SEL]                        =  "FWD_SEL",
+	[VCAP_AF_HIT_ME_ONCE]                    =  "HIT_ME_ONCE",
+	[VCAP_AF_HOST_MATCH]                     =  "HOST_MATCH",
+	[VCAP_AF_IGNORE_PIPELINE_CTRL]           =  "IGNORE_PIPELINE_CTRL",
+	[VCAP_AF_INTR_ENA]                       =  "INTR_ENA",
+	[VCAP_AF_ISDX_ADD_REPLACE_SEL]           =  "ISDX_ADD_REPLACE_SEL",
+	[VCAP_AF_ISDX_ENA]                       =  "ISDX_ENA",
+	[VCAP_AF_ISDX_VAL]                       =  "ISDX_VAL",
+	[VCAP_AF_LOOP_ENA]                       =  "LOOP_ENA",
+	[VCAP_AF_LRN_DIS]                        =  "LRN_DIS",
+	[VCAP_AF_MAP_IDX]                        =  "MAP_IDX",
+	[VCAP_AF_MAP_KEY]                        =  "MAP_KEY",
+	[VCAP_AF_MAP_LOOKUP_SEL]                 =  "MAP_LOOKUP_SEL",
+	[VCAP_AF_MASK_MODE]                      =  "MASK_MODE",
+	[VCAP_AF_MATCH_ID]                       =  "MATCH_ID",
+	[VCAP_AF_MATCH_ID_MASK]                  =  "MATCH_ID_MASK",
+	[VCAP_AF_MIRROR_ENA]                     =  "MIRROR_ENA",
+	[VCAP_AF_MIRROR_PROBE]                   =  "MIRROR_PROBE",
+	[VCAP_AF_MIRROR_PROBE_ID]                =  "MIRROR_PROBE_ID",
+	[VCAP_AF_NXT_IDX]                        =  "NXT_IDX",
+	[VCAP_AF_NXT_IDX_CTRL]                   =  "NXT_IDX_CTRL",
+	[VCAP_AF_PAG_OVERRIDE_MASK]              =  "PAG_OVERRIDE_MASK",
+	[VCAP_AF_PAG_VAL]                        =  "PAG_VAL",
+	[VCAP_AF_PCP_A_VAL]                      =  "PCP_A_VAL",
+	[VCAP_AF_PCP_B_VAL]                      =  "PCP_B_VAL",
+	[VCAP_AF_PCP_C_VAL]                      =  "PCP_C_VAL",
+	[VCAP_AF_PCP_ENA]                        =  "PCP_ENA",
+	[VCAP_AF_PCP_VAL]                        =  "PCP_VAL",
+	[VCAP_AF_PIPELINE_ACT]                   =  "PIPELINE_ACT",
+	[VCAP_AF_PIPELINE_FORCE_ENA]             =  "PIPELINE_FORCE_ENA",
+	[VCAP_AF_PIPELINE_PT]                    =  "PIPELINE_PT",
+	[VCAP_AF_POLICE_ENA]                     =  "POLICE_ENA",
+	[VCAP_AF_POLICE_IDX]                     =  "POLICE_IDX",
+	[VCAP_AF_POLICE_REMARK]                  =  "POLICE_REMARK",
+	[VCAP_AF_POLICE_VCAP_ONLY]               =  "POLICE_VCAP_ONLY",
+	[VCAP_AF_POP_VAL]                        =  "POP_VAL",
+	[VCAP_AF_PORT_MASK]                      =  "PORT_MASK",
+	[VCAP_AF_PUSH_CUSTOMER_TAG]              =  "PUSH_CUSTOMER_TAG",
+	[VCAP_AF_PUSH_INNER_TAG]                 =  "PUSH_INNER_TAG",
+	[VCAP_AF_PUSH_OUTER_TAG]                 =  "PUSH_OUTER_TAG",
+	[VCAP_AF_QOS_ENA]                        =  "QOS_ENA",
+	[VCAP_AF_QOS_VAL]                        =  "QOS_VAL",
+	[VCAP_AF_REW_OP]                         =  "REW_OP",
+	[VCAP_AF_RT_DIS]                         =  "RT_DIS",
+	[VCAP_AF_SWAP_MACS_ENA]                  =  "SWAP_MACS_ENA",
+	[VCAP_AF_TAG_A_DEI_SEL]                  =  "TAG_A_DEI_SEL",
+	[VCAP_AF_TAG_A_PCP_SEL]                  =  "TAG_A_PCP_SEL",
+	[VCAP_AF_TAG_A_TPID_SEL]                 =  "TAG_A_TPID_SEL",
+	[VCAP_AF_TAG_A_VID_SEL]                  =  "TAG_A_VID_SEL",
+	[VCAP_AF_TAG_B_DEI_SEL]                  =  "TAG_B_DEI_SEL",
+	[VCAP_AF_TAG_B_PCP_SEL]                  =  "TAG_B_PCP_SEL",
+	[VCAP_AF_TAG_B_TPID_SEL]                 =  "TAG_B_TPID_SEL",
+	[VCAP_AF_TAG_B_VID_SEL]                  =  "TAG_B_VID_SEL",
+	[VCAP_AF_TAG_C_DEI_SEL]                  =  "TAG_C_DEI_SEL",
+	[VCAP_AF_TAG_C_PCP_SEL]                  =  "TAG_C_PCP_SEL",
+	[VCAP_AF_TAG_C_TPID_SEL]                 =  "TAG_C_TPID_SEL",
+	[VCAP_AF_TAG_C_VID_SEL]                  =  "TAG_C_VID_SEL",
+	[VCAP_AF_TYPE]                           =  "TYPE",
+	[VCAP_AF_UNTAG_VID_ENA]                  =  "UNTAG_VID_ENA",
+	[VCAP_AF_VID_A_VAL]                      =  "VID_A_VAL",
+	[VCAP_AF_VID_B_VAL]                      =  "VID_B_VAL",
+	[VCAP_AF_VID_C_VAL]                      =  "VID_C_VAL",
+	[VCAP_AF_VID_VAL]                        =  "VID_VAL",
+};
+
+/* VCAPs */
+const struct vcap_info lan969x_vcaps[] = {
+	[VCAP_TYPE_IS0] = {
+		.name = "is0",
+		.rows = 256,
+		.sw_count = 12,
+		.sw_width = 52,
+		.sticky_width = 1,
+		.act_width = 103,
+		.default_cnt = 70,
+		.require_cnt_dis = 0,
+		.version = 1,
+		.keyfield_set = is0_keyfield_set,
+		.keyfield_set_size = ARRAY_SIZE(is0_keyfield_set),
+		.actionfield_set = is0_actionfield_set,
+		.actionfield_set_size = ARRAY_SIZE(is0_actionfield_set),
+		.keyfield_set_map = is0_keyfield_set_map,
+		.keyfield_set_map_size = is0_keyfield_set_map_size,
+		.actionfield_set_map = is0_actionfield_set_map,
+		.actionfield_set_map_size = is0_actionfield_set_map_size,
+		.keyfield_set_typegroups = is0_keyfield_set_typegroups,
+		.actionfield_set_typegroups = is0_actionfield_set_typegroups,
+	},
+	[VCAP_TYPE_IS2] = {
+		.name = "is2",
+		.rows = 256,
+		.sw_count = 12,
+		.sw_width = 52,
+		.sticky_width = 1,
+		.act_width = 103,
+		.default_cnt = 38,
+		.require_cnt_dis = 0,
+		.version = 1,
+		.keyfield_set = is2_keyfield_set,
+		.keyfield_set_size = ARRAY_SIZE(is2_keyfield_set),
+		.actionfield_set = is2_actionfield_set,
+		.actionfield_set_size = ARRAY_SIZE(is2_actionfield_set),
+		.keyfield_set_map = is2_keyfield_set_map,
+		.keyfield_set_map_size = is2_keyfield_set_map_size,
+		.actionfield_set_map = is2_actionfield_set_map,
+		.actionfield_set_map_size = is2_actionfield_set_map_size,
+		.keyfield_set_typegroups = is2_keyfield_set_typegroups,
+		.actionfield_set_typegroups = is2_actionfield_set_typegroups,
+	},
+	[VCAP_TYPE_ES0] = {
+		.name = "es0",
+		.rows = 1536,
+		.sw_count = 1,
+		.sw_width = 51,
+		.sticky_width = 1,
+		.act_width = 469,
+		.default_cnt = 35,
+		.require_cnt_dis = 0,
+		.version = 1,
+		.keyfield_set = es0_keyfield_set,
+		.keyfield_set_size = ARRAY_SIZE(es0_keyfield_set),
+		.actionfield_set = es0_actionfield_set,
+		.actionfield_set_size = ARRAY_SIZE(es0_actionfield_set),
+		.keyfield_set_map = es0_keyfield_set_map,
+		.keyfield_set_map_size = es0_keyfield_set_map_size,
+		.actionfield_set_map = es0_actionfield_set_map,
+		.actionfield_set_map_size = es0_actionfield_set_map_size,
+		.keyfield_set_typegroups = es0_keyfield_set_typegroups,
+		.actionfield_set_typegroups = es0_actionfield_set_typegroups,
+	},
+	[VCAP_TYPE_ES2] = {
+		.name = "es2",
+		.rows = 256,
+		.sw_count = 12,
+		.sw_width = 52,
+		.sticky_width = 1,
+		.act_width = 19,
+		.default_cnt = 39,
+		.require_cnt_dis = 0,
+		.version = 1,
+		.keyfield_set = es2_keyfield_set,
+		.keyfield_set_size = ARRAY_SIZE(es2_keyfield_set),
+		.actionfield_set = es2_actionfield_set,
+		.actionfield_set_size = ARRAY_SIZE(es2_actionfield_set),
+		.keyfield_set_map = es2_keyfield_set_map,
+		.keyfield_set_map_size = es2_keyfield_set_map_size,
+		.actionfield_set_map = es2_actionfield_set_map,
+		.actionfield_set_map_size = es2_actionfield_set_map_size,
+		.keyfield_set_typegroups = es2_keyfield_set_typegroups,
+		.actionfield_set_typegroups = es2_actionfield_set_typegroups,
+	},
+};
+
+const struct vcap_statistics lan969x_vcap_stats = {
+	.name = "lan969x",
+	.count = 4,
+	.keyfield_set_names = vcap_keyfield_set_names,
+	.actionfield_set_names = vcap_actionfield_set_names,
+	.keyfield_names = vcap_keyfield_names,
+	.actionfield_names = vcap_actionfield_names,
+};
