--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.h
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.h
@@ -76,6 +76,9 @@ struct rt2800_ops {
 	int (*drv_init_registers)(struct rt2x00_dev *rt2x00dev);
 	__le32 *(*drv_get_txwi)(struct queue_entry *entry);
 	unsigned int (*drv_get_dma_done)(struct data_queue *queue);
+	int (*hw_get_chippkg)(void);
+	int (*hw_get_chipver)(void);
+	int (*hw_get_chipeco)(void);
 };
 
 static inline u32 rt2800_register_read(struct rt2x00_dev *rt2x00dev,
@@ -184,6 +187,27 @@ static inline unsigned int rt2800_drv_ge
 	return rt2800ops->drv_get_dma_done(queue);
 }
 
+static inline int rt2800_hw_get_chippkg(struct rt2x00_dev *rt2x00dev)
+{
+	const struct rt2800_ops *rt2800ops = rt2x00dev->ops->drv;
+
+	return rt2800ops->hw_get_chippkg();
+}
+
+static inline int rt2800_hw_get_chipver(struct rt2x00_dev *rt2x00dev)
+{
+	const struct rt2800_ops *rt2800ops = rt2x00dev->ops->drv;
+
+	return rt2800ops->hw_get_chipver();
+}
+
+static inline int rt2800_hw_get_chipeco(struct rt2x00_dev *rt2x00dev)
+{
+	const struct rt2800_ops *rt2800ops = rt2x00dev->ops->drv;
+
+	return rt2800ops->hw_get_chipeco();
+}
+
 void rt2800_mcu_request(struct rt2x00_dev *rt2x00dev,
 			const u8 command, const u8 token,
 			const u8 arg0, const u8 arg1);
--- a/drivers/net/wireless/ralink/rt2x00/rt2800pci.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800pci.c
@@ -289,6 +289,10 @@ static int rt2800pci_read_eeprom(struct
 	return retval;
 }
 
+static int rt2800pci_get_chippkg(void) { return 0; }
+static int rt2800pci_get_chipver(void) { return 0; }
+static int rt2800pci_get_chipeco(void) { return 0; }
+
 static const struct ieee80211_ops rt2800pci_mac80211_ops = {
 	.add_chanctx = ieee80211_emulate_add_chanctx,
 	.remove_chanctx = ieee80211_emulate_remove_chanctx,
@@ -336,6 +340,9 @@ static const struct rt2800_ops rt2800pci
 	.drv_init_registers	= rt2800mmio_init_registers,
 	.drv_get_txwi		= rt2800mmio_get_txwi,
 	.drv_get_dma_done	= rt2800mmio_get_dma_done,
+	.hw_get_chippkg		= rt2800pci_get_chippkg,
+	.hw_get_chipver		= rt2800pci_get_chipver,
+	.hw_get_chipeco		= rt2800pci_get_chipeco,
 };
 
 static const struct rt2x00lib_ops rt2800pci_rt2x00_ops = {
--- a/drivers/net/wireless/ralink/rt2x00/rt2800soc.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800soc.c
@@ -27,6 +27,12 @@
 #include "rt2800lib.h"
 #include "rt2800mmio.h"
 
+/* Needed to probe CHIP_VER register on MT7620 */
+#ifdef CONFIG_SOC_MT7620
+#include <asm/mach-ralink/ralink_regs.h>
+#include <asm/mach-ralink/mt7620.h>
+#endif
+
 /* Allow hardware encryption to be disabled. */
 static bool modparam_nohwcrypt;
 module_param_named(nohwcrypt, modparam_nohwcrypt, bool, 0444);
@@ -136,6 +142,27 @@ static int rt2800soc_resume(struct platf
 }
 #endif /* CONFIG_PM */
 
+#ifdef CONFIG_SOC_MT7620
+static int rt2800soc_get_chippkg(void)
+{
+	return mt7620_get_pkg();
+}
+
+static int rt2800soc_get_chipver(void)
+{
+	return mt7620_get_chipver();
+}
+
+static int rt2800soc_get_chipeco(void)
+{
+	return mt7620_get_eco();
+}
+#else
+static int rt2800soc_get_chippkg(void) { return 0; }
+static int rt2800soc_get_chipver(void) { return 0; }
+static int rt2800soc_get_chipeco(void) { return 0; }
+#endif
+
 static const struct ieee80211_ops rt2800soc_mac80211_ops = {
 	.add_chanctx = ieee80211_emulate_add_chanctx,
 	.remove_chanctx = ieee80211_emulate_remove_chanctx,
@@ -183,6 +210,9 @@ static const struct rt2800_ops rt2800soc
 	.drv_init_registers	= rt2800mmio_init_registers,
 	.drv_get_txwi		= rt2800mmio_get_txwi,
 	.drv_get_dma_done	= rt2800mmio_get_dma_done,
+	.hw_get_chippkg		= rt2800soc_get_chippkg,
+	.hw_get_chipver		= rt2800soc_get_chipver,
+	.hw_get_chipeco		= rt2800soc_get_chipeco,
 };
 
 static const struct rt2x00lib_ops rt2800soc_rt2x00_ops = {
--- a/drivers/net/wireless/ralink/rt2x00/rt2800usb.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800usb.c
@@ -628,6 +628,10 @@ static int rt2800usb_probe_hw(struct rt2
 	return 0;
 }
 
+static int rt2800usb_get_chippkg(void) { return 0; }
+static int rt2800usb_get_chipver(void) { return 0; }
+static int rt2800usb_get_chipeco(void) { return 0; }
+
 static const struct ieee80211_ops rt2800usb_mac80211_ops = {
 	.add_chanctx = ieee80211_emulate_add_chanctx,
 	.remove_chanctx = ieee80211_emulate_remove_chanctx,
@@ -676,6 +680,9 @@ static const struct rt2800_ops rt2800usb
 	.drv_init_registers	= rt2800usb_init_registers,
 	.drv_get_txwi		= rt2800usb_get_txwi,
 	.drv_get_dma_done	= rt2800usb_get_dma_done,
+	.hw_get_chippkg		= rt2800usb_get_chippkg,
+	.hw_get_chipver		= rt2800usb_get_chipver,
+	.hw_get_chipeco		= rt2800usb_get_chipeco,
 };
 
 static const struct rt2x00lib_ops rt2800usb_rt2x00_ops = {
