From c5a6331c10de88a30b50f2c19342a2f9b642fa13 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Thu, 25 Jun 2020 18:03:47 +0100
Subject: [PATCH] media: bcm2835-unicam: Add support for 14bit mono sources

Now that V4L2_PIX_FMT_Y14 and V4L2_PIX_FMT_Y14P are defined,
allow passing 14bit mono data through the peripheral.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/media/platform/bcm2835/bcm2835-unicam.c | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/drivers/media/platform/bcm2835/bcm2835-unicam.c
+++ b/drivers/media/platform/bcm2835/bcm2835-unicam.c
@@ -446,6 +446,12 @@ static const struct unicam_fmt formats[]
 		.code		= MEDIA_BUS_FMT_Y12_1X12,
 		.depth		= 12,
 		.csi_dt		= MIPI_CSI2_DT_RAW12,
+	}, {
+		.fourcc		= V4L2_PIX_FMT_Y14P,
+		.repacked_fourcc = V4L2_PIX_FMT_Y14,
+		.code		= MEDIA_BUS_FMT_Y14_1X14,
+		.depth		= 14,
+		.csi_dt		= MIPI_CSI2_DT_RAW14,
 		.valid_colorspaces = MASK_CS_RAW,
 	}, {
 		.fourcc		= V4L2_PIX_FMT_Y16,
