// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "cudy,ap1300-outdoor-v1", "mediatek,mt7621-soc";
	model = "Cudy AP1300 Outdoor v1";
	
	aliases {
		led-boot = &led_sys;
		led-failsafe = &led_sys;
		led-running = &led_sys;
		led-upgrade = &led_sys;		
		label-mac-device = &gmac0;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";
		led_sys:status {
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_STATUS;
		};

		internet {
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN_ONLINE;
		};

		lan {
			gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_LAN;
		};

		wifi2g {
			gpios = <&gpio 47 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN_2GHZ;
			linux,default-trigger = "phy0tpt";
		};

		wifi5g {
			gpios = <&gpio 45 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN_5GHZ;
			linux,default-trigger = "phy1tpt";
		};	
	};
	
	watchdog {
		compatible = "linux,wdt-gpio";
		gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		hw_algo = "toggle";
		/* hw_margin_ms seems to be around 30s for this device*/
		hw_margin_ms = <10000>;
		always-running;
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_factory_0: eeprom@0 {
						reg = <0x0 0x400>;
					};

					eeprom_factory_8000: eeprom@8000 {
						reg = <0x8000 0x4da8>;
					};
				};
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xf80000>;
			};

			partition@fd0000 {
				label = "debug";
				reg = <0xfd0000 0x10000>;
				read-only;
			};

			partition@fe0000 {
				label = "backup";
				reg = <0xfe0000 0x10000>;
				read-only;
			};

			partition@ff0000 {
				label = "bdinfo";
				reg = <0xff0000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_bdinfo_de00: macaddr@de00 {
						compatible = "mac-base";
						reg = <0xde00 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};
		};
	};
};

&pcie {
	status = "okay";
};


&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>, <&macaddr_bdinfo_de00 0>;
		nvmem-cell-names = "eeprom", "mac-address";
		ieee80211-freq-limit = <2400000 2500000>;
	};
};

&pcie1 {
	wifi@1,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_8000>, <&macaddr_bdinfo_de00 1>;
		nvmem-cell-names = "eeprom", "mac-address";
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_bdinfo_de00 0>;
	nvmem-cell-names = "mac-address";
};

&switch0 {
	ports {
		port@4 {
			status = "okay";
			label = "lan";
		};
	};
};

&state_default {
	gpio {
		groups = "wdt", "i2c", "jtag";
		function = "gpio";
	};
};
