From 812b4aa3dee6bea5ec6e557a2b4e9168b7bafae9 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Tue, 7 Mar 2023 11:52:36 +0000
Subject: [PATCH] hwmon: (aht10): Add DT compatible string

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 drivers/hwmon/aht10.c | 7 +++++++
 1 file changed, 7 insertions(+)

--- a/drivers/hwmon/aht10.c
+++ b/drivers/hwmon/aht10.c
@@ -57,6 +57,12 @@ static const struct i2c_device_id aht10_
 };
 MODULE_DEVICE_TABLE(i2c, aht10_id);
 
+static const struct of_device_id aht10_of_id[] = {
+	{ .compatible = "aosong,aht10", },
+	{ }
+};
+MODULE_DEVICE_TABLE(of, aht10_of_id);
+
 /**
  *   struct aht10_data - All the data required to operate an AHT10/AHT20 chip
  *   @client: the i2c client associated with the AHT10/AHT20
@@ -380,6 +386,7 @@ static int aht10_probe(struct i2c_client
 static struct i2c_driver aht10_driver = {
 	.driver = {
 		.name = "aht10",
+		.of_match_table = aht10_of_id,
 	},
 	.probe      = aht10_probe,
 	.id_table   = aht10_id,
