--- /dev/null
+++ b/configs/mt7987a_routerich_be7200_defconfig
@@ -0,0 +1,133 @@
+CONFIG_ARM=y
+CONFIG_SYS_HAS_NONCACHED_MEMORY=y
+CONFIG_POSITION_INDEPENDENT=y
+CONFIG_ARCH_MEDIATEK=y
+CONFIG_TEXT_BASE=0x41e00000
+CONFIG_SYS_MALLOC_F_LEN=0x4000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_DEFAULT_DEVICE_TREE="mt7987a-routerich_be7200"
+CONFIG_OF_LIBFDT_OVERLAY=y
+CONFIG_TARGET_MT7987=y
+CONFIG_CPU_ARMV8=y
+CONFIG_SYS_BOOTM_LEN=0x6000000
+CONFIG_SYS_LOAD_ADDR=0x48000000
+CONFIG_PRE_CON_BUF_ADDR=0x4007ef00
+CONFIG_DEBUG_UART_BASE=0x11000000
+CONFIG_DEBUG_UART_CLOCK=40000000
+CONFIG_DEBUG_UART=y
+CONFIG_FIT=y
+CONFIG_AUTOBOOT_MENU_SHOW=y
+CONFIG_DEFAULT_FDT_FILE="mt7987a-routerich_be7200"
+CONFIG_SYS_CBSIZE=512
+CONFIG_SYS_PBSIZE=1049
+CONFIG_LOGLEVEL=7
+CONFIG_PRE_CONSOLE_BUFFER=y
+CONFIG_LOG=y
+# CONFIG_BOARD_INIT is not set
+CONFIG_BOARD_LATE_INIT=y
+CONFIG_HUSH_PARSER=y
+CONFIG_SYS_PROMPT="MT7987> "
+# CONFIG_BOOTM_NETBSD is not set
+# CONFIG_BOOTM_PLAN9 is not set
+# CONFIG_BOOTM_RTEMS is not set
+# CONFIG_BOOTM_VXWORKS is not set
+# CONFIG_CMD_BOOTEFI_BOOTMGR is not set
+CONFIG_CMD_LICENSE=y
+CONFIG_CMD_BOOTMENU=y
+CONFIG_CMD_ASKENV=y
+CONFIG_CMD_ERASEENV=y
+CONFIG_CMD_ENV_FLAGS=y
+CONFIG_CMD_STRINGS=y
+CONFIG_CMD_CPU=y
+CONFIG_CMD_DM=y
+CONFIG_CMD_GPIO=y
+CONFIG_CMD_PWM=y
+CONFIG_CMD_GPT=y
+CONFIG_CMD_I2C=y
+CONFIG_CMD_MMC=y
+CONFIG_CMD_MTD=y
+CONFIG_CMD_PART=y
+CONFIG_CMD_PCI=y
+CONFIG_CMD_USB=y
+CONFIG_CMD_TFTPSRV=y
+CONFIG_CMD_RARP=y
+CONFIG_CMD_CDP=y
+CONFIG_CMD_SNTP=y
+CONFIG_CMD_LINK_LOCAL=y
+CONFIG_CMD_DHCP=y
+CONFIG_CMD_DNS=y
+CONFIG_CMD_PING=y
+CONFIG_CMD_PXE=y
+CONFIG_CMD_CACHE=y
+CONFIG_CMD_PSTORE=y
+CONFIG_CMD_PSTORE_MEM_ADDR=0x42ff0000
+CONFIG_CMD_UUID=y
+CONFIG_CMD_HASH=y
+CONFIG_CMD_SMC=y
+CONFIG_CMD_EXT4=y
+CONFIG_CMD_FAT=y
+CONFIG_CMD_FS_GENERIC=y
+CONFIG_CMD_FS_UUID=y
+CONFIG_CMD_SF_TEST=y
+CONFIG_CMD_UBI=y
+CONFIG_CMD_UBI_RENAME=y
+# CONFIG_CMD_XIMG is not set
+CONFIG_ENV_OVERWRITE=y
+CONFIG_ENV_IS_IN_UBI=y
+CONFIG_ENV_REDUNDANT=y
+CONFIG_ENV_UBI_PART="ubi"
+CONFIG_ENV_UBI_VOLUME="ubootenv"
+CONFIG_ENV_UBI_VOLUME_REDUND="ubootenv2"
+CONFIG_ENV_USE_DEFAULT_ENV_TEXT_FILE=y
+CONFIG_ENV_DEFAULT_ENV_TEXT_FILE="defenvs/routerich_be7200_env"
+CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
+CONFIG_VERSION_VARIABLE=y
+CONFIG_NETCONSOLE=y
+CONFIG_USE_IPADDR=y
+CONFIG_IPADDR="192.168.1.1"
+CONFIG_USE_NETMASK=y
+CONFIG_NETMASK="255.255.255.0"
+CONFIG_USE_SERVERIP=y
+CONFIG_SERVERIP="192.168.1.254"
+CONFIG_NET_RANDOM_ETHADDR=y
+CONFIG_BUTTON=y
+CONFIG_BUTTON_GPIO=y
+CONFIG_CLK=y
+CONFIG_DM_I2C=y
+CONFIG_SYS_I2C_MTK=y
+CONFIG_LED=y
+CONFIG_LED_BLINK=y
+CONFIG_LED_GPIO=y
+# CONFIG_MMC is not set
+CONFIG_MTD=y
+CONFIG_DM_MTD=y
+CONFIG_MTD_SPI_NAND=y
+CONFIG_MTD_UBI_FASTMAP=y
+CONFIG_PHY_ETHERNET_ID=y
+CONFIG_PHY_FIXED=y
+CONFIG_MEDIATEK_ETH=y
+CONFIG_PHY=y
+CONFIG_PHY_MTK_TPHY=y
+CONFIG_PINCTRL=y
+CONFIG_PINCONF=y
+CONFIG_PINCTRL_MT7987=y
+CONFIG_POWER_DOMAIN=y
+CONFIG_MTK_POWER_DOMAIN=y
+CONFIG_DM_REGULATOR=y
+CONFIG_DM_REGULATOR_FIXED=y
+CONFIG_DM_REGULATOR_GPIO=y
+CONFIG_DM_PWM=y
+CONFIG_PWM_MTK=y
+CONFIG_SCSI=y
+CONFIG_DM_SERIAL=y
+CONFIG_SERIAL_RX_BUFFER=y
+CONFIG_MTK_SERIAL=y
+CONFIG_SPI=y
+CONFIG_DM_SPI=y
+CONFIG_MTK_SPIM=y
+CONFIG_USB=y
+CONFIG_USB_XHCI_HCD=y
+CONFIG_USB_XHCI_MTK=y
+CONFIG_USB_STORAGE=y
+CONFIG_ZSTD=y
+CONFIG_HEXDUMP=y
--- /dev/null
+++ b/defenvs/routerich_be7200_env
@@ -0,0 +1,57 @@
+ipaddr=192.168.1.1
+serverip=192.168.1.254
+loadaddr=0x48000000
+console=earlycon=uart8250,mmio32,0x11002000 console=ttyS0
+bootcmd=run check_buttons ; if pstore check ; then run boot_recovery ; else run boot_ubi ; fi
+bootconf=config-1
+bootdelay=0
+bootfile=openwrt-mediatek-filogic-routerich_be7200-initramfs-recovery.itb
+bootfile_bl2=openwrt-mediatek-filogic-routerich_be7200-preloader.bin
+bootfile_fip=openwrt-mediatek-filogic-routerich_be7200-bl31-uboot.fip
+bootfile_upg=openwrt-mediatek-filogic-routerich_be7200-squashfs-sysupgrade.itb
+bootled_status=blue:status
+bootmenu_confirm_return=askenv - Press ENTER to return to menu ; bootmenu 60
+bootmenu_default=0
+bootmenu_delay=0
+bootmenu_title=      [0;34m( ( ( [1;39mOpenWrt[0;34m ) ) )
+bootmenu_0=Initialize environment.=run _firstboot
+bootmenu_0d=Run default boot command.=run boot_default
+bootmenu_1=Boot system via TFTP.=run boot_tftp ; run bootmenu_confirm_return
+bootmenu_2=Boot production system from NAND.=run boot_production ; run bootmenu_confirm_return
+bootmenu_3=Boot recovery system from NAND.=run boot_recovery ; run bootmenu_confirm_return
+bootmenu_4=Load production system via TFTP then write to NAND.=setenv noboot 1 ; setenv replacevol 1 ; run boot_tftp_production ; setenv noboot ; setenv replacevol ; run bootmenu_confirm_return
+bootmenu_5=Load recovery system via TFTP then write to NAND.=setenv noboot 1 ; setenv replacevol 1 ; run boot_tftp_recovery ; setenv noboot ; setenv replacevol ; run bootmenu_confirm_return
+bootmenu_6=[31mLoad BL31+U-Boot FIP via TFTP then write to NAND.[0m=run boot_tftp_write_fip ; run bootmenu_confirm_return
+bootmenu_7=[31mLoad BL2 preloader via TFTP then write to NAND.[0m=run boot_tftp_write_bl2 ; run bootmenu_confirm_return
+bootmenu_8=Reboot.=reset
+bootmenu_9=Reset all settings to factory defaults.=run reset_factory ; reset
+boot_first=if button reset ; then led $bootled_status on ; run boot_default ; fi ; bootmenu
+boot_default=if env exists flag_recover ; then else run bootcmd ; fi ; run boot_recovery ; setenv replacevol 1 ; run boot_tftp_forever
+boot_production=led $bootled_status on ; run ubi_read_production && bootm $loadaddr#$bootconf ; led bootled_status off
+boot_recovery=led $bootled_status on ; run ubi_read_recovery && bootm $loadaddr#$bootconf ; led bootled_status off
+boot_ubi=run boot_production ; run boot_recovery ; run boot_tftp_forever
+boot_tftp_forever=led $bootled_status on ; while true ; do run boot_tftp ; sleep 1 ; done
+boot_tftp_production=tftpboot $loadaddr $bootfile_upg && env exists replacevol && iminfo $loadaddr && run ubi_write_production ; if env exists noboot ; then else bootm $loadaddr#$bootconf ; fi
+boot_tftp_recovery=tftpboot $loadaddr $bootfile && env exists replacevol && iminfo $loadaddr && run ubi_write_recovery ; if env exists noboot ; then else bootm $loadaddr#$bootconf ; fi
+boot_tftp=tftpboot $loadaddr $bootfile && bootm $loadaddr#$bootconf
+boot_tftp_write_fip=tftpboot $loadaddr $bootfile_fip && run mtd_write_fip && run reset_factory
+boot_tftp_write_bl2=tftpboot $loadaddr $bootfile_bl2 && run mtd_write_bl2
+check_buttons=if button reset ; then run boot_tftp ; fi
+ethaddr_factory=mtd read Factory 0x40080000 0x0 0x20000 && env readmem -b ethaddr 0x40080004 0x6 ; setenv ethaddr_factory
+part_default=production
+part_recovery=recovery
+reset_factory=ubi part ubi ; mw $loadaddr 0x0 0x800 ; ubi write $loadaddr ubootenv 0x800 ; ubi write $loadaddr ubootenv2 0x800
+mtd_write_fip=mtd erase FIP && mtd write FIP $loadaddr
+mtd_write_bl2=mtd erase BL2 && mtd write BL2 $loadaddr
+ubi_create_env=ubi check ubootenv || ubi create ubootenv 0x100000 dynamic || run ubi_format ; ubi check ubootenv2 || ubi create ubootenv2 0x100000 dynamic || run ubi_format
+ubi_format=ubi detach ; mtd erase ubi && ubi part ubi ; reset
+ubi_prepare_rootfs=if ubi check rootfs_data ; then else if env exists rootfs_data_max ; then ubi create rootfs_data $rootfs_data_max dynamic || ubi create rootfs_data - dynamic ; else ubi create rootfs_data - dynamic ; fi ; fi
+ubi_read_production=ubi read $loadaddr fit && iminfo $loadaddr && run ubi_prepare_rootfs
+ubi_read_recovery=ubi check recovery && ubi read $loadaddr recovery
+ubi_remove_rootfs=ubi check rootfs_data && ubi remove rootfs_data
+ubi_write_production=ubi check fit && ubi remove fit ; run ubi_remove_rootfs ; ubi create fit $filesize dynamic && ubi write $loadaddr fit $filesize
+ubi_write_recovery=ubi check recovery && ubi remove recovery ; run ubi_remove_rootfs ; ubi create recovery $filesize dynamic && ubi write $loadaddr recovery $filesize
+_init_env=setenv _init_env ; run ubi_create_env ; saveenv ; saveenv
+_firstboot=setenv _firstboot ; run ethaddr_factory ; run _switch_to_menu ; run _init_env ; run boot_first
+_switch_to_menu=setenv _switch_to_menu ; setenv bootdelay 3 ; setenv bootmenu_delay 3 ; setenv bootmenu_0 $bootmenu_0d ; setenv bootmenu_0d ; run _bootmenu_update_title
+_bootmenu_update_title=setenv _bootmenu_update_title ; setenv bootmenu_title "$bootmenu_title       [33m$ver[0m"
--- /dev/null
+++ b/arch/arm/dts/mt7987a-routerich_be7200.dts
@@ -0,0 +1,77 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (c) 2025
+ * Author: Mikhail Zhilkin <csharper2005@gmail.com>
+ */
+
+/dts-v1/;
+#include "mt7987a.dtsi"
+#include <dt-bindings/input/input.h>
+
+/ {
+	model = "Routerich BE7200";
+	compatible = "routerich,be7200",
+		     "mediatek,mt7987";
+
+	gpio-keys {
+		compatible = "gpio-keys";
+
+		button-0 {
+			label = "mesh";
+			linux,code = <KEY_WPS_BUTTON>;
+			gpios = <&pio 0 GPIO_ACTIVE_LOW>;
+			debounce-interval = <10>;
+		};
+
+		button-1 {
+			label = "reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&pio 1 GPIO_ACTIVE_LOW>;
+			debounce-interval = <10>;
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		led-0 {
+			label = "blue:status";
+			gpios = <&pio 4 GPIO_ACTIVE_LOW>;
+		};
+
+		led-1 {
+			label = "blue:wlan5g";
+			gpios = <&pio 5 GPIO_ACTIVE_LOW>;
+		};
+
+		led-2 {
+			label = "blue:mesh";
+			gpios = <&pio 7 GPIO_ACTIVE_LOW>;
+		};
+
+		led-3 {
+			label = "red:wan";
+			gpios = <&pio 8 GPIO_ACTIVE_LOW>;
+		};
+
+		led-4 {
+			label = "blue:wan";
+			gpios = <&pio 9 GPIO_ACTIVE_LOW>;
+		};
+
+		led-5 {
+			label = "blue:lan3";
+			gpios = <&pio 10 GPIO_ACTIVE_LOW>;
+		};
+
+		led-6 {
+			label = "blue:lan2";
+			gpios = <&pio 11 GPIO_ACTIVE_LOW>;
+		};
+
+		led-7 {
+			label = "blue:lan1";
+			gpios = <&pio 12 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
--- a/arch/arm/dts/Makefile
+++ b/arch/arm/dts/Makefile
@@ -1138,6 +1138,7 @@ dtb-$(CONFIG_ARCH_MEDIATEK) += \
 	mt7986b-emmc-rfb.dtb \
 	mt7987a-emmc-rfb.dtb \
 	mt7987a-rfb.dtb \
+	mt7987a-routerich_be7200.dtb \
 	mt7987a-sd-rfb.dtb \
 	mt7988-rfb.dtb \
 	mt7988-sd-rfb.dtb \
--- /dev/null
+++ b/arch/arm/dts/mt7987a-routerich_be7200-u-boot.dtsi
@@ -0,0 +1,84 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (c) 2025
+ * Author: Mikhail Zhilkin <csharper2005@gmail.com>
+ */
+
+#include "mt7987a-u-boot.dtsi"
+#include "mt7987-netsys-u-boot.dtsi"
+
+/ {
+	model = "Routerich BE7200";
+	compatible = "routerich,be7200",
+		     "mediatek,mt7987";
+};
+
+&eth0 {
+	status = "okay";
+	pinctrl-names = "default";
+	pinctrl-0 = <&mdio0_pins>;
+	phy-mode = "2500base-x";
+	mediatek,switch = "auto";
+	reset-gpios = <&pio 42 GPIO_ACTIVE_HIGH>;
+
+	fixed-link {
+		speed = <2500>;
+		full-duplex;
+		pause;
+	};
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_flash_pins>;
+	#address-cells = <1>;
+	#size-cells = <0>;
+	status = "okay";
+	must_tx;
+	enhance_timing;
+	dma_ext;
+	ipm_design;
+	support_quad;
+	tick_dly = <2>;
+	sample_sel = <0>;
+
+	spi_nand@0 {
+		compatible = "spi-nand";
+		reg = <0>;
+		spi-max-frequency = <52000000>;
+		spi-rx-bus-width = <4>;
+		spi-tx-bus-width = <4>;
+
+		partitions {
+			compatible = "fixed-partitions";
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			partition@0 {
+				label = "BL2";
+				reg = <0x0 0x100000>;
+			};
+
+			partition@100000 {
+				label = "u-boot-env (unused)";
+				reg = <0x100000 0x80000>;
+			};
+
+			partition@180000 {
+				label = "Factory";
+				reg = <0x180000 0x400000>;
+			};
+
+			partition@580000 {
+				label = "FIP";
+				reg = <0x580000 0x200000>;
+			};
+
+			partition@780000 {
+				label = "ubi";
+				reg = <0x780000 0x1f880000>;
+				compatible = "linux,ubi";
+			};
+		};
+	};
+};
