// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/dts-v1/;
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/pinctrl/mt65xx.h>

#include "mt7986b.dtsi"

/ {
	compatible = "tplink,archer-ax80-v1-eu", "mediatek,mt7986b";
	model = "TP-Link Archer AX80 v1 (EU)";
	
	aliases {
		serial0 = &uart0;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};
	
	chosen {
		stdout-path = "serial0:115200n8";
	};
	
	memory@40000000 {
		reg = <0 0x40000000 0 0x20000000>;
		device_type = "memory";
	};
	
	leds {
		compatible = "gpio-leds";
		
		led_power: power {
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_POWER;
			gpios = <&pio 15 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
		
		wlan2g {
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_WLAN_2GHZ;
			gpios = <&pio 11 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};
		
		wlan5g {
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_WLAN_5GHZ;
			gpios = <&pio 12 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
		
		internet_white {
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_WAN_ONLINE;
			gpios = <&pio 9 GPIO_ACTIVE_LOW>;
		};
		
		internet_orange {
			color = <LED_COLOR_ID_ORANGE>;
			function = LED_FUNCTION_WAN;
			gpios = <&pio 19 GPIO_ACTIVE_LOW>;
		};
		
		lan {
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_LAN;
			gpios = <&pio 16 GPIO_ACTIVE_HIGH>;
		};
		
		usb {
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_DISK;
			gpios = <&pio 10 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ssusb>;
			linux,default-trigger = "usbport";
		};
		
		wps {
			color = <LED_COLOR_ID_WHITE>;
			function = LED_FUNCTION_WPS;
			gpios = <&pio 18 GPIO_ACTIVE_LOW>;
		};
	};
	
	keys {
		compatible = "gpio-keys";
		
		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&pio 7 GPIO_ACTIVE_LOW>;
		};
		
		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&pio 14 GPIO_ACTIVE_LOW>;
		};
		
		wifi {
			label = "wlan";
			linux,code = <KEY_WLAN>;
			gpios = <&pio 20 GPIO_ACTIVE_LOW>;
		};
	};
	
	reg_3p3v: regulator-3p3v {
		compatible = "regulator-fixed";
		regulator-name = "fixed-3.3V";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		regulator-always-on;
	};
	
	reg_5v: regulator-5v {
		compatible = "regulator-fixed";
		regulator-name = "fixed-5V";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-boot-on;
		regulator-always-on;
	};
};

&auxadc {
	status = "okay";
};

&crypto {
	status = "okay";
};

&eth {
	status = "okay";
	
	gmac0: mac@0 {
		compatible = "mediatek,eth-mac";
		reg = <0>;
		phy-mode = "2500base-x";
		fixed-link {
			speed = <2500>;
			full-duplex;
		};
	};
	
	mac@1 {
		compatible = "mediatek,eth-mac";
		reg = <1>;
		phy-mode = "2500base-x";
		phy-handle = <&phy6>;
	};
	
	mdio-bus {
		#address-cells = <1>;
		#size-cells = <0>;
		reset-delay-us = <1500000>;
		reset-post-delay-us = <1000000>;		
		reset-gpios = <&pio 6 GPIO_ACTIVE_LOW>;
		phy6: phy@6 {
			compatible = "ethernet-phy-ieee802.3-c45";
			reg = <6>;
		};
		
		switch@1f {
			compatible = "mediatek,mt7531";
			reg = <31>;
			reset-gpios = <&pio 5 GPIO_ACTIVE_HIGH>;
			interrupt-controller;
			#interrupt-cells = <1>;
			interrupt-parent = <&pio>;
			interrupts = <66 IRQ_TYPE_LEVEL_HIGH>;
			
			ports {
				#address-cells = <1>;
				#size-cells = <0>;
				port@0 {
					reg = <1>;
					label = "lan0";
				};
				port@1 {
					reg = <2>;
					label = "lan1";
				};
				port@2 {
					reg = <3>;
					label = "lan2";
				};
				port@3 {
					reg = <4>;
					label = "lan3";
				};
				port@6 {
					reg = <6>;
					label = "cpu";
					ethernet = <&gmac0>;
					phy-mode = "2500base-x";
					fixed-link {
						speed = <2500>;
						full-duplex;
					};
				};
			};
		};
	};
};

&spi0 {
	pinctrl-names = "default";
	pinctrl-0 = <&spi_flash_pins>;
	status = "okay";
	
	flash@0 {
		compatible = "spi-nand";
		reg = <0>;
		spi-max-frequency = <52000000>;
		spi-tx-bus-width = <4>;
		spi-rx-bus-width = <4>;
		spi-cal-enable;
		spi-cal-mode = "read-data";
		
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;
			
			partition@0 {
				label = "boot";
				reg = <0x0 0x200000>;
				read-only;
			};
			
			partition@200000 {
				label = "u-boot-env";
				reg = <0x200000 0x100000>;
			};
			
			partition@300000 {
				label = "ubi0";
				reg = <0x300000 0x3200000>;
			};
			
			partition@3500000 {
				label = "ubi1";
				reg = <0x3500000 0x3200000>;
			};
			
			partition@6700000 {
				label = "userconfig";
				reg = <0x6700000 0x800000>;
			};
			
			partition@6f00000 {
				label = "tp_data";
				reg = <0x6f00000 0x400000>;
				read-only;
			};
			
			partition@7300000 {
				label = "mali_data";
				reg = <0x7300000 0x800000>;
			};
		};
	};
};

&pio {
	spi_flash_pins: spi-flash-pins-33-to-38 {
		mux {
			function = "spi";
			groups = "spi0", "spi0_wp_hold";
		};
		conf-pu {
			pins = "SPI2_CS", "SPI2_HOLD", "SPI2_WP";
			drive-strength = <MTK_DRIVE_8mA>;
			bias-disable; /* bias-disable */
		};
		conf-pd {
			pins = "SPI2_CLK", "SPI2_MOSI", "SPI2_MISO";
			drive-strength = <MTK_DRIVE_8mA>;
			bias-disable; /* bias-disable */
		};
	};
	
	wf_2g_5g_pins: wf_2g_5g-pins {
		mux {
			function = "wifi";
			groups = "wf_2g", "wf_5g";
		};
		conf {
			pins = "WF0_HB1", "WF0_HB2", "WF0_HB3", "WF0_HB4",
			"WF0_HB0", "WF0_HB0_B", "WF0_HB5", "WF0_HB6",
			"WF0_HB7", "WF0_HB8", "WF0_HB9", "WF0_HB10",
			"WF0_TOP_CLK", "WF0_TOP_DATA", "WF1_HB1",
			"WF1_HB2", "WF1_HB3", "WF1_HB4", "WF1_HB0",
			"WF1_HB5", "WF1_HB6", "WF1_HB7", "WF1_HB8",
			"WF1_TOP_CLK", "WF1_TOP_DATA";
			drive-strength = <MTK_DRIVE_4mA>;
		};
	};
};

&trng {
	status = "okay";
};

&uart0 {
	status = "okay";
};

&ssusb {
	vusb33-supply = <&reg_3p3v>;
	vbus-supply = <&reg_5v>;
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&watchdog {
	status = "okay";
};

&wifi {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&wf_2g_5g_pins>;
};
