// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "dlink,dir-x1860-b1", "mediatek,mt7621-soc";
	model = "D-Link DIR-X1860 B1 / DIR-X1550 A1";

	aliases {
		label-mac-device = &ethernet;
		led-boot = &status_orange;
		led-failsafe = &status_orange;
		led-running = &status_white;
		led-upgrade = &status_orange;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		status_white: power {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		status_orange: status_orange {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_ORANGE>;
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wan_white {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "mt7530-0:04:link";
		};

		wan_orange {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_ORANGE>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};
	};

	virtual_flash {
		compatible = "mtd-concat";

		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "ubi";
				reg = <0x0 0x0>;
			};
		};
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "bootloader";
			reg = <0x0 0x80000>;
			read-only;
		};

		partition@80000 {
			label = "config";
			reg = <0x80000 0x80000>;
			read-only;
		};

		partition@100000 {
			label = "factory";
			reg = <0x100000 0x80000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				eeprom_factory_0: eeprom@0 {
					reg = <0x0 0xe00>;
				};

				precal_factory_e10: precal@e10 {
					reg = <0xe10 0x19c10>;
				};
			};
		};

		partition@180000 {
			label = "config2";
			reg = <0x180000 0x40000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_config2_10: macaddr@10 {
					compatible = "mac-base";
					reg = <0x10 0x11>;
					#nvmem-cell-cells = <1>;
				};
			};
		};

		partition@1c0000 {
			label = "kernel";
			reg = <0x1c0000 0x800000>;
		};

		fwconcat0: partition@9c0000 {
			label = "fwconcat0";
			reg = <0x9c0000 0x2000000>;
		};

		partition@29c0000 {
			label = "kernel2";
			reg = <0x29c0000 0x800000>;
			read-only;
		};

		fwconcat1: partition@31c0000 {
			label = "fwconcat1";
			reg = <0x31c0000 0x2a00000>;
		};

		partition@5bc0000 {
			label = "private";
			reg = <0x5bc0000 0x1400000>;
			read-only;
		};

		partition@6fc0000 {
			label = "mydlink";
			reg = <0x6fc0000 0x600000>;
			read-only;
		};

		partition@75c0000 {
			label = "myconfig";
			reg = <0x75c0000 0xa00000>;
			read-only;
		};
	};
};

&pcie {
	status = "okay";
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>, <&precal_factory_e10>;
		nvmem-cell-names = "eeprom", "precal";
		mediatek,disable-radar-background;

		#address-cells = <1>;
		#size-cells = <0>;

		band@0 {
			reg = <0>;
			nvmem-cells = <&macaddr_config2_10 1>;
			nvmem-cell-names = "mac-address";
		};

		band@1 {
			reg = <1>;
			nvmem-cells = <&macaddr_config2_10 2>;
			nvmem-cell-names = "mac-address";
		};
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_config2_10 0>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy4>;
	nvmem-cells = <&macaddr_config2_10 3>;
	nvmem-cell-names = "mac-address";
};

&ethphy4 {
	/delete-property/ interrupts;
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "lan3";
		};

		port@1 {
			status = "okay";
			label = "lan2";
		};

		port@2 {
			status = "okay";
			label = "lan1";
		};
	};
};
