Force update_cache_variants to use reset for Foresee NAND with bad blocks

Tested on Xiaomi AX3000T + F35SQA001G with bad blocks and without bad blocks

Signed-off-by: Dim Fish <dimfish@gmail.com>

--- a/drivers/mtd/nand/spi/foresee.c
+++ b/drivers/mtd/nand/spi/foresee.c
@@ -22,8 +22,8 @@ static SPINAND_OP_VARIANTS(write_cache_v
 		SPINAND_PROG_LOAD(true, 0, NULL, 0));
 
 static SPINAND_OP_VARIANTS(update_cache_variants,
-		SPINAND_PROG_LOAD_X4(false, 0, NULL, 0),
-		SPINAND_PROG_LOAD(false, 0, NULL, 0));
+		SPINAND_PROG_LOAD_X4(true, 0, NULL, 0),
+		SPINAND_PROG_LOAD(true, 0, NULL, 0));
 
 static int f35sqa002g_ooblayout_ecc(struct mtd_info *mtd, int section,
 				    struct mtd_oob_region *region)
