From 20a4b57c0fafd23ae0f6bcab5b5adf4af4c80280 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Thu, 16 Mar 2023 19:31:21 +0100
Subject: [PATCH] mips: bmips: tweak Kconfig options
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
---
 arch/mips/Kconfig | 7 +------
 1 file changed, 1 insertion(+), 6 deletions(-)

--- a/arch/mips/Kconfig
+++ b/arch/mips/Kconfig
@@ -259,19 +259,13 @@ config BMIPS_GENERIC
 	select SYNC_R4K
 	select COMMON_CLK
 	select BCM6345_L1_IRQ
-	select BCM7038_L1_IRQ
-	select BCM7120_L2_IRQ
-	select BRCMSTB_L2_IRQ
 	select IRQ_MIPS_CPU
 	select DMA_NONCOHERENT
 	select SYS_SUPPORTS_32BIT_KERNEL
-	select SYS_SUPPORTS_LITTLE_ENDIAN
 	select SYS_SUPPORTS_BIG_ENDIAN
-	select SYS_SUPPORTS_HIGHMEM
 	select SYS_HAS_CPU_BMIPS32_3300
 	select SYS_HAS_CPU_BMIPS4350
 	select SYS_HAS_CPU_BMIPS4380
-	select SYS_HAS_CPU_BMIPS5000
 	select SWAP_IO_SPACE
 	select USB_EHCI_BIG_ENDIAN_DESC if CPU_BIG_ENDIAN
 	select USB_EHCI_BIG_ENDIAN_MMIO if CPU_BIG_ENDIAN
@@ -281,6 +275,7 @@ config BMIPS_GENERIC
 	select HAVE_PCI
 	select PCI_DRIVERS_GENERIC
 	select FW_CFE
+	select MIPS_L1_CACHE_SHIFT_4
 	help
 	  Build a generic DT-based kernel image that boots on select
 	  BCM33xx cable modem chips, BCM63xx DSL chips, and BCM7xxx set-top
--- a/drivers/irqchip/Kconfig
+++ b/drivers/irqchip/Kconfig
@@ -123,7 +123,6 @@ config BCM6345_L1_IRQ
 config BCM7038_L1_IRQ
 	tristate "Broadcom STB 7038-style L1/L2 interrupt controller driver"
 	depends on ARCH_BRCMSTB || BMIPS_GENERIC
-	default ARCH_BRCMSTB || BMIPS_GENERIC
 	select GENERIC_IRQ_CHIP
 	select IRQ_DOMAIN
 	select GENERIC_IRQ_EFFECTIVE_AFF_MASK if SMP
@@ -131,14 +130,12 @@ config BCM7038_L1_IRQ
 config BCM7120_L2_IRQ
 	tristate "Broadcom STB 7120-style L2 interrupt controller driver"
 	depends on ARCH_BRCMSTB || BMIPS_GENERIC
-	default ARCH_BRCMSTB || BMIPS_GENERIC
 	select GENERIC_IRQ_CHIP
 	select IRQ_DOMAIN
 
 config BRCMSTB_L2_IRQ
 	tristate "Broadcom STB generic L2 interrupt controller driver"
 	depends on ARCH_BCM2835 || ARCH_BRCMSTB || BMIPS_GENERIC
-	default ARCH_BCM2835 || ARCH_BRCMSTB || BMIPS_GENERIC
 	select GENERIC_IRQ_CHIP
 	select IRQ_DOMAIN
 
