From 1c0608d860db973ad09b5a9ccb19b76ae07622a3 Mon Sep 17 00:00:00 2001
From: Mikhail Kshevetskiy <mikhail.kshevetskiy@iopsys.eu>
Date: Mon, 10 Nov 2025 06:56:44 +0300
Subject: [PATCH] clk: en7523: Add reset-controller support for EN7523 SoC

Introduce reset API support to EN7523 clock driver. EN7523 uses the
same reset logic as EN7581, so just reuse existing code.

Signed-off-by: Mikhail Kshevetskiy <mikhail.kshevetskiy@iopsys.eu>
Reviewed-by: AngeloGioacchino Del Regno <angelogioacchino.delregno@collabora.com>
Reviewed-by: Philipp Zabel <p.zabel@pengutronix.de>
Signed-off-by: Stephen Boyd <sboyd@kernel.org>
---
 drivers/clk/clk-en7523.c | 64 ++++++++++++++++++++++++++++++++++++----
 1 file changed, 59 insertions(+), 5 deletions(-)

diff --git a/drivers/clk/clk-en7523.c b/drivers/clk/clk-en7523.c
index 15bbdeb60b8e..08cc8e5acf43 100644
--- a/drivers/clk/clk-en7523.c
+++ b/drivers/clk/clk-en7523.c
@@ -9,6 +9,7 @@
 #include <linux/regmap.h>
 #include <linux/reset-controller.h>
 #include <dt-bindings/clock/en7523-clk.h>
+#include <dt-bindings/reset/airoha,en7523-reset.h>
 #include <dt-bindings/reset/airoha,en7581-reset.h>
 
 #define RST_NR_PER_BANK			32
@@ -299,6 +300,53 @@ static const u16 en7581_rst_ofs[] = {
 	REG_RST_CTRL1,
 };
 
+static const u16 en7523_rst_map[] = {
+	/* RST_CTRL2 */
+	[EN7523_XPON_PHY_RST]		= 0,
+	[EN7523_XSI_MAC_RST]		= 7,
+	[EN7523_XSI_PHY_RST]		= 8,
+	[EN7523_NPU_RST]		= 9,
+	[EN7523_I2S_RST]		= 10,
+	[EN7523_TRNG_RST]		= 11,
+	[EN7523_TRNG_MSTART_RST]	= 12,
+	[EN7523_DUAL_HSI0_RST]		= 13,
+	[EN7523_DUAL_HSI1_RST]		= 14,
+	[EN7523_HSI_RST]		= 15,
+	[EN7523_DUAL_HSI0_MAC_RST]	= 16,
+	[EN7523_DUAL_HSI1_MAC_RST]	= 17,
+	[EN7523_HSI_MAC_RST]		= 18,
+	[EN7523_WDMA_RST]		= 19,
+	[EN7523_WOE0_RST]		= 20,
+	[EN7523_WOE1_RST]		= 21,
+	[EN7523_HSDMA_RST]		= 22,
+	[EN7523_I2C2RBUS_RST]		= 23,
+	[EN7523_TDMA_RST]		= 24,
+	/* RST_CTRL1 */
+	[EN7523_PCM1_ZSI_ISI_RST]	= RST_NR_PER_BANK + 0,
+	[EN7523_FE_PDMA_RST]		= RST_NR_PER_BANK + 1,
+	[EN7523_FE_QDMA_RST]		= RST_NR_PER_BANK + 2,
+	[EN7523_PCM_SPIWP_RST]		= RST_NR_PER_BANK + 4,
+	[EN7523_CRYPTO_RST]		= RST_NR_PER_BANK + 6,
+	[EN7523_TIMER_RST]		= RST_NR_PER_BANK + 8,
+	[EN7523_PCM1_RST]		= RST_NR_PER_BANK + 11,
+	[EN7523_UART_RST]		= RST_NR_PER_BANK + 12,
+	[EN7523_GPIO_RST]		= RST_NR_PER_BANK + 13,
+	[EN7523_GDMA_RST]		= RST_NR_PER_BANK + 14,
+	[EN7523_I2C_MASTER_RST]		= RST_NR_PER_BANK + 16,
+	[EN7523_PCM2_ZSI_ISI_RST]	= RST_NR_PER_BANK + 17,
+	[EN7523_SFC_RST]		= RST_NR_PER_BANK + 18,
+	[EN7523_UART2_RST]		= RST_NR_PER_BANK + 19,
+	[EN7523_GDMP_RST]		= RST_NR_PER_BANK + 20,
+	[EN7523_FE_RST]			= RST_NR_PER_BANK + 21,
+	[EN7523_USB_HOST_P0_RST]	= RST_NR_PER_BANK + 22,
+	[EN7523_GSW_RST]		= RST_NR_PER_BANK + 23,
+	[EN7523_SFC2_PCM_RST]		= RST_NR_PER_BANK + 25,
+	[EN7523_PCIE0_RST]		= RST_NR_PER_BANK + 26,
+	[EN7523_PCIE1_RST]		= RST_NR_PER_BANK + 27,
+	[EN7523_PCIE_HB_RST]		= RST_NR_PER_BANK + 29,
+	[EN7523_XPON_MAC_RST]		= RST_NR_PER_BANK + 31,
+};
+
 static const u16 en7581_rst_map[] = {
 	/* RST_CTRL2 */
 	[EN7581_XPON_PHY_RST]		= 0,
@@ -357,6 +405,9 @@ static const u16 en7581_rst_map[] = {
 	[EN7581_XPON_MAC_RST]		= RST_NR_PER_BANK + 31,
 };
 
+static int en7581_reset_register(struct device *dev, void __iomem *base,
+				 const u16 *rst_map, int nr_resets);
+
 static u32 en7523_get_base_rate(const struct en_clk_desc *desc, u32 val)
 {
 	if (!desc->base_bits)
@@ -552,7 +603,8 @@ static int en7523_clk_hw_init(struct platform_device *pdev,
 
 	en7523_register_clocks(&pdev->dev, clk_data, base, np_base);
 
-	return 0;
+	return en7581_reset_register(&pdev->dev, np_base, en7523_rst_map,
+				     ARRAY_SIZE(en7523_rst_map));
 }
 
 static void en7581_register_clocks(struct device *dev, struct clk_hw_onecell_data *clk_data,
@@ -652,7 +704,8 @@ static const struct reset_control_ops en7581_reset_ops = {
 	.status = en7523_reset_status,
 };
 
-static int en7581_reset_register(struct device *dev, void __iomem *base)
+static int en7581_reset_register(struct device *dev, void __iomem *base,
+				 const u16 *rst_map, int nr_resets)
 {
 	struct en_rst_data *rst_data;
 
@@ -661,10 +714,10 @@ static int en7581_reset_register(struct device *dev, void __iomem *base)
 		return -ENOMEM;
 
 	rst_data->bank_ofs = en7581_rst_ofs;
-	rst_data->idx_map = en7581_rst_map;
+	rst_data->idx_map = rst_map;
 	rst_data->base = base;
 
-	rst_data->rcdev.nr_resets = ARRAY_SIZE(en7581_rst_map);
+	rst_data->rcdev.nr_resets = nr_resets;
 	rst_data->rcdev.of_xlate = en7523_reset_xlate;
 	rst_data->rcdev.ops = &en7581_reset_ops;
 	rst_data->rcdev.of_node = dev->of_node;
@@ -698,7 +751,8 @@ static int en7581_clk_hw_init(struct platform_device *pdev,
 	val = readl(base + REG_NP_SCU_PCIC);
 	writel(val | 3, base + REG_NP_SCU_PCIC);
 
-	return en7581_reset_register(&pdev->dev, base);
+	return en7581_reset_register(&pdev->dev, base, en7581_rst_map,
+				     ARRAY_SIZE(en7581_rst_map));
 }
 
 static int en7523_clk_probe(struct platform_device *pdev)
-- 
2.39.5

