// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
#include "qcom-ipq8064-v2.0-smb208.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "Linksys E8350 V1 WiFi Router";
	compatible = "linksys,e8350-v1", "qcom,ipq8064";

	memory@0 {
		reg = <0x42000000 0x1e000000>;
		device_type = "memory";
	};

	aliases {
		serial0 = &gsbi4_serial;

		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		reset {
			label = "reset";
			gpios = <&qcom_pinmux 68 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wps {
			label = "wps";
			gpios = <&qcom_pinmux 65 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
			wakeup-source;
		};

		wifi {
			label = "wifi";
			gpios = <&qcom_pinmux 67 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
			debounce-interval = <60>;
			wakeup-source;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-0 = <&led_pins>;
		pinctrl-names = "default";

		led_power: power {
			label = "green:power";
			gpios = <&qcom_pinmux 26 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};

		wps {
			label = "green:wps";
			gpios = <&qcom_pinmux 53 GPIO_ACTIVE_HIGH>;
		};

		wifi {
			label = "green:wifi";
			gpios = <&qcom_pinmux 54 GPIO_ACTIVE_HIGH>;
		};
	};
};

&nand {
	status = "okay";

	nand@0 {
		reg = <0>;

		nand-ecc-strength = <4>;
		nand-bus-width = <8>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "ubi";
				reg = <0 0x4000000>;
			};
			partition@4000000 {
				label = "extra";
				reg = <0x4000000 0x4000000>;
			};
		};
	};
};

&qcom_pinmux {
	button_pins: button_pins {
		mux {
			pins = "gpio68","gpio65", "gpio67";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	led_pins: led_pins {
		mux {
			pins = "gpio26","gpio53", "gpio54";
			function = "gpio";
			drive-strength = <2>;
			bias-pull-up;
		};
	};

	switch_reset: switch_reset_pins {
		mux {
			pins = "gpio63";
			function = "gpio";
			drive-strength = <12>;
			bias-pull-up;
		};
	};
};

&gsbi5 {
	qcom,mode = <GSBI_PROT_SPI>;
	status = "okay";

	spi5: spi@1a280000 {
		status = "okay";

		pinctrl-0 = <&spi_pins>;
		pinctrl-names = "default";

		cs-gpios = <&qcom_pinmux 20 GPIO_ACTIVE_LOW>;

		m25p80@0 {
			compatible = "jedec,spi-nor";
			spi-max-frequency = <51200000>;
			reg = <0>;

			partitions {
				compatible = "fixed-partitions";
				#address-cells = <1>;
				#size-cells = <1>;

				partition@0 {
					label = "0:sbl1";
					reg = <0x0000000 0x0010000>;
					read-only;
				};

				partition@10000 {
					label = "0:mibib";
					reg = <0x0010000 0x0020000>;
					read-only;
				};

				partition@30000 {
					label = "0:sbl2";
					reg = <0x0030000 0x0020000>;
					read-only;
				};

				partition@50000 {
					label = "0:sbl3";
					reg = <0x0050000 0x0030000>;
					read-only;
				};

				partition@80000 {
					label = "0:ddrconfig";
					reg = <0x0080000 0x0010000>;
					read-only;
				};

				partition@90000 {
					label = "0:ssd";
					reg = <0x0090000 0x0010000>;
					read-only;
				};

				partition@a0000 {
					label = "0:tz";
					reg = <0x00a0000 0x0030000>;
					read-only;
				};

				partition@d0000 {
					label = "0:rpm";
					reg = <0x00d0000 0x0020000>;
					read-only;
				};

				partition@f0000 {
					label = "0:oldappsbl";
					reg = <0x00f0000 0x0040000>;
					read-only;
				};

				partition@130000 {
					label = "0:appsblenv";
					reg = <0x0130000 0x0040000>;
					read-only;
				};

				art: partition@170000 {
					label = "0:ART";
					reg = <0x0170000 0x0020000>;
					read-only;
				};

				partition@190000 {
					label = "0:uboot";
					reg = <0x0190000 0x0050000>;
					read-only;
				};

				partition@1e0000 {
					label = "0:oldnss1";
					reg = <0x01e0000 0x0020000>;
					read-only;
				};

				partition@200000 {
					label = "0:nvram";
					reg = <0x0200000 0x0020000>;
					read-only;
				};

				partition@220000 {
					label = "0:oldkernel";
					reg = <0x0220000 0x01e0000>;
					read-only;
				};
			};
		};
	};
};

&hs_phy_0 {
	status = "okay";
};

&ss_phy_0 {
	status = "okay";
};

&usb3_0 {
	status = "okay";
};

&hs_phy_1 {
	status = "okay";
};

&ss_phy_1 {
	status = "okay";
};

&usb3_1 {
	status = "okay";
};

&pcie0 {
	status = "okay";

	max-link-speed = <1>;
};

&pcie1 {
	status = "okay";
};

&mdio0 {
	status = "okay";

	pinctrl-0 = <&mdio0_pins>;
	pinctrl-names = "default";

	/* Switch from documentation require at least 12ms for reset */
	reset-gpios = <&qcom_pinmux 63 GPIO_ACTIVE_HIGH>;
	reset-post-delay-us = <12000>;

	switch@10 {
		compatible = "qca,qca8337";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x10>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "cpu";
				ethernet = <&gmac1>;
				phy-mode = "rgmii";
				tx-internal-delay-ps = <1000>;
				rx-internal-delay-ps = <1000>;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};

			port@1 {
				reg = <1>;
				label = "lan1";
				phy-mode = "internal";
				phy-handle = <&phy_port1>;
			};

			port@2 {
				reg = <2>;
				label = "lan2";
				phy-mode = "internal";
				phy-handle = <&phy_port2>;
			};

			port@3 {
				reg = <3>;
				label = "lan3";
				phy-mode = "internal";
				phy-handle = <&phy_port3>;
			};

			port@4 {
				reg = <4>;
				label = "lan4";
				phy-mode = "internal";
				phy-handle = <&phy_port4>;
			};

			port@5 {
				reg = <5>;
				label = "wan";
				phy-mode = "internal";
				phy-handle = <&phy_port5>;
			};

			port@6 {
				reg = <6>;
				label = "cpu";
				ethernet = <&gmac2>;
				phy-mode = "sgmii";
				qca,sgmii-enable-pll;

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};

		mdio {
			#address-cells = <1>;
			#size-cells = <0>;

			phy_port1: phy@0 {
				reg = <0>;
			};

			phy_port2: phy@1 {
				reg = <1>;
			};

			phy_port3: phy@2 {
				reg = <2>;
			};

			phy_port4: phy@3 {
				reg = <3>;
			};

			phy_port5: phy@4 {
				reg = <4>;
			};
		};
	};
};

&gmac1 {
	status = "okay";

	phy-mode = "rgmii";
	qcom,id = <1>;

	pinctrl-0 = <&rgmii2_pins>;
	pinctrl-names = "default";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gmac2 {
	status = "okay";

	phy-mode = "sgmii";
	qcom,id = <2>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&tcsr {
	qcom,usb-ctrl-select = <TCSR_USB_SELECT_USB3_DUAL>;
	compatible = "qcom,tcsr", "syscon";
};

&adm_dma {
	status = "okay";
};
