From 3d3a406dea89b789dfb550bd05d0eba5ae926755 Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Fri, 7 Feb 2025 14:17:06 +0100
Subject: [PATCH 08/10] usb: host: add ARCH_AIROHA in XHCI MTK dependency

Airoha SoC use the same register map a logic of the Mediatek xHCI
driver, hence add it to the dependency list to permit compilation also
on this ARCH.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 drivers/usb/host/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/usb/host/Kconfig
+++ b/drivers/usb/host/Kconfig
@@ -71,7 +71,7 @@ config USB_XHCI_HISTB
 config USB_XHCI_MTK
 	tristate "xHCI support for MediaTek SoCs"
 	select MFD_SYSCON
-	depends on (MIPS && SOC_MT7621) || ARCH_MEDIATEK || COMPILE_TEST
+	depends on (MIPS && SOC_MT7621) || ARCH_MEDIATEK || ARCH_AIROHA || COMPILE_TEST
 	help
 	  Say 'Y' to enable the support for the xHCI host controller
 	  found in MediaTek SoCs.
