// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	aliases {
		led-boot = &led_status_green;
		led-failsafe = &led_status_yellow;
		led-running = &led_status_green;
		led-upgrade = &led_status_yellow;
		label-mac-device = &eth0;
	};

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	leds {
		compatible = "gpio-leds";

		led_status_green: status_green {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led_status_yellow: status_yellow {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_YELLOW>;
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			partition@50000 {
				label = "art";
				reg = <0x050000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					cal_art_1000: calibration@1000 {
						reg = <0x1000 0x440>;
					};
				};
			};

			partition@60000 {
				label = "config";
				reg = <0x060000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_config_201a: macaddr@201a {
						reg = <0x201a 0x6>;
					};
				};
			};

			partition@70000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x070000 0xf90000>;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy-mask = <0x10>;

	phy4: ethernet-phy@4 {
		reg = <4>;
		eee-broken-100tx;
		eee-broken-1000t;
	};
};

&eth0 {
	status = "okay";

	pll-data = <0xa6000000 0xa0000101 0xa0001313>;

	nvmem-cells = <&macaddr_config_201a>;
	nvmem-cell-names = "mac-address";

	phy-mode = "rgmii-id";
	phy-handle = <&phy4>;

	gmac_config: gmac-config {
		device = <&gmac>;

		rgmii-enabled = <1>;

		rxdv-delay = <3>;
		rxd-delay = <3>;
		txen-delay = <3>;
		txd-delay = <3>;
	};
};

&wmac {
	status = "okay";

	nvmem-cells = <&cal_art_1000>;
	nvmem-cell-names = "calibration";
};
