From af87d38c442c75a40c7d0a7d8c31557e2e6ccf98 Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Sun, 25 May 2025 20:22:40 +0200
Subject: [PATCH 1/2] pinctrl: airoha: fix wrong PHY LED mux value for LED1
 GPIO46

In all the MUX value for LED1 GPIO46 there is a Copy-Paste error where
the MUX value is set to LED0_MODE_MASK instead of LED1_MODE_MASK.

This wasn't notice as there were no board that made use of the
secondary PHY LED but looking at the internal Documentation the actual
value should be LED1_MODE_MASK similar to the other GPIO entry.

Fix the wrong value to apply the correct MUX configuration.

Cc: stable@vger.kernel.org
Fixes: 1c8ace2d0725 ("pinctrl: airoha: Add support for EN7581 SoC")
Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
---
 drivers/pinctrl/mediatek/pinctrl-airoha.c | 16 ++++++++--------
 1 file changed, 8 insertions(+), 8 deletions(-)

--- a/drivers/pinctrl/mediatek/pinctrl-airoha.c
+++ b/drivers/pinctrl/mediatek/pinctrl-airoha.c
@@ -1747,8 +1747,8 @@ static const struct airoha_pinctrl_func_
 		.regmap[0] = {
 			AIROHA_FUNC_MUX,
 			REG_GPIO_2ND_I2C_MODE,
-			GPIO_LAN3_LED0_MODE_MASK,
-			GPIO_LAN3_LED0_MODE_MASK
+			GPIO_LAN3_LED1_MODE_MASK,
+			GPIO_LAN3_LED1_MODE_MASK
 		},
 		.regmap[1] = {
 			AIROHA_FUNC_MUX,
@@ -1811,8 +1811,8 @@ static const struct airoha_pinctrl_func_
 		.regmap[0] = {
 			AIROHA_FUNC_MUX,
 			REG_GPIO_2ND_I2C_MODE,
-			GPIO_LAN3_LED0_MODE_MASK,
-			GPIO_LAN3_LED0_MODE_MASK
+			GPIO_LAN3_LED1_MODE_MASK,
+			GPIO_LAN3_LED1_MODE_MASK
 		},
 		.regmap[1] = {
 			AIROHA_FUNC_MUX,
@@ -1875,8 +1875,8 @@ static const struct airoha_pinctrl_func_
 		.regmap[0] = {
 			AIROHA_FUNC_MUX,
 			REG_GPIO_2ND_I2C_MODE,
-			GPIO_LAN3_LED0_MODE_MASK,
-			GPIO_LAN3_LED0_MODE_MASK
+			GPIO_LAN3_LED1_MODE_MASK,
+			GPIO_LAN3_LED1_MODE_MASK
 		},
 		.regmap[1] = {
 			AIROHA_FUNC_MUX,
@@ -1939,8 +1939,8 @@ static const struct airoha_pinctrl_func_
 		.regmap[0] = {
 			AIROHA_FUNC_MUX,
 			REG_GPIO_2ND_I2C_MODE,
-			GPIO_LAN3_LED0_MODE_MASK,
-			GPIO_LAN3_LED0_MODE_MASK
+			GPIO_LAN3_LED1_MODE_MASK,
+			GPIO_LAN3_LED1_MODE_MASK
 		},
 		.regmap[1] = {
 			AIROHA_FUNC_MUX,
