// SPDX-License-Identifier: (GPL-2.0 OR MIT)

/dts-v1/;

#include "mt7981b-cudy-wr3000-nand.dtsi"

/ {
	model = "Cudy WR3000H v1";
	compatible = "cudy,wr3000h-v1", "mediatek,mt7981";

	aliases {
		label-mac-device = &gmac0;
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
		serial0 = &uart0;
	};

	leds {
		compatible = "gpio-leds";

		led_status: led-status {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 5 GPIO_ACTIVE_LOW>;
		};

		led-internet {
			function = LED_FUNCTION_WAN_ONLINE;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 11 GPIO_ACTIVE_LOW>;
		};

		led-wps {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 9 GPIO_ACTIVE_LOW>;
		};

		led-wlan2g {
			function = LED_FUNCTION_WLAN_2GHZ;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 6 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led-wlan5g {
			function = LED_FUNCTION_WLAN_5GHZ;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 7 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		led-lan1 {
			function = LED_FUNCTION_LAN;
			function-enumerator = <1>;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 8 GPIO_ACTIVE_LOW>;
		};

		led-lan2 {
			function = LED_FUNCTION_LAN;
			function-enumerator = <2>;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 10 GPIO_ACTIVE_LOW>;
		};

		led-lan3 {
			function = LED_FUNCTION_LAN;
			function-enumerator = <3>;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 12 GPIO_ACTIVE_LOW>;
		};

		led-lan4 {
			function = LED_FUNCTION_LAN;
			function-enumerator = <4>;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 13 GPIO_ACTIVE_LOW>;
		};

		led-wan {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&pio 35 GPIO_ACTIVE_LOW>;
		};
	};
};

&eth {
	gmac1: mac@1 {
		compatible = "mediatek,eth-mac";
		reg = <1>;
		phy-mode = "2500base-x";
		phy-handle = <&phy6>;
		nvmem-cell-names = "mac-address";
		nvmem-cells = <&macaddr_bdinfo_de00 1>;
		label = "wan";
	};
};

&mdio_bus {
	/* We need to have the reset GPIO on the MDIO bus node,
	 * otherwise the PHY would be held in reset during PHY detection */
	reset-gpios = <&pio 3 GPIO_ACTIVE_LOW>;
	reset-delay-us = <100000>;
	reset-post-delay-us = <100000>;

	phy6: ethernet-phy@6 {
		/* Either Realtek RTL8221B-VB-CG or Motorcomm YT8821,
		 * depending on HW revision */
		compatible = "ethernet-phy-ieee802.3-c45";
		reg = <6>;
	};
};

&switch {
	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			label = "lan4";
		};

		port@1 {
			reg = <1>;
			label = "lan3";
		};

		port@2 {
			reg = <2>;
			label = "lan2";
		};

		port@3 {
			reg = <3>;
			label = "lan1";
		};

		port@6 {
			reg = <6>;
			label = "cpu";
			ethernet = <&gmac0>;
			phy-mode = "2500base-x";

			fixed-link {
				speed = <2500>;
				full-duplex;
				pause;
			};
		};
	};
};

