// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/dts-v1/;
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

#include "mt7981b.dtsi"

/ {
	model = "Huasifei WH3000";
	compatible = "huasifei,wh3000", "mediatek,mt7981";

	aliases {
		serial0 = &uart0;
		led-boot = &wlan_led;
		led-failsafe = &wlan_led;
		led-upgrade = &wlan_led;
	};

	chosen {
		bootargs = "root=PARTLABEL=rootfs rootwait";
		stdout-path = "serial0:115200n8";
	};

	gpio-keys {
		compatible = "gpio-keys";

		button-mode {
			label = "mode";
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
			gpios = <&pio 0 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		button-reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&pio 1 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		wan_led: led-0 {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_RED>;
			gpios = <&pio 11 GPIO_ACTIVE_LOW>;
		};

		wlan_led: led-1 {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&pio 10 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	memory@40000000 {
		reg = <0 0x40000000 0 0x40000000>;
		device_type = "memory";
	};
};

&eth {
	pinctrl-names = "default";
	pinctrl-0 = <&mdio_pins>;
	status = "okay";

	gmac0: mac@0 {
		compatible = "mediatek,eth-mac";
		reg = <0>;
		nvmem-cells = <&macaddr_factory_4 2>;
		nvmem-cell-names = "mac-address";
		phy-mode = "2500base-x";
		phy-handle = <&phy1>;
	};

	gmac1: mac@1 {
		compatible = "mediatek,eth-mac";
		reg = <1>;
		nvmem-cells = <&macaddr_factory_4 3>;
		nvmem-cell-names = "mac-address";
		phy-mode = "gmii";
		phy-handle = <&int_gbe_phy>;
	};
};

&mdio_bus {
	phy1: ethernet-phy@1 {
		compatible = "ethernet-phy-ieee802.3-c45";
		reg = <1>;
		interrupts = <38 IRQ_TYPE_LEVEL_LOW>;
		interrupt-parent = <&pio>;
		reset-assert-us = <100000>;
		reset-deassert-us = <100000>;
		reset-gpios = <&pio 39 GPIO_ACTIVE_LOW>;
		realtek,aldps-enable;
	};
};

&mmc0 {
	#address-cells = <1>;
	#size-cells = <0>;
	bus-width = <8>;
	cap-mmc-highspeed;
	max-frequency = <52000000>;
	no-sd;
	no-sdio;
	non-removable;
	pinctrl-names = "default", "state_uhs";
	pinctrl-0 = <&mmc0_pins_default>;
	pinctrl-1 = <&mmc0_pins_uhs>;
	vmmc-supply = <&reg_3p3v>;
	status = "okay";

	card@0 {
		compatible = "mmc-card";
		reg = <0>;

		block {
			compatible = "block-device";

			partitions {
				block-partition-factory {
					partname = "factory";

					nvmem-layout {
						compatible = "fixed-layout";
						#address-cells = <1>;
						#size-cells = <1>;

						eeprom_factory_0: eeprom@0 {
							reg = <0x0 0x1000>;
						};

						macaddr_factory_4: macaddr@4 {
							compatible = "mac-base";
							reg = <0x4 0x6>;
							#nvmem-cell-cells = <1>;
						};
					};
				};
			};
		};
	};
};

&pio {
	mmc0_pins_default: mmc0-pins-default {
		mux {
			function = "flash";
			groups = "emmc_45";
		};
	};

	mmc0_pins_uhs: mmc0-pins-uhs {
		mux {
			function = "flash";
			groups = "emmc_45";
		};
	};
};

&uart0 {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&watchdog {
	status = "okay";
};

&wifi {
	#address-cells = <1>;
	#size-cells = <0>;
	nvmem-cells = <&eeprom_factory_0>;
	nvmem-cell-names = "eeprom";
	status = "okay";

	band@1 {
		reg = <1>;
		nvmem-cells = <&macaddr_factory_4 1>;
		nvmem-cell-names = "mac-address";
	};
};

&xhci {
	status = "okay";
};
