// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	compatible = "humax,e2", "ralink,mt7620a-soc";
	model = "HUMAX E2";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &ethernet;
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio1 3 GPIO_ACTIVE_LOW>;
		};

		pairing {
			label = "green:pairing";
			gpios = <&gpio1 8 GPIO_ACTIVE_LOW>;
		};

		wlan {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio1 9 GPIO_ACTIVE_LOW>;
		};

		lan {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio1 4 GPIO_ACTIVE_LOW>;
		};

		wps {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio1 5 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio1 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "factory";
				reg = <0x40000 0x30000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					eeprom_factory_0: eeprom@0 {
						reg = <0x0 0x200>;
					};

					eeprom_factory_8000: eeprom@8000 {
						reg = <0x8000 0x200>;
					};

					macaddr_factory_10007: macaddr@10007 {
						reg = <0x10007 0x6>;
					};
				};
			};

			partition@70000 {
				compatible = "openwrt,uimage", "denx,uimage";
				openwrt,offset = <FW_EDIMAX_OFFSET>;
				openwrt,partition-magic = <FW_MAGIC_EDIMAX>;
				label = "firmware";
				reg = <0x70000 0x790000>;
			};
		};
	};
};

&ethernet {
	nvmem-cells = <&macaddr_factory_10007>;
	nvmem-cell-names = "mac-address";
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_8000>;
		nvmem-cell-names = "eeprom";
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&wmac {
	nvmem-cells = <&eeprom_factory_0>;
	nvmem-cell-names = "eeprom";
};

&state_default {
	gpio {
		groups = "rgmii1";
		function = "gpio";
	};
};
