From 2cd02f2fdd8a92e5b6b85ff64eab0fc549b30c07 Mon Sep 17 00:00:00 2001
From: Heiner Kallweit <hkallweit1@gmail.com>
Date: Sat, 2 Nov 2024 14:49:01 +0100
Subject: [PATCH] r8169: improve initialization of RSS registers on
 RTL8125/RTL8126

Replace the register addresses with the names used in r8125/r8126
vendor driver, and consider that RSS_CTRL_8125 is a 32 bit register.

Signed-off-by: Heiner Kallweit <hkallweit1@gmail.com>
Link: https://patch.msgid.link/3bf2f340-b369-4174-97bf-fd38d4217492@gmail.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/realtek/r8169_main.c | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

--- a/drivers/net/ethernet/realtek/r8169_main.c
+++ b/drivers/net/ethernet/realtek/r8169_main.c
@@ -346,6 +346,8 @@ enum rtl8125_registers {
 	TxPoll_8125		= 0x90,
 	LEDSEL3			= 0x96,
 	MAC0_BKP		= 0x19e0,
+	RSS_CTRL_8125		= 0x4500,
+	Q_NUM_CTRL_8125		= 0x4800,
 	EEE_TXIDLE_TIMER_8125	= 0x6048,
 };
 
@@ -3788,8 +3790,8 @@ static void rtl_hw_start_8125_common(str
 	rtl_pcie_state_l2l3_disable(tp);
 
 	RTL_W16(tp, 0x382, 0x221b);
-	RTL_W8(tp, 0x4500, 0);
-	RTL_W16(tp, 0x4800, 0);
+	RTL_W32(tp, RSS_CTRL_8125, 0);
+	RTL_W16(tp, Q_NUM_CTRL_8125, 0);
 
 	/* disable UPS */
 	r8168_mac_ocp_modify(tp, 0xd40a, 0x0010, 0x0000);
